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Division 06 61 00
PRISM® DECORATIVE TRIM

PART 1 – GENERAL

1.01 SUMMARY

A. Prism® Solid Surface Decorative Trim

1.02 SECTION INCLUDES

A. Decorative Trim

1.03 REFERENCES

A. American National Standards Institute (ANSI)

B. International Cast Polymer Alliance (ICPA)

C. National Fire Protection Association (NFPA)

1.04 SYSTEM DESCRIPTION

A. Performance Requirements: Provide decorative trim that conform to the following requirements of regulatory agencies and the quality control of InPro Corporation.

1. Provide solid surface material that conforms to ANSI/ICPA SS-1 for workmanship and finish, structural integrity and material characteristics.

2. Fungal and Bacterial Resistance: Provide Prism Solid Surface that does not support fungal or bacterial growth as tested in accordance with ASTM G-21 and ASTM G-22.

3. Fire Performance Characteristics: Provide Prism Solid Surface Wall Cladding conforming with the NFPA class A fire rating as determined by ASTM E-84.

1.05 SUBMITTALS

A. Product Data: Manufacturer’s printed product data for each type of decorative trim specified.

B. Samples: Verification samples minimum of 2" x 2" samples indicating color and pattern.

D. Manufacturer’s Installation Instruction: Printed installation instructions for decorative trim.

1.06 DELIVERY, STORAGE AND HANDLING

A. Deliver materials in unopened factory packaging to the jobsite

B. Inspect materials at delivery to assure that specified products have been received.

C. Store in original packaging in an interior climate controlled location away from direct sunlight.

1.07 PROJECT CONDITIONS

A. Environmental Requirements: Products must be installed in an interior climate controlled environment.

1.08 WARRANTY

A. Standard PRISM® Solid Surface Limited 10 Year Warranty against material and manufacturing defects.

PART 2 – PRODUCTS

2.01 MANUFACTURER

A. Acceptable Manufacturer: 
InPro Corporation

PO Box 406 Muskego, WI 53150 USA

Telephone: 800-222-5556

Fax: 888-715-8407

inprocorp.com
B. Substitutions: Not permitted

C. Provide all solid surface systems from a single source.

2.02 MANUFACTURED UNITS

A. Solid Surface Decorative Trim

1. Decorative Trim

a. Decorative Trim Piece , Small, 1-1/8” high x 96” wide, protrudes ¾” from the wall.

b. Decorative Trim Piece , Large, 4-¾” high x 96” wide, protrudes 2” from the wall.

2.03 MATERIALS

A. Prism Solid Surface: Wall panels shall be manufactured from polyester/acrylic blended resins with natural filler material.

2.04 FINISHES

A. Color and pattern of Prism Solid Surface wall panels to be selected by the architect from the Prism Solid Surface finish selection. Surface shall have a matte, semi-gloss or high-gloss finish.

PART 3 - EXECUTION

3.01 EXAMINATION

A. Examine areas and conditions in which solid surface decorative trim will be installed.

3.02 PREPARATION

A. General: Prior to installation, clean area to remove dust, debris and loose particles.

3.03 INSTALLATION

A. General: Install components plumb and level, scribe adjacent finishes, in accordance with approved shop drawings and recommended installation instructions.

3.04 CLEANING

A. At completion of the installation, clean surfaces in accordance with the InPro Decorative Surfaces clean-up and maintenance instructions

END OF SECTION
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