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Division 10 14 00
S450/S455 ACTIVITY/CALENDAR SIGN

PART 1 - GENERAL

1.01 SUMMARY

A. This section includes ADA compliant tactile signage and changeable message signage

1.02 SECTION INCLUDES

A. S450/S455 Activity/Calendar Sign

1.03 REFERENCES

A. Americans with Disabilities Act (ADA)

B. American National Standards Institute (ANSI)

1.04 SYSTEM DESCRIPTION

A. Performance Requirements: Provide signage systems that conform to the following requirements of regulatory agencies and the quality control of InPro SignScape.

1. Signage shall comply with all applicable provisions of the ADA and ANSI A117.1-1998

1.05 SUBMITTALS

A. Product Data: Manufacturer’s printed product data for each signage system indicated in this section.

B. Detail Drawings: Detail drawings showing sizes and lettering, construction details of each type of sign and mounting details with appropriate fasteners for specific project substrates.

C. Samples: Verification samples of signage systems minimum of 6 inches square of each type and color indicated.

D. Manufacturer’s Installation Instructions: Printed Installation Instructions for each signage system.

1.06 DELIVERY, STORAGE AND HANDLING

A. Deliver materials in unopened factory packaging to the jobsite.

B. Inspect materials at delivery to assure that specified product have been received.

C. Store in original packaging in a climate controlled environment away from direct sunlight.

1.07 WARRANTY

A. Standard InPro SignScape limited lifetime warranty against material and manufacturing defects.

PART 2 PRODUCTS

2.01 MANUFACTURERS

A. Acceptable Manufacturer: 
InPro SignScape, InPro

Corporation PO Box 406, Muskego, WI 53150 USA

Telephone 800-222-5556, Fax: 888-715-8407

E-mail: service@inprocorp.com

B. Substitutions: Not permitted

C. Provide all signage systems from a single manufacturer.

2.02 MATERIALS

C. Production Style

1. Tactile (Raised Letter)

a. Provide sign material consisting of .040” sheet bonded to .060” sheet. Top layer is cut and assembled to create signage.

b. Provide clear sign window consisting of a top layer of .060” sheet, .010” clear polycarbonate sheet and a back layer of.060” sheet. Top layer is cut and bonded to clear sheet to create window. Clear sheet is bonded to back layer with space to allow user supplied paper to slide behind clear sheet.

2. Flush Inlay

Provide sign panel consisting of .080" (2mm) sheet that is engraved to receive .040" (1mm) sheet that is cut and assembled to create signage.

2.03 MANUFACTURED UNITS

A. S450 Activity/Calendar Sign

1. Overall size: 477/8”(1.22m)h x 681/2”(1.74m)w 

Clear window: size 61/2”(165mm)h x 81/2”(216mm)w, quantity - 35, Clear windows are to be mounted to sign with magnetic strips. 

Monthly header Sign: Size 11/2”(38mm)h x 237/8”(606mm)w

B. S455 Activity/Calendar Sign

1. Overall size: 281/2”(.724m)h x 44” (1.12m)w

Clear window: size 31/2”(89mm)h x 51/2”(140mm)w, quantity - 35, Clear windows are to be mounted to sign with magnetic strips.

Monthly Header Sign: Size 11/4”(32mm)h x 10”(254mm)w

PART 3 EXECUTION

3.01 EXAMINATION

A. Examine areas and conditions in which the signage system will be installed.

1. Complete all finishing operations, including painting, before beginning installation of signage systems.

2. Wall surface shall be dry and free from dirt, grease and loose paint.

3.02 PREPARATION

A. General: Prior to installation, clean substrate to remove dust, debris and loose particles.

3.03 INSTALLATION

A. General: Locate the signage system as indicated on the approved detail drawing for the appropriate substrate and in compliance with the InPro SignScape installation instructions. Install signage systems level and plumb at the height indicated on the drawings.

3.04 CLEANING

A. At completion of the installation, clean surfaces in accordance with the InPro SignScape clean up and maintenance instructions.
END OF SECTION
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