,Luminaire Styles##other##,Size##other##,Optic##other##,Light Output##other##,CRI##other##,LED Color Temperature##other##,Voltage##electrical_potential##volts,Ceiling Type##other##,Width##length##inches,Length##length##inches
HPR LED-A-2x4-DCO-S -8-120-C1,Angled,2x4,Diffuse,Standard,80,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-120-C1,Flat,2x4,Diffuse,Standard,80,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-120-C1,Angled,2x4,Slotted,Standard,80,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-120-C1,Flat,2x4,Slotted,Standard,80,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-277-C1,Angled,2x4,Diffuse,Standard,80,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-277-C1,Flat,2x4,Diffuse,Standard,80,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-277-C1,Angled,2x4,Slotted,Standard,80,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-277-C1,Flat,2x4,Slotted,Standard,80,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-120-C2,Angled,2x4,Diffuse,Standard,80,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-120-C2,Flat,2x4,Diffuse,Standard,80,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-120-C2,Angled,2x4,Slotted,Standard,80,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-120-C2,Flat,2x4,Slotted,Standard,80,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-277-C2,Angled,2x4,Diffuse,Standard,80,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-277-C2,Flat,2x4,Diffuse,Standard,80,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-277-C2,Angled,2x4,Slotted,Standard,80,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-277-C2,Flat,2x4,Slotted,Standard,80,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-120-C3,Angled,2x4,Diffuse,Standard,80,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-S -8-120-C3,Flat,2x4,Diffuse,Standard,80,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-S -8-120-C3,Angled,2x4,Slotted,Standard,80,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-S -8-120-C3,Flat,2x4,Slotted,Standard,80,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-S -8-277-C3,Angled,2x4,Diffuse,Standard,80,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-S -8-277-C3,Flat,2x4,Diffuse,Standard,80,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-S -8-277-C3,Angled,2x4,Slotted,Standard,80,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-S -8-277-C3,Flat,2x4,Slotted,Standard,80,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-S -8-120-DW,Angled,2x4,Diffuse,Standard,80,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-S -8-120-DW,Flat,2x4,Diffuse,Standard,80,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-S -8-120-DW,Angled,2x4,Slotted,Standard,80,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-S -8-120-DW,Flat,2x4,Slotted,Standard,80,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-S -8-277-DW,Angled,2x4,Diffuse,Standard,80,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-S -8-277-DW,Flat,2x4,Diffuse,Standard,80,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-S -8-277-DW,Angled,2x4,Slotted,Standard,80,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-S -8-277-DW,Flat,2x4,Slotted,Standard,80,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-S -8-120-C1,Angled Narrow Rail,2x4,Diffuse,Standard,80,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-120-C1,Angled Narrow Rail,2x4,Slotted,Standard,80,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-277-C1,Angled Narrow Rail,2x4,Diffuse,Standard,80,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-277-C1,Angled Narrow Rail,2x4,Slotted,Standard,80,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-120-C2,Angled Narrow Rail,2x4,Diffuse,Standard,80,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-120-C2,Angled Narrow Rail,2x4,Slotted,Standard,80,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-277-C2,Angled Narrow Rail,2x4,Diffuse,Standard,80,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-277-C2,Angled Narrow Rail,2x4,Slotted,Standard,80,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-120-C3,Angled Narrow Rail,2x4,Diffuse,Standard,80,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-S -8-120-C3,Angled Narrow Rail,2x4,Slotted,Standard,80,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-S -8-277-C3,Angled Narrow Rail,2x4,Diffuse,Standard,80,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-S -8-277-C3,Angled Narrow Rail,2x4,Slotted,Standard,80,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-S -8-120-DW,Angled Narrow Rail,2x4,Diffuse,Standard,80,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-S -8-120-DW,Angled Narrow Rail,2x4,Slotted,Standard,80,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-S -8-277-DW,Angled Narrow Rail,2x4,Diffuse,Standard,80,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-S -8-277-DW,Angled Narrow Rail,2x4,Slotted,Standard,80,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-S -8-120-C1,Angled,2x4,Round,Standard,80,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-120-C1,Flat,2x4,Round,Standard,80,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-277-C1,Angled,2x4,Round,Standard,80,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-277-C1,Flat,2x4,Round,Standard,80,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-120-C2,Angled,2x4,Round,Standard,80,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-120-C2,Flat,2x4,Round,Standard,80,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-277-C2,Angled,2x4,Round,Standard,80,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-277-C2,Flat,2x4,Round,Standard,80,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-120-C3,Angled,2x4,Round,Standard,80,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-S -8-120-C3,Flat,2x4,Round,Standard,80,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-S -8-277-C3,Angled,2x4,Round,Standard,80,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-S -8-277-C3,Flat,2x4,Round,Standard,80,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-S -8-120-DW,Angled,2x4,Round,Standard,80,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-S -8-120-DW,Flat,2x4,Round,Standard,80,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-S -8-277-DW,Angled,2x4,Round,Standard,80,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-S -8-277-DW,Flat,2x4,Round,Standard,80,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-S -8-120-C1,Angled Narrow Rail,2x4,Round,Standard,80,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-277-C1,Angled Narrow Rail,2x4,Round,Standard,80,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-120-C2,Angled Narrow Rail,2x4,Round,Standard,80,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-277-C2,Angled Narrow Rail,2x4,Round,Standard,80,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-120-C3,Angled Narrow Rail,2x4,Round,Standard,80,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-S -8-277-C3,Angled Narrow Rail,2x4,Round,Standard,80,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-S -8-120-DW,Angled Narrow Rail,2x4,Round,Standard,80,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-S -8-277-DW,Angled Narrow Rail,2x4,Round,Standard,80,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-S -8-120-C1,Angled,2x4,Diffuse,Standard,80,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-120-C1,Flat,2x4,Diffuse,Standard,80,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-120-C1,Angled,2x4,Slotted,Standard,80,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-120-C1,Flat,2x4,Slotted,Standard,80,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-277-C1,Angled,2x4,Diffuse,Standard,80,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-277-C1,Flat,2x4,Diffuse,Standard,80,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-277-C1,Angled,2x4,Slotted,Standard,80,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-277-C1,Flat,2x4,Slotted,Standard,80,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-120-C2,Angled,2x4,Diffuse,Standard,80,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-120-C2,Flat,2x4,Diffuse,Standard,80,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-120-C2,Angled,2x4,Slotted,Standard,80,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-120-C2,Flat,2x4,Slotted,Standard,80,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-277-C2,Angled,2x4,Diffuse,Standard,80,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-277-C2,Flat,2x4,Diffuse,Standard,80,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-277-C2,Angled,2x4,Slotted,Standard,80,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-277-C2,Flat,2x4,Slotted,Standard,80,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-120-C3,Angled,2x4,Diffuse,Standard,80,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-S -8-120-C3,Flat,2x4,Diffuse,Standard,80,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-S -8-120-C3,Angled,2x4,Slotted,Standard,80,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-S -8-120-C3,Flat,2x4,Slotted,Standard,80,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-S -8-277-C3,Angled,2x4,Diffuse,Standard,80,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-S -8-277-C3,Flat,2x4,Diffuse,Standard,80,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-S -8-277-C3,Angled,2x4,Slotted,Standard,80,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-S -8-277-C3,Flat,2x4,Slotted,Standard,80,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-S -8-120-DW,Angled,2x4,Diffuse,Standard,80,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-S -8-120-DW,Flat,2x4,Diffuse,Standard,80,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-S -8-120-DW,Angled,2x4,Slotted,Standard,80,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-S -8-120-DW,Flat,2x4,Slotted,Standard,80,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-S -8-277-DW,Angled,2x4,Diffuse,Standard,80,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-S -8-277-DW,Flat,2x4,Diffuse,Standard,80,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-S -8-277-DW,Angled,2x4,Slotted,Standard,80,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-S -8-277-DW,Flat,2x4,Slotted,Standard,80,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-S -8-120-C1,Angled Narrow Rail,2x4,Diffuse,Standard,80,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-120-C1,Angled Narrow Rail,2x4,Slotted,Standard,80,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-277-C1,Angled Narrow Rail,2x4,Diffuse,Standard,80,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-277-C1,Angled Narrow Rail,2x4,Slotted,Standard,80,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-120-C2,Angled Narrow Rail,2x4,Diffuse,Standard,80,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-120-C2,Angled Narrow Rail,2x4,Slotted,Standard,80,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-277-C2,Angled Narrow Rail,2x4,Diffuse,Standard,80,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-277-C2,Angled Narrow Rail,2x4,Slotted,Standard,80,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-120-C3,Angled Narrow Rail,2x4,Diffuse,Standard,80,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-S -8-120-C3,Angled Narrow Rail,2x4,Slotted,Standard,80,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-S -8-277-C3,Angled Narrow Rail,2x4,Diffuse,Standard,80,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-S -8-277-C3,Angled Narrow Rail,2x4,Slotted,Standard,80,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-S -8-120-DW,Angled Narrow Rail,2x4,Diffuse,Standard,80,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-S -8-120-DW,Angled Narrow Rail,2x4,Slotted,Standard,80,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-S -8-277-DW,Angled Narrow Rail,2x4,Diffuse,Standard,80,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-S -8-277-DW,Angled Narrow Rail,2x4,Slotted,Standard,80,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-S -8-120-C1,Angled,2x4,Round,Standard,80,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-120-C1,Flat,2x4,Round,Standard,80,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-277-C1,Angled,2x4,Round,Standard,80,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-277-C1,Flat,2x4,Round,Standard,80,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-120-C2,Angled,2x4,Round,Standard,80,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-120-C2,Flat,2x4,Round,Standard,80,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-277-C2,Angled,2x4,Round,Standard,80,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-277-C2,Flat,2x4,Round,Standard,80,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-120-C3,Angled,2x4,Round,Standard,80,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-S -8-120-C3,Flat,2x4,Round,Standard,80,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-S -8-277-C3,Angled,2x4,Round,Standard,80,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-S -8-277-C3,Flat,2x4,Round,Standard,80,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-S -8-120-DW,Angled,2x4,Round,Standard,80,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-S -8-120-DW,Flat,2x4,Round,Standard,80,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-S -8-277-DW,Angled,2x4,Round,Standard,80,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-S -8-277-DW,Flat,2x4,Round,Standard,80,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-S -8-120-C1,Angled Narrow Rail,2x4,Round,Standard,80,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-277-C1,Angled Narrow Rail,2x4,Round,Standard,80,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-120-C2,Angled Narrow Rail,2x4,Round,Standard,80,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-277-C2,Angled Narrow Rail,2x4,Round,Standard,80,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-120-C3,Angled Narrow Rail,2x4,Round,Standard,80,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-S -8-277-C3,Angled Narrow Rail,2x4,Round,Standard,80,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-S -8-120-DW,Angled Narrow Rail,2x4,Round,Standard,80,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-S -8-277-DW,Angled Narrow Rail,2x4,Round,Standard,80,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-S -8-120-C1,Angled,2x4,Diffuse,Standard,80,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-120-C1,Flat,2x4,Diffuse,Standard,80,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-120-C1,Angled,2x4,Slotted,Standard,80,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-120-C1,Flat,2x4,Slotted,Standard,80,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-277-C1,Angled,2x4,Diffuse,Standard,80,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-277-C1,Flat,2x4,Diffuse,Standard,80,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-277-C1,Angled,2x4,Slotted,Standard,80,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-277-C1,Flat,2x4,Slotted,Standard,80,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-120-C2,Angled,2x4,Diffuse,Standard,80,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-120-C2,Flat,2x4,Diffuse,Standard,80,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-120-C2,Angled,2x4,Slotted,Standard,80,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-120-C2,Flat,2x4,Slotted,Standard,80,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-277-C2,Angled,2x4,Diffuse,Standard,80,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-277-C2,Flat,2x4,Diffuse,Standard,80,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-277-C2,Angled,2x4,Slotted,Standard,80,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-277-C2,Flat,2x4,Slotted,Standard,80,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-120-C3,Angled,2x4,Diffuse,Standard,80,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-S -8-120-C3,Flat,2x4,Diffuse,Standard,80,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-S -8-120-C3,Angled,2x4,Slotted,Standard,80,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-S -8-120-C3,Flat,2x4,Slotted,Standard,80,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-S -8-277-C3,Angled,2x4,Diffuse,Standard,80,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-S -8-277-C3,Flat,2x4,Diffuse,Standard,80,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-S -8-277-C3,Angled,2x4,Slotted,Standard,80,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-S -8-277-C3,Flat,2x4,Slotted,Standard,80,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-S -8-120-DW,Angled,2x4,Diffuse,Standard,80,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-S -8-120-DW,Flat,2x4,Diffuse,Standard,80,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-S -8-120-DW,Angled,2x4,Slotted,Standard,80,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-S -8-120-DW,Flat,2x4,Slotted,Standard,80,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-S -8-277-DW,Angled,2x4,Diffuse,Standard,80,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-S -8-277-DW,Flat,2x4,Diffuse,Standard,80,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-S -8-277-DW,Angled,2x4,Slotted,Standard,80,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-S -8-277-DW,Flat,2x4,Slotted,Standard,80,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-S -8-120-C1,Angled Narrow Rail,2x4,Diffuse,Standard,80,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-120-C1,Angled Narrow Rail,2x4,Slotted,Standard,80,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-277-C1,Angled Narrow Rail,2x4,Diffuse,Standard,80,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-277-C1,Angled Narrow Rail,2x4,Slotted,Standard,80,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-120-C2,Angled Narrow Rail,2x4,Diffuse,Standard,80,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-120-C2,Angled Narrow Rail,2x4,Slotted,Standard,80,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-277-C2,Angled Narrow Rail,2x4,Diffuse,Standard,80,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-277-C2,Angled Narrow Rail,2x4,Slotted,Standard,80,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-120-C3,Angled Narrow Rail,2x4,Diffuse,Standard,80,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-S -8-120-C3,Angled Narrow Rail,2x4,Slotted,Standard,80,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-S -8-277-C3,Angled Narrow Rail,2x4,Diffuse,Standard,80,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-S -8-277-C3,Angled Narrow Rail,2x4,Slotted,Standard,80,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-S -8-120-DW,Angled Narrow Rail,2x4,Diffuse,Standard,80,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-S -8-120-DW,Angled Narrow Rail,2x4,Slotted,Standard,80,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-S -8-277-DW,Angled Narrow Rail,2x4,Diffuse,Standard,80,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-S -8-277-DW,Angled Narrow Rail,2x4,Slotted,Standard,80,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-S -8-120-C1,Angled,2x4,Round,Standard,80,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-120-C1,Flat,2x4,Round,Standard,80,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-277-C1,Angled,2x4,Round,Standard,80,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-277-C1,Flat,2x4,Round,Standard,80,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-120-C2,Angled,2x4,Round,Standard,80,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-120-C2,Flat,2x4,Round,Standard,80,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-277-C2,Angled,2x4,Round,Standard,80,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-277-C2,Flat,2x4,Round,Standard,80,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-120-C3,Angled,2x4,Round,Standard,80,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-S -8-120-C3,Flat,2x4,Round,Standard,80,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-S -8-277-C3,Angled,2x4,Round,Standard,80,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-S -8-277-C3,Flat,2x4,Round,Standard,80,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-S -8-120-DW,Angled,2x4,Round,Standard,80,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-S -8-120-DW,Flat,2x4,Round,Standard,80,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-S -8-277-DW,Angled,2x4,Round,Standard,80,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-S -8-277-DW,Flat,2x4,Round,Standard,80,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-S -8-120-C1,Angled Narrow Rail,2x4,Round,Standard,80,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-277-C1,Angled Narrow Rail,2x4,Round,Standard,80,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-120-C2,Angled Narrow Rail,2x4,Round,Standard,80,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-277-C2,Angled Narrow Rail,2x4,Round,Standard,80,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-120-C3,Angled Narrow Rail,2x4,Round,Standard,80,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-S -8-277-C3,Angled Narrow Rail,2x4,Round,Standard,80,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-S -8-120-DW,Angled Narrow Rail,2x4,Round,Standard,80,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-S -8-277-DW,Angled Narrow Rail,2x4,Round,Standard,80,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-S -8-120-C2,Angled,2x4,Diffuse,Standard,80,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-120-C2,Flat,2x4,Diffuse,Standard,80,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-120-C2,Angled,2x4,Slotted,Standard,80,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-120-C2,Flat,2x4,Slotted,Standard,80,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-277-C2,Angled,2x4,Diffuse,Standard,80,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-277-C2,Flat,2x4,Diffuse,Standard,80,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-277-C2,Angled,2x4,Slotted,Standard,80,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-277-C2,Flat,2x4,Slotted,Standard,80,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-120-C2,Angled Narrow Rail,2x4,Diffuse,Standard,80,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-120-C2,Angled Narrow Rail,2x4,Slotted,Standard,80,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-277-C2,Angled Narrow Rail,2x4,Diffuse,Standard,80,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-277-C2,Angled Narrow Rail,2x4,Slotted,Standard,80,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-120-C2,Angled,2x4,Round,Standard,80,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-120-C2,Flat,2x4,Round,Standard,80,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-277-C2,Angled,2x4,Round,Standard,80,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-277-C2,Flat,2x4,Round,Standard,80,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-120-C2,Angled Narrow Rail,2x4,Round,Standard,80,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-277-C2,Angled Narrow Rail,2x4,Round,Standard,80,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-120-C2,Angled,2x4,Diffuse,Standard,80,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-120-C2,Flat,2x4,Diffuse,Standard,80,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-120-C2,Angled,2x4,Slotted,Standard,80,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-120-C2,Flat,2x4,Slotted,Standard,80,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-277-C2,Angled,2x4,Diffuse,Standard,80,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-277-C2,Flat,2x4,Diffuse,Standard,80,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-277-C2,Angled,2x4,Slotted,Standard,80,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-277-C2,Flat,2x4,Slotted,Standard,80,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-120-C2,Angled Narrow Rail,2x4,Diffuse,Standard,80,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-120-C2,Angled Narrow Rail,2x4,Slotted,Standard,80,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-277-C2,Angled Narrow Rail,2x4,Diffuse,Standard,80,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-277-C2,Angled Narrow Rail,2x4,Slotted,Standard,80,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-120-C2,Angled,2x4,Round,Standard,80,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-120-C2,Flat,2x4,Round,Standard,80,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-277-C2,Angled,2x4,Round,Standard,80,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-277-C2,Flat,2x4,Round,Standard,80,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-120-C2,Angled Narrow Rail,2x4,Round,Standard,80,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-277-C2,Angled Narrow Rail,2x4,Round,Standard,80,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-120-C2,Angled,2x4,Diffuse,Standard,80,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-120-C2,Flat,2x4,Diffuse,Standard,80,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-120-C2,Angled,2x4,Slotted,Standard,80,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-120-C2,Flat,2x4,Slotted,Standard,80,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-S -8-277-C2,Angled,2x4,Diffuse,Standard,80,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-S -8-277-C2,Flat,2x4,Diffuse,Standard,80,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-S -8-277-C2,Angled,2x4,Slotted,Standard,80,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-S -8-277-C2,Flat,2x4,Slotted,Standard,80,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-120-C2,Angled Narrow Rail,2x4,Diffuse,Standard,80,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-120-C2,Angled Narrow Rail,2x4,Slotted,Standard,80,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -8-277-C2,Angled Narrow Rail,2x4,Diffuse,Standard,80,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -8-277-C2,Angled Narrow Rail,2x4,Slotted,Standard,80,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-120-C2,Angled,2x4,Round,Standard,80,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-120-C2,Flat,2x4,Round,Standard,80,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-S -8-277-C2,Angled,2x4,Round,Standard,80,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-S -8-277-C2,Flat,2x4,Round,Standard,80,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-120-C2,Angled Narrow Rail,2x4,Round,Standard,80,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -8-277-C2,Angled Narrow Rail,2x4,Round,Standard,80,4000K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-120-C1,Wave,2x4,Diffuse,Standard,80,3500K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-277-C1,Wave,2x4,Diffuse,Standard,80,3500K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-120-C2,Wave,2x4,Diffuse,Standard,80,3500K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-277-C2,Wave,2x4,Diffuse,Standard,80,3500K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-120-C3,Wave,2x4,Diffuse,Standard,80,3500K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-S -8-277-C3,Wave,2x4,Diffuse,Standard,80,3500K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-S -8-120-DW,Wave,2x4,Diffuse,Standard,80,3500K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-S -8-277-DW,Wave,2x4,Diffuse,Standard,80,3500K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-S -8-120-C1,Wave,2x4,Diffuse,Standard,80,3000K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-277-C1,Wave,2x4,Diffuse,Standard,80,3000K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-120-C2,Wave,2x4,Diffuse,Standard,80,3000K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-277-C2,Wave,2x4,Diffuse,Standard,80,3000K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-120-C3,Wave,2x4,Diffuse,Standard,80,3000K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-S -8-277-C3,Wave,2x4,Diffuse,Standard,80,3000K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-S -8-120-DW,Wave,2x4,Diffuse,Standard,80,3000K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-S -8-277-DW,Wave,2x4,Diffuse,Standard,80,3000K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-S -8-120-C1,Wave,2x4,Diffuse,Standard,80,4000K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-277-C1,Wave,2x4,Diffuse,Standard,80,4000K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-120-C2,Wave,2x4,Diffuse,Standard,80,4000K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-277-C2,Wave,2x4,Diffuse,Standard,80,4000K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-120-C3,Wave,2x4,Diffuse,Standard,80,4000K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-S -8-277-C3,Wave,2x4,Diffuse,Standard,80,4000K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-S -8-120-DW,Wave,2x4,Diffuse,Standard,80,4000K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-S -8-277-DW,Wave,2x4,Diffuse,Standard,80,4000K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-S -8-120-C2,Wave,2x4,Diffuse,Standard,80,3500K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-277-C2,Wave,2x4,Diffuse,Standard,80,3500K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-120-C2,Wave,2x4,Diffuse,Standard,80,3000K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-277-C2,Wave,2x4,Diffuse,Standard,80,3000K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-120-C2,Wave,2x4,Diffuse,Standard,80,4000K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -8-277-C2,Wave,2x4,Diffuse,Standard,80,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-120-C1,Angled,2x4,Diffuse,Boosted,80,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-120-C1,Flat,2x4,Diffuse,Boosted,80,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-120-C1,Angled,2x4,Slotted,Boosted,80,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-120-C1,Flat,2x4,Slotted,Boosted,80,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-277-C1,Angled,2x4,Diffuse,Boosted,80,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-277-C1,Flat,2x4,Diffuse,Boosted,80,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-277-C1,Angled,2x4,Slotted,Boosted,80,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-277-C1,Flat,2x4,Slotted,Boosted,80,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-120-C2,Angled,2x4,Diffuse,Boosted,80,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-120-C2,Flat,2x4,Diffuse,Boosted,80,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-120-C2,Angled,2x4,Slotted,Boosted,80,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-120-C2,Flat,2x4,Slotted,Boosted,80,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-277-C2,Angled,2x4,Diffuse,Boosted,80,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-277-C2,Flat,2x4,Diffuse,Boosted,80,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-277-C2,Angled,2x4,Slotted,Boosted,80,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-277-C2,Flat,2x4,Slotted,Boosted,80,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-120-C3,Angled,2x4,Diffuse,Boosted,80,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-B-8-120-C3,Flat,2x4,Diffuse,Boosted,80,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-B-8-120-C3,Angled,2x4,Slotted,Boosted,80,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-B-8-120-C3,Flat,2x4,Slotted,Boosted,80,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-B-8-277-C3,Angled,2x4,Diffuse,Boosted,80,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-B-8-277-C3,Flat,2x4,Diffuse,Boosted,80,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-B-8-277-C3,Angled,2x4,Slotted,Boosted,80,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-B-8-277-C3,Flat,2x4,Slotted,Boosted,80,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-B-8-120-DW,Angled,2x4,Diffuse,Boosted,80,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-B-8-120-DW,Flat,2x4,Diffuse,Boosted,80,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-B-8-120-DW,Angled,2x4,Slotted,Boosted,80,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-B-8-120-DW,Flat,2x4,Slotted,Boosted,80,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-B-8-277-DW,Angled,2x4,Diffuse,Boosted,80,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-B-8-277-DW,Flat,2x4,Diffuse,Boosted,80,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-B-8-277-DW,Angled,2x4,Slotted,Boosted,80,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-B-8-277-DW,Flat,2x4,Slotted,Boosted,80,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-B-8-120-C1,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-120-C1,Angled Narrow Rail,2x4,Slotted,Boosted,80,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-277-C1,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-277-C1,Angled Narrow Rail,2x4,Slotted,Boosted,80,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-120-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-120-C2,Angled Narrow Rail,2x4,Slotted,Boosted,80,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-277-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-277-C2,Angled Narrow Rail,2x4,Slotted,Boosted,80,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-120-C3,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-B-8-120-C3,Angled Narrow Rail,2x4,Slotted,Boosted,80,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-B-8-277-C3,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-B-8-277-C3,Angled Narrow Rail,2x4,Slotted,Boosted,80,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-B-8-120-DW,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-B-8-120-DW,Angled Narrow Rail,2x4,Slotted,Boosted,80,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-B-8-277-DW,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-B-8-277-DW,Angled Narrow Rail,2x4,Slotted,Boosted,80,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-B-8-120-C1,Angled,2x4,Round,Boosted,80,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-120-C1,Flat,2x4,Round,Boosted,80,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-277-C1,Angled,2x4,Round,Boosted,80,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-277-C1,Flat,2x4,Round,Boosted,80,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-120-C2,Angled,2x4,Round,Boosted,80,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-120-C2,Flat,2x4,Round,Boosted,80,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-277-C2,Angled,2x4,Round,Boosted,80,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-277-C2,Flat,2x4,Round,Boosted,80,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-120-C3,Angled,2x4,Round,Boosted,80,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-B-8-120-C3,Flat,2x4,Round,Boosted,80,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-B-8-277-C3,Angled,2x4,Round,Boosted,80,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-B-8-277-C3,Flat,2x4,Round,Boosted,80,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-B-8-120-DW,Angled,2x4,Round,Boosted,80,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-B-8-120-DW,Flat,2x4,Round,Boosted,80,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-B-8-277-DW,Angled,2x4,Round,Boosted,80,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-B-8-277-DW,Flat,2x4,Round,Boosted,80,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-B-8-120-C1,Angled Narrow Rail,2x4,Round,Boosted,80,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-277-C1,Angled Narrow Rail,2x4,Round,Boosted,80,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-120-C2,Angled Narrow Rail,2x4,Round,Boosted,80,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-277-C2,Angled Narrow Rail,2x4,Round,Boosted,80,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-120-C3,Angled Narrow Rail,2x4,Round,Boosted,80,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-B-8-277-C3,Angled Narrow Rail,2x4,Round,Boosted,80,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-B-8-120-DW,Angled Narrow Rail,2x4,Round,Boosted,80,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-B-8-277-DW,Angled Narrow Rail,2x4,Round,Boosted,80,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-B-8-120-C1,Angled,2x4,Diffuse,Boosted,80,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-120-C1,Flat,2x4,Diffuse,Boosted,80,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-120-C1,Angled,2x4,Slotted,Boosted,80,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-120-C1,Flat,2x4,Slotted,Boosted,80,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-277-C1,Angled,2x4,Diffuse,Boosted,80,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-277-C1,Flat,2x4,Diffuse,Boosted,80,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-277-C1,Angled,2x4,Slotted,Boosted,80,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-277-C1,Flat,2x4,Slotted,Boosted,80,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-120-C2,Angled,2x4,Diffuse,Boosted,80,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-120-C2,Flat,2x4,Diffuse,Boosted,80,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-120-C2,Angled,2x4,Slotted,Boosted,80,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-120-C2,Flat,2x4,Slotted,Boosted,80,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-277-C2,Angled,2x4,Diffuse,Boosted,80,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-277-C2,Flat,2x4,Diffuse,Boosted,80,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-277-C2,Angled,2x4,Slotted,Boosted,80,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-277-C2,Flat,2x4,Slotted,Boosted,80,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-120-C3,Angled,2x4,Diffuse,Boosted,80,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-B-8-120-C3,Flat,2x4,Diffuse,Boosted,80,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-B-8-120-C3,Angled,2x4,Slotted,Boosted,80,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-B-8-120-C3,Flat,2x4,Slotted,Boosted,80,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-B-8-277-C3,Angled,2x4,Diffuse,Boosted,80,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-B-8-277-C3,Flat,2x4,Diffuse,Boosted,80,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-B-8-277-C3,Angled,2x4,Slotted,Boosted,80,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-B-8-277-C3,Flat,2x4,Slotted,Boosted,80,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-B-8-120-DW,Angled,2x4,Diffuse,Boosted,80,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-B-8-120-DW,Flat,2x4,Diffuse,Boosted,80,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-B-8-120-DW,Angled,2x4,Slotted,Boosted,80,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-B-8-120-DW,Flat,2x4,Slotted,Boosted,80,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-B-8-277-DW,Angled,2x4,Diffuse,Boosted,80,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-B-8-277-DW,Flat,2x4,Diffuse,Boosted,80,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-B-8-277-DW,Angled,2x4,Slotted,Boosted,80,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-B-8-277-DW,Flat,2x4,Slotted,Boosted,80,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-B-8-120-C1,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-120-C1,Angled Narrow Rail,2x4,Slotted,Boosted,80,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-277-C1,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-277-C1,Angled Narrow Rail,2x4,Slotted,Boosted,80,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-120-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-120-C2,Angled Narrow Rail,2x4,Slotted,Boosted,80,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-277-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-277-C2,Angled Narrow Rail,2x4,Slotted,Boosted,80,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-120-C3,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-B-8-120-C3,Angled Narrow Rail,2x4,Slotted,Boosted,80,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-B-8-277-C3,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-B-8-277-C3,Angled Narrow Rail,2x4,Slotted,Boosted,80,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-B-8-120-DW,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-B-8-120-DW,Angled Narrow Rail,2x4,Slotted,Boosted,80,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-B-8-277-DW,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-B-8-277-DW,Angled Narrow Rail,2x4,Slotted,Boosted,80,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-B-8-120-C1,Angled,2x4,Round,Boosted,80,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-120-C1,Flat,2x4,Round,Boosted,80,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-277-C1,Angled,2x4,Round,Boosted,80,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-277-C1,Flat,2x4,Round,Boosted,80,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-120-C2,Angled,2x4,Round,Boosted,80,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-120-C2,Flat,2x4,Round,Boosted,80,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-277-C2,Angled,2x4,Round,Boosted,80,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-277-C2,Flat,2x4,Round,Boosted,80,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-120-C3,Angled,2x4,Round,Boosted,80,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-B-8-120-C3,Flat,2x4,Round,Boosted,80,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-B-8-277-C3,Angled,2x4,Round,Boosted,80,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-B-8-277-C3,Flat,2x4,Round,Boosted,80,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-B-8-120-DW,Angled,2x4,Round,Boosted,80,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-B-8-120-DW,Flat,2x4,Round,Boosted,80,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-B-8-277-DW,Angled,2x4,Round,Boosted,80,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-B-8-277-DW,Flat,2x4,Round,Boosted,80,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-B-8-120-C1,Angled Narrow Rail,2x4,Round,Boosted,80,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-277-C1,Angled Narrow Rail,2x4,Round,Boosted,80,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-120-C2,Angled Narrow Rail,2x4,Round,Boosted,80,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-277-C2,Angled Narrow Rail,2x4,Round,Boosted,80,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-120-C3,Angled Narrow Rail,2x4,Round,Boosted,80,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-B-8-277-C3,Angled Narrow Rail,2x4,Round,Boosted,80,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-B-8-120-DW,Angled Narrow Rail,2x4,Round,Boosted,80,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-B-8-277-DW,Angled Narrow Rail,2x4,Round,Boosted,80,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-B-8-120-C1,Angled,2x4,Diffuse,Boosted,80,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-120-C1,Flat,2x4,Diffuse,Boosted,80,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-120-C1,Angled,2x4,Slotted,Boosted,80,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-120-C1,Flat,2x4,Slotted,Boosted,80,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-277-C1,Angled,2x4,Diffuse,Boosted,80,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-277-C1,Flat,2x4,Diffuse,Boosted,80,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-277-C1,Angled,2x4,Slotted,Boosted,80,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-277-C1,Flat,2x4,Slotted,Boosted,80,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-120-C2,Angled,2x4,Diffuse,Boosted,80,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-120-C2,Flat,2x4,Diffuse,Boosted,80,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-120-C2,Angled,2x4,Slotted,Boosted,80,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-120-C2,Flat,2x4,Slotted,Boosted,80,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-277-C2,Angled,2x4,Diffuse,Boosted,80,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-277-C2,Flat,2x4,Diffuse,Boosted,80,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-277-C2,Angled,2x4,Slotted,Boosted,80,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-277-C2,Flat,2x4,Slotted,Boosted,80,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-120-C3,Angled,2x4,Diffuse,Boosted,80,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-B-8-120-C3,Flat,2x4,Diffuse,Boosted,80,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-B-8-120-C3,Angled,2x4,Slotted,Boosted,80,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-B-8-120-C3,Flat,2x4,Slotted,Boosted,80,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-B-8-277-C3,Angled,2x4,Diffuse,Boosted,80,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-B-8-277-C3,Flat,2x4,Diffuse,Boosted,80,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-B-8-277-C3,Angled,2x4,Slotted,Boosted,80,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-B-8-277-C3,Flat,2x4,Slotted,Boosted,80,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-B-8-120-DW,Angled,2x4,Diffuse,Boosted,80,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-B-8-120-DW,Flat,2x4,Diffuse,Boosted,80,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-B-8-120-DW,Angled,2x4,Slotted,Boosted,80,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-B-8-120-DW,Flat,2x4,Slotted,Boosted,80,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-B-8-277-DW,Angled,2x4,Diffuse,Boosted,80,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-B-8-277-DW,Flat,2x4,Diffuse,Boosted,80,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-B-8-277-DW,Angled,2x4,Slotted,Boosted,80,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-B-8-277-DW,Flat,2x4,Slotted,Boosted,80,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-B-8-120-C1,Angled Narrow Rail,2x4,Diffuse,Boosted,80,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-120-C1,Angled Narrow Rail,2x4,Slotted,Boosted,80,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-277-C1,Angled Narrow Rail,2x4,Diffuse,Boosted,80,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-277-C1,Angled Narrow Rail,2x4,Slotted,Boosted,80,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-120-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,80,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-120-C2,Angled Narrow Rail,2x4,Slotted,Boosted,80,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-277-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,80,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-277-C2,Angled Narrow Rail,2x4,Slotted,Boosted,80,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-120-C3,Angled Narrow Rail,2x4,Diffuse,Boosted,80,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-B-8-120-C3,Angled Narrow Rail,2x4,Slotted,Boosted,80,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-B-8-277-C3,Angled Narrow Rail,2x4,Diffuse,Boosted,80,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-B-8-277-C3,Angled Narrow Rail,2x4,Slotted,Boosted,80,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-B-8-120-DW,Angled Narrow Rail,2x4,Diffuse,Boosted,80,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-B-8-120-DW,Angled Narrow Rail,2x4,Slotted,Boosted,80,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-B-8-277-DW,Angled Narrow Rail,2x4,Diffuse,Boosted,80,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-B-8-277-DW,Angled Narrow Rail,2x4,Slotted,Boosted,80,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-B-8-120-C1,Angled,2x4,Round,Boosted,80,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-120-C1,Flat,2x4,Round,Boosted,80,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-277-C1,Angled,2x4,Round,Boosted,80,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-277-C1,Flat,2x4,Round,Boosted,80,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-120-C2,Angled,2x4,Round,Boosted,80,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-120-C2,Flat,2x4,Round,Boosted,80,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-277-C2,Angled,2x4,Round,Boosted,80,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-277-C2,Flat,2x4,Round,Boosted,80,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-120-C3,Angled,2x4,Round,Boosted,80,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-B-8-120-C3,Flat,2x4,Round,Boosted,80,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-B-8-277-C3,Angled,2x4,Round,Boosted,80,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-B-8-277-C3,Flat,2x4,Round,Boosted,80,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-B-8-120-DW,Angled,2x4,Round,Boosted,80,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-B-8-120-DW,Flat,2x4,Round,Boosted,80,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-B-8-277-DW,Angled,2x4,Round,Boosted,80,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-B-8-277-DW,Flat,2x4,Round,Boosted,80,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-B-8-120-C1,Angled Narrow Rail,2x4,Round,Boosted,80,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-277-C1,Angled Narrow Rail,2x4,Round,Boosted,80,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-120-C2,Angled Narrow Rail,2x4,Round,Boosted,80,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-277-C2,Angled Narrow Rail,2x4,Round,Boosted,80,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-120-C3,Angled Narrow Rail,2x4,Round,Boosted,80,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-B-8-277-C3,Angled Narrow Rail,2x4,Round,Boosted,80,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-B-8-120-DW,Angled Narrow Rail,2x4,Round,Boosted,80,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-B-8-277-DW,Angled Narrow Rail,2x4,Round,Boosted,80,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-B-8-120-C2,Angled,2x4,Diffuse,Boosted,80,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-120-C2,Flat,2x4,Diffuse,Boosted,80,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-120-C2,Angled,2x4,Slotted,Boosted,80,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-120-C2,Flat,2x4,Slotted,Boosted,80,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-277-C2,Angled,2x4,Diffuse,Boosted,80,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-277-C2,Flat,2x4,Diffuse,Boosted,80,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-277-C2,Angled,2x4,Slotted,Boosted,80,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-277-C2,Flat,2x4,Slotted,Boosted,80,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-120-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-120-C2,Angled Narrow Rail,2x4,Slotted,Boosted,80,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-277-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-277-C2,Angled Narrow Rail,2x4,Slotted,Boosted,80,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-120-C2,Angled,2x4,Round,Boosted,80,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-120-C2,Flat,2x4,Round,Boosted,80,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-277-C2,Angled,2x4,Round,Boosted,80,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-277-C2,Flat,2x4,Round,Boosted,80,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-120-C2,Angled Narrow Rail,2x4,Round,Boosted,80,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-277-C2,Angled Narrow Rail,2x4,Round,Boosted,80,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-120-C2,Angled,2x4,Diffuse,Boosted,80,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-120-C2,Flat,2x4,Diffuse,Boosted,80,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-120-C2,Angled,2x4,Slotted,Boosted,80,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-120-C2,Flat,2x4,Slotted,Boosted,80,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-277-C2,Angled,2x4,Diffuse,Boosted,80,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-277-C2,Flat,2x4,Diffuse,Boosted,80,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-277-C2,Angled,2x4,Slotted,Boosted,80,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-277-C2,Flat,2x4,Slotted,Boosted,80,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-120-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-120-C2,Angled Narrow Rail,2x4,Slotted,Boosted,80,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-277-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,80,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-277-C2,Angled Narrow Rail,2x4,Slotted,Boosted,80,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-120-C2,Angled,2x4,Round,Boosted,80,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-120-C2,Flat,2x4,Round,Boosted,80,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-277-C2,Angled,2x4,Round,Boosted,80,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-277-C2,Flat,2x4,Round,Boosted,80,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-120-C2,Angled Narrow Rail,2x4,Round,Boosted,80,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-277-C2,Angled Narrow Rail,2x4,Round,Boosted,80,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-120-C2,Angled,2x4,Diffuse,Boosted,80,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-120-C2,Flat,2x4,Diffuse,Boosted,80,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-120-C2,Angled,2x4,Slotted,Boosted,80,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-120-C2,Flat,2x4,Slotted,Boosted,80,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-B-8-277-C2,Angled,2x4,Diffuse,Boosted,80,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-B-8-277-C2,Flat,2x4,Diffuse,Boosted,80,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-B-8-277-C2,Angled,2x4,Slotted,Boosted,80,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-B-8-277-C2,Flat,2x4,Slotted,Boosted,80,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-120-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,80,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-120-C2,Angled Narrow Rail,2x4,Slotted,Boosted,80,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-8-277-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,80,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-8-277-C2,Angled Narrow Rail,2x4,Slotted,Boosted,80,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-120-C2,Angled,2x4,Round,Boosted,80,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-120-C2,Flat,2x4,Round,Boosted,80,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-B-8-277-C2,Angled,2x4,Round,Boosted,80,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-B-8-277-C2,Flat,2x4,Round,Boosted,80,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-120-C2,Angled Narrow Rail,2x4,Round,Boosted,80,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-8-277-C2,Angled Narrow Rail,2x4,Round,Boosted,80,4000K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-120-C1,Wave,2x4,Diffuse,Boosted,80,3500K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-277-C1,Wave,2x4,Diffuse,Boosted,80,3500K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-120-C2,Wave,2x4,Diffuse,Boosted,80,3500K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-277-C2,Wave,2x4,Diffuse,Boosted,80,3500K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-120-C3,Wave,2x4,Diffuse,Boosted,80,3500K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-B-8-277-C3,Wave,2x4,Diffuse,Boosted,80,3500K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-B-8-120-DW,Wave,2x4,Diffuse,Boosted,80,3500K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-B-8-277-DW,Wave,2x4,Diffuse,Boosted,80,3500K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-B-8-120-C1,Wave,2x4,Diffuse,Boosted,80,3000K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-277-C1,Wave,2x4,Diffuse,Boosted,80,3000K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-120-C2,Wave,2x4,Diffuse,Boosted,80,3000K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-277-C2,Wave,2x4,Diffuse,Boosted,80,3000K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-120-C3,Wave,2x4,Diffuse,Boosted,80,3000K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-B-8-277-C3,Wave,2x4,Diffuse,Boosted,80,3000K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-B-8-120-DW,Wave,2x4,Diffuse,Boosted,80,3000K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-B-8-277-DW,Wave,2x4,Diffuse,Boosted,80,3000K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-B-8-120-C1,Wave,2x4,Diffuse,Boosted,80,4000K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-277-C1,Wave,2x4,Diffuse,Boosted,80,4000K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-120-C2,Wave,2x4,Diffuse,Boosted,80,4000K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-277-C2,Wave,2x4,Diffuse,Boosted,80,4000K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-120-C3,Wave,2x4,Diffuse,Boosted,80,4000K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-B-8-277-C3,Wave,2x4,Diffuse,Boosted,80,4000K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-B-8-120-DW,Wave,2x4,Diffuse,Boosted,80,4000K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-B-8-277-DW,Wave,2x4,Diffuse,Boosted,80,4000K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-B-8-120-C2,Wave,2x4,Diffuse,Boosted,80,3500K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-277-C2,Wave,2x4,Diffuse,Boosted,80,3500K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-120-C2,Wave,2x4,Diffuse,Boosted,80,3000K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-277-C2,Wave,2x4,Diffuse,Boosted,80,3000K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-120-C2,Wave,2x4,Diffuse,Boosted,80,4000K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-8-277-C2,Wave,2x4,Diffuse,Boosted,80,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-120-C1,Angled,2x4,Diffuse,High,80,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-120-C1,Flat,2x4,Diffuse,High,80,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-120-C1,Angled,2x4,Slotted,High,80,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-120-C1,Flat,2x4,Slotted,High,80,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-277-C1,Angled,2x4,Diffuse,High,80,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-277-C1,Flat,2x4,Diffuse,High,80,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-277-C1,Angled,2x4,Slotted,High,80,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-277-C1,Flat,2x4,Slotted,High,80,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-120-C2,Angled,2x4,Diffuse,High,80,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-120-C2,Flat,2x4,Diffuse,High,80,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-120-C2,Angled,2x4,Slotted,High,80,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-120-C2,Flat,2x4,Slotted,High,80,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-277-C2,Angled,2x4,Diffuse,High,80,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-277-C2,Flat,2x4,Diffuse,High,80,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-277-C2,Angled,2x4,Slotted,High,80,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-277-C2,Flat,2x4,Slotted,High,80,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-120-C3,Angled,2x4,Diffuse,High,80,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-H -8-120-C3,Flat,2x4,Diffuse,High,80,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-H -8-120-C3,Angled,2x4,Slotted,High,80,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-H -8-120-C3,Flat,2x4,Slotted,High,80,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-H -8-277-C3,Angled,2x4,Diffuse,High,80,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-H -8-277-C3,Flat,2x4,Diffuse,High,80,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-H -8-277-C3,Angled,2x4,Slotted,High,80,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-H -8-277-C3,Flat,2x4,Slotted,High,80,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-H -8-120-DW,Angled,2x4,Diffuse,High,80,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-H -8-120-DW,Flat,2x4,Diffuse,High,80,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-H -8-120-DW,Angled,2x4,Slotted,High,80,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-H -8-120-DW,Flat,2x4,Slotted,High,80,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-H -8-277-DW,Angled,2x4,Diffuse,High,80,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-H -8-277-DW,Flat,2x4,Diffuse,High,80,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-H -8-277-DW,Angled,2x4,Slotted,High,80,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-H -8-277-DW,Flat,2x4,Slotted,High,80,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-H -8-120-C1,Angled Narrow Rail,2x4,Diffuse,High,80,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-120-C1,Angled Narrow Rail,2x4,Slotted,High,80,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-277-C1,Angled Narrow Rail,2x4,Diffuse,High,80,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-277-C1,Angled Narrow Rail,2x4,Slotted,High,80,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-120-C2,Angled Narrow Rail,2x4,Diffuse,High,80,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-120-C2,Angled Narrow Rail,2x4,Slotted,High,80,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-277-C2,Angled Narrow Rail,2x4,Diffuse,High,80,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-277-C2,Angled Narrow Rail,2x4,Slotted,High,80,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-120-C3,Angled Narrow Rail,2x4,Diffuse,High,80,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-H -8-120-C3,Angled Narrow Rail,2x4,Slotted,High,80,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-H -8-277-C3,Angled Narrow Rail,2x4,Diffuse,High,80,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-H -8-277-C3,Angled Narrow Rail,2x4,Slotted,High,80,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-H -8-120-DW,Angled Narrow Rail,2x4,Diffuse,High,80,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-H -8-120-DW,Angled Narrow Rail,2x4,Slotted,High,80,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-H -8-277-DW,Angled Narrow Rail,2x4,Diffuse,High,80,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-H -8-277-DW,Angled Narrow Rail,2x4,Slotted,High,80,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-H -8-120-C1,Angled,2x4,Round,High,80,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-120-C1,Flat,2x4,Round,High,80,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-277-C1,Angled,2x4,Round,High,80,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-277-C1,Flat,2x4,Round,High,80,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-120-C2,Angled,2x4,Round,High,80,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-120-C2,Flat,2x4,Round,High,80,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-277-C2,Angled,2x4,Round,High,80,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-277-C2,Flat,2x4,Round,High,80,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-120-C3,Angled,2x4,Round,High,80,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-H -8-120-C3,Flat,2x4,Round,High,80,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-H -8-277-C3,Angled,2x4,Round,High,80,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-H -8-277-C3,Flat,2x4,Round,High,80,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-H -8-120-DW,Angled,2x4,Round,High,80,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-H -8-120-DW,Flat,2x4,Round,High,80,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-H -8-277-DW,Angled,2x4,Round,High,80,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-H -8-277-DW,Flat,2x4,Round,High,80,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-H -8-120-C1,Angled Narrow Rail,2x4,Round,High,80,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-277-C1,Angled Narrow Rail,2x4,Round,High,80,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-120-C2,Angled Narrow Rail,2x4,Round,High,80,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-277-C2,Angled Narrow Rail,2x4,Round,High,80,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-120-C3,Angled Narrow Rail,2x4,Round,High,80,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-H -8-277-C3,Angled Narrow Rail,2x4,Round,High,80,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-H -8-120-DW,Angled Narrow Rail,2x4,Round,High,80,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-H -8-277-DW,Angled Narrow Rail,2x4,Round,High,80,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-H -8-120-C1,Angled,2x4,Diffuse,High,80,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-120-C1,Flat,2x4,Diffuse,High,80,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-120-C1,Angled,2x4,Slotted,High,80,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-120-C1,Flat,2x4,Slotted,High,80,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-277-C1,Angled,2x4,Diffuse,High,80,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-277-C1,Flat,2x4,Diffuse,High,80,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-277-C1,Angled,2x4,Slotted,High,80,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-277-C1,Flat,2x4,Slotted,High,80,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-120-C2,Angled,2x4,Diffuse,High,80,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-120-C2,Flat,2x4,Diffuse,High,80,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-120-C2,Angled,2x4,Slotted,High,80,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-120-C2,Flat,2x4,Slotted,High,80,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-277-C2,Angled,2x4,Diffuse,High,80,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-277-C2,Flat,2x4,Diffuse,High,80,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-277-C2,Angled,2x4,Slotted,High,80,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-277-C2,Flat,2x4,Slotted,High,80,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-120-C3,Angled,2x4,Diffuse,High,80,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-H -8-120-C3,Flat,2x4,Diffuse,High,80,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-H -8-120-C3,Angled,2x4,Slotted,High,80,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-H -8-120-C3,Flat,2x4,Slotted,High,80,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-H -8-277-C3,Angled,2x4,Diffuse,High,80,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-H -8-277-C3,Flat,2x4,Diffuse,High,80,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-H -8-277-C3,Angled,2x4,Slotted,High,80,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-H -8-277-C3,Flat,2x4,Slotted,High,80,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-H -8-120-DW,Angled,2x4,Diffuse,High,80,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-H -8-120-DW,Flat,2x4,Diffuse,High,80,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-H -8-120-DW,Angled,2x4,Slotted,High,80,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-H -8-120-DW,Flat,2x4,Slotted,High,80,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-H -8-277-DW,Angled,2x4,Diffuse,High,80,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-H -8-277-DW,Flat,2x4,Diffuse,High,80,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-H -8-277-DW,Angled,2x4,Slotted,High,80,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-H -8-277-DW,Flat,2x4,Slotted,High,80,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-H -8-120-C1,Angled Narrow Rail,2x4,Diffuse,High,80,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-120-C1,Angled Narrow Rail,2x4,Slotted,High,80,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-277-C1,Angled Narrow Rail,2x4,Diffuse,High,80,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-277-C1,Angled Narrow Rail,2x4,Slotted,High,80,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-120-C2,Angled Narrow Rail,2x4,Diffuse,High,80,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-120-C2,Angled Narrow Rail,2x4,Slotted,High,80,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-277-C2,Angled Narrow Rail,2x4,Diffuse,High,80,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-277-C2,Angled Narrow Rail,2x4,Slotted,High,80,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-120-C3,Angled Narrow Rail,2x4,Diffuse,High,80,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-H -8-120-C3,Angled Narrow Rail,2x4,Slotted,High,80,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-H -8-277-C3,Angled Narrow Rail,2x4,Diffuse,High,80,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-H -8-277-C3,Angled Narrow Rail,2x4,Slotted,High,80,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-H -8-120-DW,Angled Narrow Rail,2x4,Diffuse,High,80,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-H -8-120-DW,Angled Narrow Rail,2x4,Slotted,High,80,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-H -8-277-DW,Angled Narrow Rail,2x4,Diffuse,High,80,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-H -8-277-DW,Angled Narrow Rail,2x4,Slotted,High,80,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-H -8-120-C1,Angled,2x4,Round,High,80,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-120-C1,Flat,2x4,Round,High,80,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-277-C1,Angled,2x4,Round,High,80,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-277-C1,Flat,2x4,Round,High,80,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-120-C2,Angled,2x4,Round,High,80,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-120-C2,Flat,2x4,Round,High,80,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-277-C2,Angled,2x4,Round,High,80,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-277-C2,Flat,2x4,Round,High,80,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-120-C3,Angled,2x4,Round,High,80,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-H -8-120-C3,Flat,2x4,Round,High,80,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-H -8-277-C3,Angled,2x4,Round,High,80,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-H -8-277-C3,Flat,2x4,Round,High,80,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-H -8-120-DW,Angled,2x4,Round,High,80,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-H -8-120-DW,Flat,2x4,Round,High,80,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-H -8-277-DW,Angled,2x4,Round,High,80,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-H -8-277-DW,Flat,2x4,Round,High,80,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-H -8-120-C1,Angled Narrow Rail,2x4,Round,High,80,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-277-C1,Angled Narrow Rail,2x4,Round,High,80,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-120-C2,Angled Narrow Rail,2x4,Round,High,80,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-277-C2,Angled Narrow Rail,2x4,Round,High,80,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-120-C3,Angled Narrow Rail,2x4,Round,High,80,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-H -8-277-C3,Angled Narrow Rail,2x4,Round,High,80,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-H -8-120-DW,Angled Narrow Rail,2x4,Round,High,80,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-H -8-277-DW,Angled Narrow Rail,2x4,Round,High,80,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-H -8-120-C1,Angled,2x4,Diffuse,High,80,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-120-C1,Flat,2x4,Diffuse,High,80,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-120-C1,Angled,2x4,Slotted,High,80,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-120-C1,Flat,2x4,Slotted,High,80,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-277-C1,Angled,2x4,Diffuse,High,80,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-277-C1,Flat,2x4,Diffuse,High,80,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-277-C1,Angled,2x4,Slotted,High,80,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-277-C1,Flat,2x4,Slotted,High,80,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-120-C2,Angled,2x4,Diffuse,High,80,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-120-C2,Flat,2x4,Diffuse,High,80,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-120-C2,Angled,2x4,Slotted,High,80,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-120-C2,Flat,2x4,Slotted,High,80,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-277-C2,Angled,2x4,Diffuse,High,80,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-277-C2,Flat,2x4,Diffuse,High,80,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-277-C2,Angled,2x4,Slotted,High,80,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-277-C2,Flat,2x4,Slotted,High,80,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-120-C3,Angled,2x4,Diffuse,High,80,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-H -8-120-C3,Flat,2x4,Diffuse,High,80,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-H -8-120-C3,Angled,2x4,Slotted,High,80,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-H -8-120-C3,Flat,2x4,Slotted,High,80,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-H -8-277-C3,Angled,2x4,Diffuse,High,80,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-H -8-277-C3,Flat,2x4,Diffuse,High,80,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-H -8-277-C3,Angled,2x4,Slotted,High,80,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-H -8-277-C3,Flat,2x4,Slotted,High,80,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-H -8-120-DW,Angled,2x4,Diffuse,High,80,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-H -8-120-DW,Flat,2x4,Diffuse,High,80,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-H -8-120-DW,Angled,2x4,Slotted,High,80,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-H -8-120-DW,Flat,2x4,Slotted,High,80,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-H -8-277-DW,Angled,2x4,Diffuse,High,80,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-H -8-277-DW,Flat,2x4,Diffuse,High,80,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-H -8-277-DW,Angled,2x4,Slotted,High,80,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-H -8-277-DW,Flat,2x4,Slotted,High,80,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-H -8-120-C1,Angled Narrow Rail,2x4,Diffuse,High,80,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-120-C1,Angled Narrow Rail,2x4,Slotted,High,80,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-277-C1,Angled Narrow Rail,2x4,Diffuse,High,80,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-277-C1,Angled Narrow Rail,2x4,Slotted,High,80,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-120-C2,Angled Narrow Rail,2x4,Diffuse,High,80,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-120-C2,Angled Narrow Rail,2x4,Slotted,High,80,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-277-C2,Angled Narrow Rail,2x4,Diffuse,High,80,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-277-C2,Angled Narrow Rail,2x4,Slotted,High,80,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-120-C3,Angled Narrow Rail,2x4,Diffuse,High,80,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-H -8-120-C3,Angled Narrow Rail,2x4,Slotted,High,80,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-H -8-277-C3,Angled Narrow Rail,2x4,Diffuse,High,80,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-H -8-277-C3,Angled Narrow Rail,2x4,Slotted,High,80,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-H -8-120-DW,Angled Narrow Rail,2x4,Diffuse,High,80,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-H -8-120-DW,Angled Narrow Rail,2x4,Slotted,High,80,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-H -8-277-DW,Angled Narrow Rail,2x4,Diffuse,High,80,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-H -8-277-DW,Angled Narrow Rail,2x4,Slotted,High,80,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-H -8-120-C1,Angled,2x4,Round,High,80,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-120-C1,Flat,2x4,Round,High,80,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-277-C1,Angled,2x4,Round,High,80,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-277-C1,Flat,2x4,Round,High,80,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-120-C2,Angled,2x4,Round,High,80,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-120-C2,Flat,2x4,Round,High,80,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-277-C2,Angled,2x4,Round,High,80,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-277-C2,Flat,2x4,Round,High,80,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-120-C3,Angled,2x4,Round,High,80,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-H -8-120-C3,Flat,2x4,Round,High,80,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-H -8-277-C3,Angled,2x4,Round,High,80,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-H -8-277-C3,Flat,2x4,Round,High,80,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-H -8-120-DW,Angled,2x4,Round,High,80,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-H -8-120-DW,Flat,2x4,Round,High,80,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-H -8-277-DW,Angled,2x4,Round,High,80,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-H -8-277-DW,Flat,2x4,Round,High,80,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-H -8-120-C1,Angled Narrow Rail,2x4,Round,High,80,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-277-C1,Angled Narrow Rail,2x4,Round,High,80,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-120-C2,Angled Narrow Rail,2x4,Round,High,80,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-277-C2,Angled Narrow Rail,2x4,Round,High,80,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-120-C3,Angled Narrow Rail,2x4,Round,High,80,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-H -8-277-C3,Angled Narrow Rail,2x4,Round,High,80,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-H -8-120-DW,Angled Narrow Rail,2x4,Round,High,80,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-H -8-277-DW,Angled Narrow Rail,2x4,Round,High,80,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-H -8-120-C2,Angled,2x4,Diffuse,High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-120-C2,Flat,2x4,Diffuse,High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-120-C2,Angled,2x4,Slotted,High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-120-C2,Flat,2x4,Slotted,High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-277-C2,Angled,2x4,Diffuse,High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-277-C2,Flat,2x4,Diffuse,High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-277-C2,Angled,2x4,Slotted,High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-277-C2,Flat,2x4,Slotted,High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-120-C2,Angled Narrow Rail,2x4,Diffuse,High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-120-C2,Angled Narrow Rail,2x4,Slotted,High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-277-C2,Angled Narrow Rail,2x4,Diffuse,High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-277-C2,Angled Narrow Rail,2x4,Slotted,High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-120-C2,Angled,2x4,Round,High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-120-C2,Flat,2x4,Round,High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-277-C2,Angled,2x4,Round,High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-277-C2,Flat,2x4,Round,High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-120-C2,Angled Narrow Rail,2x4,Round,High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-277-C2,Angled Narrow Rail,2x4,Round,High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-120-C2,Angled,2x4,Diffuse,High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-120-C2,Flat,2x4,Diffuse,High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-120-C2,Angled,2x4,Slotted,High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-120-C2,Flat,2x4,Slotted,High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-277-C2,Angled,2x4,Diffuse,High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-277-C2,Flat,2x4,Diffuse,High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-277-C2,Angled,2x4,Slotted,High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-277-C2,Flat,2x4,Slotted,High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-120-C2,Angled Narrow Rail,2x4,Diffuse,High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-120-C2,Angled Narrow Rail,2x4,Slotted,High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-277-C2,Angled Narrow Rail,2x4,Diffuse,High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-277-C2,Angled Narrow Rail,2x4,Slotted,High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-120-C2,Angled,2x4,Round,High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-120-C2,Flat,2x4,Round,High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-277-C2,Angled,2x4,Round,High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-277-C2,Flat,2x4,Round,High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-120-C2,Angled Narrow Rail,2x4,Round,High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-277-C2,Angled Narrow Rail,2x4,Round,High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-120-C2,Angled,2x4,Diffuse,High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-120-C2,Flat,2x4,Diffuse,High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-120-C2,Angled,2x4,Slotted,High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-120-C2,Flat,2x4,Slotted,High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-H -8-277-C2,Angled,2x4,Diffuse,High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-H -8-277-C2,Flat,2x4,Diffuse,High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-H -8-277-C2,Angled,2x4,Slotted,High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-H -8-277-C2,Flat,2x4,Slotted,High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-120-C2,Angled Narrow Rail,2x4,Diffuse,High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-120-C2,Angled Narrow Rail,2x4,Slotted,High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -8-277-C2,Angled Narrow Rail,2x4,Diffuse,High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -8-277-C2,Angled Narrow Rail,2x4,Slotted,High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-120-C2,Angled,2x4,Round,High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-120-C2,Flat,2x4,Round,High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-H -8-277-C2,Angled,2x4,Round,High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-H -8-277-C2,Flat,2x4,Round,High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-120-C2,Angled Narrow Rail,2x4,Round,High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -8-277-C2,Angled Narrow Rail,2x4,Round,High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-120-C1,Wave,2x4,Diffuse,High,80,3500K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-277-C1,Wave,2x4,Diffuse,High,80,3500K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-120-C2,Wave,2x4,Diffuse,High,80,3500K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-277-C2,Wave,2x4,Diffuse,High,80,3500K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-120-C3,Wave,2x4,Diffuse,High,80,3500K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-H -8-277-C3,Wave,2x4,Diffuse,High,80,3500K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-H -8-120-DW,Wave,2x4,Diffuse,High,80,3500K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-H -8-277-DW,Wave,2x4,Diffuse,High,80,3500K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-H -8-120-C1,Wave,2x4,Diffuse,High,80,3000K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-277-C1,Wave,2x4,Diffuse,High,80,3000K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-120-C2,Wave,2x4,Diffuse,High,80,3000K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-277-C2,Wave,2x4,Diffuse,High,80,3000K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-120-C3,Wave,2x4,Diffuse,High,80,3000K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-H -8-277-C3,Wave,2x4,Diffuse,High,80,3000K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-H -8-120-DW,Wave,2x4,Diffuse,High,80,3000K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-H -8-277-DW,Wave,2x4,Diffuse,High,80,3000K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-H -8-120-C1,Wave,2x4,Diffuse,High,80,4000K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-277-C1,Wave,2x4,Diffuse,High,80,4000K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-120-C2,Wave,2x4,Diffuse,High,80,4000K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-277-C2,Wave,2x4,Diffuse,High,80,4000K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-120-C3,Wave,2x4,Diffuse,High,80,4000K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-H -8-277-C3,Wave,2x4,Diffuse,High,80,4000K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-H -8-120-DW,Wave,2x4,Diffuse,High,80,4000K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-H -8-277-DW,Wave,2x4,Diffuse,High,80,4000K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-H -8-120-C2,Wave,2x4,Diffuse,High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-277-C2,Wave,2x4,Diffuse,High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-120-C2,Wave,2x4,Diffuse,High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-277-C2,Wave,2x4,Diffuse,High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-120-C2,Wave,2x4,Diffuse,High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -8-277-C2,Wave,2x4,Diffuse,High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-120-C1,Angled,2x4,Diffuse,Very High,80,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-120-C1,Flat,2x4,Diffuse,Very High,80,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-120-C1,Angled,2x4,Slotted,Very High,80,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-120-C1,Flat,2x4,Slotted,Very High,80,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-277-C1,Angled,2x4,Diffuse,Very High,80,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-277-C1,Flat,2x4,Diffuse,Very High,80,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-277-C1,Angled,2x4,Slotted,Very High,80,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-277-C1,Flat,2x4,Slotted,Very High,80,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-120-C2,Angled,2x4,Diffuse,Very High,80,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-120-C2,Flat,2x4,Diffuse,Very High,80,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-120-C2,Angled,2x4,Slotted,Very High,80,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-120-C2,Flat,2x4,Slotted,Very High,80,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-277-C2,Angled,2x4,Diffuse,Very High,80,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-277-C2,Flat,2x4,Diffuse,Very High,80,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-277-C2,Angled,2x4,Slotted,Very High,80,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-277-C2,Flat,2x4,Slotted,Very High,80,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-120-C3,Angled,2x4,Diffuse,Very High,80,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-V-8-120-C3,Flat,2x4,Diffuse,Very High,80,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-V-8-120-C3,Angled,2x4,Slotted,Very High,80,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-V-8-120-C3,Flat,2x4,Slotted,Very High,80,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-V-8-277-C3,Angled,2x4,Diffuse,Very High,80,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-V-8-277-C3,Flat,2x4,Diffuse,Very High,80,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-V-8-277-C3,Angled,2x4,Slotted,Very High,80,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-V-8-277-C3,Flat,2x4,Slotted,Very High,80,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-V-8-120-DW,Angled,2x4,Diffuse,Very High,80,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-V-8-120-DW,Flat,2x4,Diffuse,Very High,80,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-V-8-120-DW,Angled,2x4,Slotted,Very High,80,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-V-8-120-DW,Flat,2x4,Slotted,Very High,80,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-V-8-277-DW,Angled,2x4,Diffuse,Very High,80,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-V-8-277-DW,Flat,2x4,Diffuse,Very High,80,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-V-8-277-DW,Angled,2x4,Slotted,Very High,80,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-V-8-277-DW,Flat,2x4,Slotted,Very High,80,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-V-8-120-C1,Angled Narrow Rail,2x4,Diffuse,Very High,80,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-120-C1,Angled Narrow Rail,2x4,Slotted,Very High,80,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-277-C1,Angled Narrow Rail,2x4,Diffuse,Very High,80,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-277-C1,Angled Narrow Rail,2x4,Slotted,Very High,80,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-120-C2,Angled Narrow Rail,2x4,Diffuse,Very High,80,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-120-C2,Angled Narrow Rail,2x4,Slotted,Very High,80,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-277-C2,Angled Narrow Rail,2x4,Diffuse,Very High,80,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-277-C2,Angled Narrow Rail,2x4,Slotted,Very High,80,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-120-C3,Angled Narrow Rail,2x4,Diffuse,Very High,80,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-V-8-120-C3,Angled Narrow Rail,2x4,Slotted,Very High,80,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-V-8-277-C3,Angled Narrow Rail,2x4,Diffuse,Very High,80,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-V-8-277-C3,Angled Narrow Rail,2x4,Slotted,Very High,80,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-V-8-120-DW,Angled Narrow Rail,2x4,Diffuse,Very High,80,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-V-8-120-DW,Angled Narrow Rail,2x4,Slotted,Very High,80,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-V-8-277-DW,Angled Narrow Rail,2x4,Diffuse,Very High,80,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-V-8-277-DW,Angled Narrow Rail,2x4,Slotted,Very High,80,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-V-8-120-C1,Angled,2x4,Round,Very High,80,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-120-C1,Flat,2x4,Round,Very High,80,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-277-C1,Angled,2x4,Round,Very High,80,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-277-C1,Flat,2x4,Round,Very High,80,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-120-C2,Angled,2x4,Round,Very High,80,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-120-C2,Flat,2x4,Round,Very High,80,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-277-C2,Angled,2x4,Round,Very High,80,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-277-C2,Flat,2x4,Round,Very High,80,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-120-C3,Angled,2x4,Round,Very High,80,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-V-8-120-C3,Flat,2x4,Round,Very High,80,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-V-8-277-C3,Angled,2x4,Round,Very High,80,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-V-8-277-C3,Flat,2x4,Round,Very High,80,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-V-8-120-DW,Angled,2x4,Round,Very High,80,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-V-8-120-DW,Flat,2x4,Round,Very High,80,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-V-8-277-DW,Angled,2x4,Round,Very High,80,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-V-8-277-DW,Flat,2x4,Round,Very High,80,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-V-8-120-C1,Angled Narrow Rail,2x4,Round,Very High,80,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-277-C1,Angled Narrow Rail,2x4,Round,Very High,80,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-120-C2,Angled Narrow Rail,2x4,Round,Very High,80,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-277-C2,Angled Narrow Rail,2x4,Round,Very High,80,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-120-C3,Angled Narrow Rail,2x4,Round,Very High,80,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-V-8-277-C3,Angled Narrow Rail,2x4,Round,Very High,80,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-V-8-120-DW,Angled Narrow Rail,2x4,Round,Very High,80,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-V-8-277-DW,Angled Narrow Rail,2x4,Round,Very High,80,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-V-8-120-C1,Angled,2x4,Diffuse,Very High,80,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-120-C1,Flat,2x4,Diffuse,Very High,80,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-120-C1,Angled,2x4,Slotted,Very High,80,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-120-C1,Flat,2x4,Slotted,Very High,80,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-277-C1,Angled,2x4,Diffuse,Very High,80,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-277-C1,Flat,2x4,Diffuse,Very High,80,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-277-C1,Angled,2x4,Slotted,Very High,80,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-277-C1,Flat,2x4,Slotted,Very High,80,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-120-C2,Angled,2x4,Diffuse,Very High,80,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-120-C2,Flat,2x4,Diffuse,Very High,80,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-120-C2,Angled,2x4,Slotted,Very High,80,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-120-C2,Flat,2x4,Slotted,Very High,80,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-277-C2,Angled,2x4,Diffuse,Very High,80,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-277-C2,Flat,2x4,Diffuse,Very High,80,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-277-C2,Angled,2x4,Slotted,Very High,80,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-277-C2,Flat,2x4,Slotted,Very High,80,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-120-C3,Angled,2x4,Diffuse,Very High,80,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-V-8-120-C3,Flat,2x4,Diffuse,Very High,80,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-V-8-120-C3,Angled,2x4,Slotted,Very High,80,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-V-8-120-C3,Flat,2x4,Slotted,Very High,80,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-V-8-277-C3,Angled,2x4,Diffuse,Very High,80,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-V-8-277-C3,Flat,2x4,Diffuse,Very High,80,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-V-8-277-C3,Angled,2x4,Slotted,Very High,80,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-V-8-277-C3,Flat,2x4,Slotted,Very High,80,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-V-8-120-DW,Angled,2x4,Diffuse,Very High,80,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-V-8-120-DW,Flat,2x4,Diffuse,Very High,80,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-V-8-120-DW,Angled,2x4,Slotted,Very High,80,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-V-8-120-DW,Flat,2x4,Slotted,Very High,80,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-V-8-277-DW,Angled,2x4,Diffuse,Very High,80,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-V-8-277-DW,Flat,2x4,Diffuse,Very High,80,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-V-8-277-DW,Angled,2x4,Slotted,Very High,80,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-V-8-277-DW,Flat,2x4,Slotted,Very High,80,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-V-8-120-C1,Angled Narrow Rail,2x4,Diffuse,Very High,80,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-120-C1,Angled Narrow Rail,2x4,Slotted,Very High,80,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-277-C1,Angled Narrow Rail,2x4,Diffuse,Very High,80,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-277-C1,Angled Narrow Rail,2x4,Slotted,Very High,80,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-120-C2,Angled Narrow Rail,2x4,Diffuse,Very High,80,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-120-C2,Angled Narrow Rail,2x4,Slotted,Very High,80,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-277-C2,Angled Narrow Rail,2x4,Diffuse,Very High,80,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-277-C2,Angled Narrow Rail,2x4,Slotted,Very High,80,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-120-C3,Angled Narrow Rail,2x4,Diffuse,Very High,80,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-V-8-120-C3,Angled Narrow Rail,2x4,Slotted,Very High,80,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-V-8-277-C3,Angled Narrow Rail,2x4,Diffuse,Very High,80,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-V-8-277-C3,Angled Narrow Rail,2x4,Slotted,Very High,80,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-V-8-120-DW,Angled Narrow Rail,2x4,Diffuse,Very High,80,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-V-8-120-DW,Angled Narrow Rail,2x4,Slotted,Very High,80,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-V-8-277-DW,Angled Narrow Rail,2x4,Diffuse,Very High,80,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-V-8-277-DW,Angled Narrow Rail,2x4,Slotted,Very High,80,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-V-8-120-C1,Angled,2x4,Round,Very High,80,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-120-C1,Flat,2x4,Round,Very High,80,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-277-C1,Angled,2x4,Round,Very High,80,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-277-C1,Flat,2x4,Round,Very High,80,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-120-C2,Angled,2x4,Round,Very High,80,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-120-C2,Flat,2x4,Round,Very High,80,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-277-C2,Angled,2x4,Round,Very High,80,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-277-C2,Flat,2x4,Round,Very High,80,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-120-C3,Angled,2x4,Round,Very High,80,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-V-8-120-C3,Flat,2x4,Round,Very High,80,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-V-8-277-C3,Angled,2x4,Round,Very High,80,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-V-8-277-C3,Flat,2x4,Round,Very High,80,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-V-8-120-DW,Angled,2x4,Round,Very High,80,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-V-8-120-DW,Flat,2x4,Round,Very High,80,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-V-8-277-DW,Angled,2x4,Round,Very High,80,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-V-8-277-DW,Flat,2x4,Round,Very High,80,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-V-8-120-C1,Angled Narrow Rail,2x4,Round,Very High,80,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-277-C1,Angled Narrow Rail,2x4,Round,Very High,80,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-120-C2,Angled Narrow Rail,2x4,Round,Very High,80,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-277-C2,Angled Narrow Rail,2x4,Round,Very High,80,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-120-C3,Angled Narrow Rail,2x4,Round,Very High,80,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-V-8-277-C3,Angled Narrow Rail,2x4,Round,Very High,80,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-V-8-120-DW,Angled Narrow Rail,2x4,Round,Very High,80,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-V-8-277-DW,Angled Narrow Rail,2x4,Round,Very High,80,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-V-8-120-C1,Angled,2x4,Diffuse,Very High,80,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-120-C1,Flat,2x4,Diffuse,Very High,80,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-120-C1,Angled,2x4,Slotted,Very High,80,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-120-C1,Flat,2x4,Slotted,Very High,80,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-277-C1,Angled,2x4,Diffuse,Very High,80,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-277-C1,Flat,2x4,Diffuse,Very High,80,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-277-C1,Angled,2x4,Slotted,Very High,80,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-277-C1,Flat,2x4,Slotted,Very High,80,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-120-C2,Angled,2x4,Diffuse,Very High,80,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-120-C2,Flat,2x4,Diffuse,Very High,80,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-120-C2,Angled,2x4,Slotted,Very High,80,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-120-C2,Flat,2x4,Slotted,Very High,80,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-277-C2,Angled,2x4,Diffuse,Very High,80,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-277-C2,Flat,2x4,Diffuse,Very High,80,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-277-C2,Angled,2x4,Slotted,Very High,80,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-277-C2,Flat,2x4,Slotted,Very High,80,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-120-C3,Angled,2x4,Diffuse,Very High,80,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-V-8-120-C3,Flat,2x4,Diffuse,Very High,80,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-V-8-120-C3,Angled,2x4,Slotted,Very High,80,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-V-8-120-C3,Flat,2x4,Slotted,Very High,80,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-V-8-277-C3,Angled,2x4,Diffuse,Very High,80,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-V-8-277-C3,Flat,2x4,Diffuse,Very High,80,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-V-8-277-C3,Angled,2x4,Slotted,Very High,80,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-V-8-277-C3,Flat,2x4,Slotted,Very High,80,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-V-8-120-DW,Angled,2x4,Diffuse,Very High,80,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-V-8-120-DW,Flat,2x4,Diffuse,Very High,80,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-V-8-120-DW,Angled,2x4,Slotted,Very High,80,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-V-8-120-DW,Flat,2x4,Slotted,Very High,80,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-V-8-277-DW,Angled,2x4,Diffuse,Very High,80,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-V-8-277-DW,Flat,2x4,Diffuse,Very High,80,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-V-8-277-DW,Angled,2x4,Slotted,Very High,80,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-V-8-277-DW,Flat,2x4,Slotted,Very High,80,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-V-8-120-C1,Angled Narrow Rail,2x4,Diffuse,Very High,80,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-120-C1,Angled Narrow Rail,2x4,Slotted,Very High,80,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-277-C1,Angled Narrow Rail,2x4,Diffuse,Very High,80,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-277-C1,Angled Narrow Rail,2x4,Slotted,Very High,80,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-120-C2,Angled Narrow Rail,2x4,Diffuse,Very High,80,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-120-C2,Angled Narrow Rail,2x4,Slotted,Very High,80,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-277-C2,Angled Narrow Rail,2x4,Diffuse,Very High,80,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-277-C2,Angled Narrow Rail,2x4,Slotted,Very High,80,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-120-C3,Angled Narrow Rail,2x4,Diffuse,Very High,80,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-V-8-120-C3,Angled Narrow Rail,2x4,Slotted,Very High,80,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-V-8-277-C3,Angled Narrow Rail,2x4,Diffuse,Very High,80,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-V-8-277-C3,Angled Narrow Rail,2x4,Slotted,Very High,80,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-V-8-120-DW,Angled Narrow Rail,2x4,Diffuse,Very High,80,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-V-8-120-DW,Angled Narrow Rail,2x4,Slotted,Very High,80,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-V-8-277-DW,Angled Narrow Rail,2x4,Diffuse,Very High,80,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-V-8-277-DW,Angled Narrow Rail,2x4,Slotted,Very High,80,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-V-8-120-C1,Angled,2x4,Round,Very High,80,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-120-C1,Flat,2x4,Round,Very High,80,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-277-C1,Angled,2x4,Round,Very High,80,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-277-C1,Flat,2x4,Round,Very High,80,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-120-C2,Angled,2x4,Round,Very High,80,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-120-C2,Flat,2x4,Round,Very High,80,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-277-C2,Angled,2x4,Round,Very High,80,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-277-C2,Flat,2x4,Round,Very High,80,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-120-C3,Angled,2x4,Round,Very High,80,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-V-8-120-C3,Flat,2x4,Round,Very High,80,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-V-8-277-C3,Angled,2x4,Round,Very High,80,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-V-8-277-C3,Flat,2x4,Round,Very High,80,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-V-8-120-DW,Angled,2x4,Round,Very High,80,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-V-8-120-DW,Flat,2x4,Round,Very High,80,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-V-8-277-DW,Angled,2x4,Round,Very High,80,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-V-8-277-DW,Flat,2x4,Round,Very High,80,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-V-8-120-C1,Angled Narrow Rail,2x4,Round,Very High,80,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-277-C1,Angled Narrow Rail,2x4,Round,Very High,80,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-120-C2,Angled Narrow Rail,2x4,Round,Very High,80,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-277-C2,Angled Narrow Rail,2x4,Round,Very High,80,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-120-C3,Angled Narrow Rail,2x4,Round,Very High,80,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-V-8-277-C3,Angled Narrow Rail,2x4,Round,Very High,80,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-V-8-120-DW,Angled Narrow Rail,2x4,Round,Very High,80,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-V-8-277-DW,Angled Narrow Rail,2x4,Round,Very High,80,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-V-8-120-C2,Angled,2x4,Diffuse,Very High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-120-C2,Flat,2x4,Diffuse,Very High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-120-C2,Angled,2x4,Slotted,Very High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-120-C2,Flat,2x4,Slotted,Very High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-277-C2,Angled,2x4,Diffuse,Very High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-277-C2,Flat,2x4,Diffuse,Very High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-277-C2,Angled,2x4,Slotted,Very High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-277-C2,Flat,2x4,Slotted,Very High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-120-C2,Angled Narrow Rail,2x4,Diffuse,Very High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-120-C2,Angled Narrow Rail,2x4,Slotted,Very High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-277-C2,Angled Narrow Rail,2x4,Diffuse,Very High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-277-C2,Angled Narrow Rail,2x4,Slotted,Very High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-120-C2,Angled,2x4,Round,Very High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-120-C2,Flat,2x4,Round,Very High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-277-C2,Angled,2x4,Round,Very High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-277-C2,Flat,2x4,Round,Very High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-120-C2,Angled Narrow Rail,2x4,Round,Very High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-277-C2,Angled Narrow Rail,2x4,Round,Very High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-120-C2,Angled,2x4,Diffuse,Very High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-120-C2,Flat,2x4,Diffuse,Very High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-120-C2,Angled,2x4,Slotted,Very High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-120-C2,Flat,2x4,Slotted,Very High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-277-C2,Angled,2x4,Diffuse,Very High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-277-C2,Flat,2x4,Diffuse,Very High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-277-C2,Angled,2x4,Slotted,Very High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-277-C2,Flat,2x4,Slotted,Very High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-120-C2,Angled Narrow Rail,2x4,Diffuse,Very High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-120-C2,Angled Narrow Rail,2x4,Slotted,Very High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-277-C2,Angled Narrow Rail,2x4,Diffuse,Very High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-277-C2,Angled Narrow Rail,2x4,Slotted,Very High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-120-C2,Angled,2x4,Round,Very High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-120-C2,Flat,2x4,Round,Very High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-277-C2,Angled,2x4,Round,Very High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-277-C2,Flat,2x4,Round,Very High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-120-C2,Angled Narrow Rail,2x4,Round,Very High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-277-C2,Angled Narrow Rail,2x4,Round,Very High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-120-C2,Angled,2x4,Diffuse,Very High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-120-C2,Flat,2x4,Diffuse,Very High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-120-C2,Angled,2x4,Slotted,Very High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-120-C2,Flat,2x4,Slotted,Very High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-V-8-277-C2,Angled,2x4,Diffuse,Very High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-V-8-277-C2,Flat,2x4,Diffuse,Very High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-V-8-277-C2,Angled,2x4,Slotted,Very High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-V-8-277-C2,Flat,2x4,Slotted,Very High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-120-C2,Angled Narrow Rail,2x4,Diffuse,Very High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-120-C2,Angled Narrow Rail,2x4,Slotted,Very High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-8-277-C2,Angled Narrow Rail,2x4,Diffuse,Very High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-8-277-C2,Angled Narrow Rail,2x4,Slotted,Very High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-120-C2,Angled,2x4,Round,Very High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-120-C2,Flat,2x4,Round,Very High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-V-8-277-C2,Angled,2x4,Round,Very High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-V-8-277-C2,Flat,2x4,Round,Very High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-120-C2,Angled Narrow Rail,2x4,Round,Very High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-8-277-C2,Angled Narrow Rail,2x4,Round,Very High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-120-C1,Wave,2x4,Diffuse,Very High,80,3500K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-277-C1,Wave,2x4,Diffuse,Very High,80,3500K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-120-C2,Wave,2x4,Diffuse,Very High,80,3500K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-277-C2,Wave,2x4,Diffuse,Very High,80,3500K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-120-C3,Wave,2x4,Diffuse,Very High,80,3500K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-V-8-277-C3,Wave,2x4,Diffuse,Very High,80,3500K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-V-8-120-DW,Wave,2x4,Diffuse,Very High,80,3500K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-V-8-277-DW,Wave,2x4,Diffuse,Very High,80,3500K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-V-8-120-C1,Wave,2x4,Diffuse,Very High,80,3000K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-277-C1,Wave,2x4,Diffuse,Very High,80,3000K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-120-C2,Wave,2x4,Diffuse,Very High,80,3000K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-277-C2,Wave,2x4,Diffuse,Very High,80,3000K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-120-C3,Wave,2x4,Diffuse,Very High,80,3000K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-V-8-277-C3,Wave,2x4,Diffuse,Very High,80,3000K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-V-8-120-DW,Wave,2x4,Diffuse,Very High,80,3000K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-V-8-277-DW,Wave,2x4,Diffuse,Very High,80,3000K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-V-8-120-C1,Wave,2x4,Diffuse,Very High,80,4000K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-277-C1,Wave,2x4,Diffuse,Very High,80,4000K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-120-C2,Wave,2x4,Diffuse,Very High,80,4000K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-277-C2,Wave,2x4,Diffuse,Very High,80,4000K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-120-C3,Wave,2x4,Diffuse,Very High,80,4000K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-V-8-277-C3,Wave,2x4,Diffuse,Very High,80,4000K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-V-8-120-DW,Wave,2x4,Diffuse,Very High,80,4000K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-V-8-277-DW,Wave,2x4,Diffuse,Very High,80,4000K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-V-8-120-C2,Wave,2x4,Diffuse,Very High,80,3500K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-277-C2,Wave,2x4,Diffuse,Very High,80,3500K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-120-C2,Wave,2x4,Diffuse,Very High,80,3000K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-277-C2,Wave,2x4,Diffuse,Very High,80,3000K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-120-C2,Wave,2x4,Diffuse,Very High,80,4000K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-8-277-C2,Wave,2x4,Diffuse,Very High,80,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-120-C1,Angled,2x4,Diffuse,Standard,90,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-120-C1,Flat,2x4,Diffuse,Standard,90,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-120-C1,Angled,2x4,Slotted,Standard,90,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-120-C1,Flat,2x4,Slotted,Standard,90,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-277-C1,Angled,2x4,Diffuse,Standard,90,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-277-C1,Flat,2x4,Diffuse,Standard,90,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-277-C1,Angled,2x4,Slotted,Standard,90,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-277-C1,Flat,2x4,Slotted,Standard,90,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-120-C2,Angled,2x4,Diffuse,Standard,90,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-120-C2,Flat,2x4,Diffuse,Standard,90,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-120-C2,Angled,2x4,Slotted,Standard,90,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-120-C2,Flat,2x4,Slotted,Standard,90,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-277-C2,Angled,2x4,Diffuse,Standard,90,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-277-C2,Flat,2x4,Diffuse,Standard,90,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-277-C2,Angled,2x4,Slotted,Standard,90,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-277-C2,Flat,2x4,Slotted,Standard,90,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-120-C3,Angled,2x4,Diffuse,Standard,90,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-S -9-120-C3,Flat,2x4,Diffuse,Standard,90,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-S -9-120-C3,Angled,2x4,Slotted,Standard,90,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-S -9-120-C3,Flat,2x4,Slotted,Standard,90,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-S -9-277-C3,Angled,2x4,Diffuse,Standard,90,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-S -9-277-C3,Flat,2x4,Diffuse,Standard,90,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-S -9-277-C3,Angled,2x4,Slotted,Standard,90,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-S -9-277-C3,Flat,2x4,Slotted,Standard,90,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-S -9-120-DW,Angled,2x4,Diffuse,Standard,90,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-S -9-120-DW,Flat,2x4,Diffuse,Standard,90,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-S -9-120-DW,Angled,2x4,Slotted,Standard,90,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-S -9-120-DW,Flat,2x4,Slotted,Standard,90,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-S -9-277-DW,Angled,2x4,Diffuse,Standard,90,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-S -9-277-DW,Flat,2x4,Diffuse,Standard,90,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-S -9-277-DW,Angled,2x4,Slotted,Standard,90,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-S -9-277-DW,Flat,2x4,Slotted,Standard,90,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-S -9-120-C1,Angled Narrow Rail,2x4,Diffuse,Standard,90,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-120-C1,Angled Narrow Rail,2x4,Slotted,Standard,90,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-277-C1,Angled Narrow Rail,2x4,Diffuse,Standard,90,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-277-C1,Angled Narrow Rail,2x4,Slotted,Standard,90,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-120-C2,Angled Narrow Rail,2x4,Diffuse,Standard,90,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-120-C2,Angled Narrow Rail,2x4,Slotted,Standard,90,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-277-C2,Angled Narrow Rail,2x4,Diffuse,Standard,90,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-277-C2,Angled Narrow Rail,2x4,Slotted,Standard,90,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-120-C3,Angled Narrow Rail,2x4,Diffuse,Standard,90,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-S -9-120-C3,Angled Narrow Rail,2x4,Slotted,Standard,90,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-S -9-277-C3,Angled Narrow Rail,2x4,Diffuse,Standard,90,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-S -9-277-C3,Angled Narrow Rail,2x4,Slotted,Standard,90,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-S -9-120-DW,Angled Narrow Rail,2x4,Diffuse,Standard,90,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-S -9-120-DW,Angled Narrow Rail,2x4,Slotted,Standard,90,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-S -9-277-DW,Angled Narrow Rail,2x4,Diffuse,Standard,90,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-S -9-277-DW,Angled Narrow Rail,2x4,Slotted,Standard,90,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-S -9-120-C1,Angled,2x4,Round,Standard,90,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-120-C1,Flat,2x4,Round,Standard,90,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-277-C1,Angled,2x4,Round,Standard,90,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-277-C1,Flat,2x4,Round,Standard,90,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-120-C2,Angled,2x4,Round,Standard,90,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-120-C2,Flat,2x4,Round,Standard,90,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-277-C2,Angled,2x4,Round,Standard,90,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-277-C2,Flat,2x4,Round,Standard,90,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-120-C3,Angled,2x4,Round,Standard,90,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-S -9-120-C3,Flat,2x4,Round,Standard,90,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-S -9-277-C3,Angled,2x4,Round,Standard,90,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-S -9-277-C3,Flat,2x4,Round,Standard,90,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-S -9-120-DW,Angled,2x4,Round,Standard,90,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-S -9-120-DW,Flat,2x4,Round,Standard,90,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-S -9-277-DW,Angled,2x4,Round,Standard,90,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-S -9-277-DW,Flat,2x4,Round,Standard,90,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-S -9-120-C1,Angled Narrow Rail,2x4,Round,Standard,90,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-277-C1,Angled Narrow Rail,2x4,Round,Standard,90,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-120-C2,Angled Narrow Rail,2x4,Round,Standard,90,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-277-C2,Angled Narrow Rail,2x4,Round,Standard,90,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-120-C3,Angled Narrow Rail,2x4,Round,Standard,90,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-S -9-277-C3,Angled Narrow Rail,2x4,Round,Standard,90,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-S -9-120-DW,Angled Narrow Rail,2x4,Round,Standard,90,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-S -9-277-DW,Angled Narrow Rail,2x4,Round,Standard,90,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-S -9-120-C1,Angled,2x4,Diffuse,Standard,90,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-120-C1,Flat,2x4,Diffuse,Standard,90,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-120-C1,Angled,2x4,Slotted,Standard,90,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-120-C1,Flat,2x4,Slotted,Standard,90,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-277-C1,Angled,2x4,Diffuse,Standard,90,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-277-C1,Flat,2x4,Diffuse,Standard,90,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-277-C1,Angled,2x4,Slotted,Standard,90,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-277-C1,Flat,2x4,Slotted,Standard,90,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-120-C2,Angled,2x4,Diffuse,Standard,90,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-120-C2,Flat,2x4,Diffuse,Standard,90,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-120-C2,Angled,2x4,Slotted,Standard,90,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-120-C2,Flat,2x4,Slotted,Standard,90,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-277-C2,Angled,2x4,Diffuse,Standard,90,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-277-C2,Flat,2x4,Diffuse,Standard,90,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-277-C2,Angled,2x4,Slotted,Standard,90,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-277-C2,Flat,2x4,Slotted,Standard,90,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-120-C3,Angled,2x4,Diffuse,Standard,90,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-S -9-120-C3,Flat,2x4,Diffuse,Standard,90,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-S -9-120-C3,Angled,2x4,Slotted,Standard,90,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-S -9-120-C3,Flat,2x4,Slotted,Standard,90,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-S -9-277-C3,Angled,2x4,Diffuse,Standard,90,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-S -9-277-C3,Flat,2x4,Diffuse,Standard,90,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-S -9-277-C3,Angled,2x4,Slotted,Standard,90,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-S -9-277-C3,Flat,2x4,Slotted,Standard,90,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-S -9-120-DW,Angled,2x4,Diffuse,Standard,90,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-S -9-120-DW,Flat,2x4,Diffuse,Standard,90,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-S -9-120-DW,Angled,2x4,Slotted,Standard,90,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-S -9-120-DW,Flat,2x4,Slotted,Standard,90,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-S -9-277-DW,Angled,2x4,Diffuse,Standard,90,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-S -9-277-DW,Flat,2x4,Diffuse,Standard,90,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-S -9-277-DW,Angled,2x4,Slotted,Standard,90,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-S -9-277-DW,Flat,2x4,Slotted,Standard,90,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-S -9-120-C1,Angled Narrow Rail,2x4,Diffuse,Standard,90,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-120-C1,Angled Narrow Rail,2x4,Slotted,Standard,90,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-277-C1,Angled Narrow Rail,2x4,Diffuse,Standard,90,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-277-C1,Angled Narrow Rail,2x4,Slotted,Standard,90,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-120-C2,Angled Narrow Rail,2x4,Diffuse,Standard,90,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-120-C2,Angled Narrow Rail,2x4,Slotted,Standard,90,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-277-C2,Angled Narrow Rail,2x4,Diffuse,Standard,90,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-277-C2,Angled Narrow Rail,2x4,Slotted,Standard,90,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-120-C3,Angled Narrow Rail,2x4,Diffuse,Standard,90,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-S -9-120-C3,Angled Narrow Rail,2x4,Slotted,Standard,90,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-S -9-277-C3,Angled Narrow Rail,2x4,Diffuse,Standard,90,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-S -9-277-C3,Angled Narrow Rail,2x4,Slotted,Standard,90,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-S -9-120-DW,Angled Narrow Rail,2x4,Diffuse,Standard,90,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-S -9-120-DW,Angled Narrow Rail,2x4,Slotted,Standard,90,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-S -9-277-DW,Angled Narrow Rail,2x4,Diffuse,Standard,90,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-S -9-277-DW,Angled Narrow Rail,2x4,Slotted,Standard,90,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-S -9-120-C1,Angled,2x4,Round,Standard,90,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-120-C1,Flat,2x4,Round,Standard,90,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-277-C1,Angled,2x4,Round,Standard,90,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-277-C1,Flat,2x4,Round,Standard,90,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-120-C2,Angled,2x4,Round,Standard,90,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-120-C2,Flat,2x4,Round,Standard,90,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-277-C2,Angled,2x4,Round,Standard,90,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-277-C2,Flat,2x4,Round,Standard,90,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-120-C3,Angled,2x4,Round,Standard,90,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-S -9-120-C3,Flat,2x4,Round,Standard,90,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-S -9-277-C3,Angled,2x4,Round,Standard,90,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-S -9-277-C3,Flat,2x4,Round,Standard,90,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-S -9-120-DW,Angled,2x4,Round,Standard,90,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-S -9-120-DW,Flat,2x4,Round,Standard,90,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-S -9-277-DW,Angled,2x4,Round,Standard,90,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-S -9-277-DW,Flat,2x4,Round,Standard,90,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-S -9-120-C1,Angled Narrow Rail,2x4,Round,Standard,90,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-277-C1,Angled Narrow Rail,2x4,Round,Standard,90,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-120-C2,Angled Narrow Rail,2x4,Round,Standard,90,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-277-C2,Angled Narrow Rail,2x4,Round,Standard,90,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-120-C3,Angled Narrow Rail,2x4,Round,Standard,90,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-S -9-277-C3,Angled Narrow Rail,2x4,Round,Standard,90,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-S -9-120-DW,Angled Narrow Rail,2x4,Round,Standard,90,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-S -9-277-DW,Angled Narrow Rail,2x4,Round,Standard,90,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-S -9-120-C1,Angled,2x4,Diffuse,Standard,90,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-120-C1,Flat,2x4,Diffuse,Standard,90,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-120-C1,Angled,2x4,Slotted,Standard,90,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-120-C1,Flat,2x4,Slotted,Standard,90,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-277-C1,Angled,2x4,Diffuse,Standard,90,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-277-C1,Flat,2x4,Diffuse,Standard,90,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-277-C1,Angled,2x4,Slotted,Standard,90,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-277-C1,Flat,2x4,Slotted,Standard,90,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-120-C2,Angled,2x4,Diffuse,Standard,90,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-120-C2,Flat,2x4,Diffuse,Standard,90,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-120-C2,Angled,2x4,Slotted,Standard,90,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-120-C2,Flat,2x4,Slotted,Standard,90,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-277-C2,Angled,2x4,Diffuse,Standard,90,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-277-C2,Flat,2x4,Diffuse,Standard,90,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-277-C2,Angled,2x4,Slotted,Standard,90,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-277-C2,Flat,2x4,Slotted,Standard,90,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-120-C3,Angled,2x4,Diffuse,Standard,90,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-S -9-120-C3,Flat,2x4,Diffuse,Standard,90,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-S -9-120-C3,Angled,2x4,Slotted,Standard,90,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-S -9-120-C3,Flat,2x4,Slotted,Standard,90,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-S -9-277-C3,Angled,2x4,Diffuse,Standard,90,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-S -9-277-C3,Flat,2x4,Diffuse,Standard,90,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-S -9-277-C3,Angled,2x4,Slotted,Standard,90,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-S -9-277-C3,Flat,2x4,Slotted,Standard,90,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-S -9-120-DW,Angled,2x4,Diffuse,Standard,90,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-S -9-120-DW,Flat,2x4,Diffuse,Standard,90,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-S -9-120-DW,Angled,2x4,Slotted,Standard,90,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-S -9-120-DW,Flat,2x4,Slotted,Standard,90,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-S -9-277-DW,Angled,2x4,Diffuse,Standard,90,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-S -9-277-DW,Flat,2x4,Diffuse,Standard,90,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-S -9-277-DW,Angled,2x4,Slotted,Standard,90,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-S -9-277-DW,Flat,2x4,Slotted,Standard,90,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-S -9-120-C1,Angled Narrow Rail,2x4,Diffuse,Standard,90,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-120-C1,Angled Narrow Rail,2x4,Slotted,Standard,90,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-277-C1,Angled Narrow Rail,2x4,Diffuse,Standard,90,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-277-C1,Angled Narrow Rail,2x4,Slotted,Standard,90,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-120-C2,Angled Narrow Rail,2x4,Diffuse,Standard,90,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-120-C2,Angled Narrow Rail,2x4,Slotted,Standard,90,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-277-C2,Angled Narrow Rail,2x4,Diffuse,Standard,90,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-277-C2,Angled Narrow Rail,2x4,Slotted,Standard,90,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-120-C3,Angled Narrow Rail,2x4,Diffuse,Standard,90,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-S -9-120-C3,Angled Narrow Rail,2x4,Slotted,Standard,90,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-S -9-277-C3,Angled Narrow Rail,2x4,Diffuse,Standard,90,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-S -9-277-C3,Angled Narrow Rail,2x4,Slotted,Standard,90,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-S -9-120-DW,Angled Narrow Rail,2x4,Diffuse,Standard,90,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-S -9-120-DW,Angled Narrow Rail,2x4,Slotted,Standard,90,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-S -9-277-DW,Angled Narrow Rail,2x4,Diffuse,Standard,90,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-S -9-277-DW,Angled Narrow Rail,2x4,Slotted,Standard,90,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-S -9-120-C1,Angled,2x4,Round,Standard,90,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-120-C1,Flat,2x4,Round,Standard,90,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-277-C1,Angled,2x4,Round,Standard,90,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-277-C1,Flat,2x4,Round,Standard,90,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-120-C2,Angled,2x4,Round,Standard,90,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-120-C2,Flat,2x4,Round,Standard,90,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-277-C2,Angled,2x4,Round,Standard,90,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-277-C2,Flat,2x4,Round,Standard,90,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-120-C3,Angled,2x4,Round,Standard,90,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-S -9-120-C3,Flat,2x4,Round,Standard,90,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-S -9-277-C3,Angled,2x4,Round,Standard,90,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-S -9-277-C3,Flat,2x4,Round,Standard,90,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-S -9-120-DW,Angled,2x4,Round,Standard,90,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-S -9-120-DW,Flat,2x4,Round,Standard,90,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-S -9-277-DW,Angled,2x4,Round,Standard,90,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-S -9-277-DW,Flat,2x4,Round,Standard,90,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-S -9-120-C1,Angled Narrow Rail,2x4,Round,Standard,90,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-277-C1,Angled Narrow Rail,2x4,Round,Standard,90,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-120-C2,Angled Narrow Rail,2x4,Round,Standard,90,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-277-C2,Angled Narrow Rail,2x4,Round,Standard,90,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-120-C3,Angled Narrow Rail,2x4,Round,Standard,90,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-S -9-277-C3,Angled Narrow Rail,2x4,Round,Standard,90,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-S -9-120-DW,Angled Narrow Rail,2x4,Round,Standard,90,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-S -9-277-DW,Angled Narrow Rail,2x4,Round,Standard,90,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-S -9-120-C2,Angled,2x4,Diffuse,Standard,90,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-120-C2,Flat,2x4,Diffuse,Standard,90,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-120-C2,Angled,2x4,Slotted,Standard,90,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-120-C2,Flat,2x4,Slotted,Standard,90,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-277-C2,Angled,2x4,Diffuse,Standard,90,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-277-C2,Flat,2x4,Diffuse,Standard,90,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-277-C2,Angled,2x4,Slotted,Standard,90,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-277-C2,Flat,2x4,Slotted,Standard,90,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-120-C2,Angled Narrow Rail,2x4,Diffuse,Standard,90,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-120-C2,Angled Narrow Rail,2x4,Slotted,Standard,90,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-277-C2,Angled Narrow Rail,2x4,Diffuse,Standard,90,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-277-C2,Angled Narrow Rail,2x4,Slotted,Standard,90,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-120-C2,Angled,2x4,Round,Standard,90,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-120-C2,Flat,2x4,Round,Standard,90,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-277-C2,Angled,2x4,Round,Standard,90,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-277-C2,Flat,2x4,Round,Standard,90,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-120-C2,Angled Narrow Rail,2x4,Round,Standard,90,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-277-C2,Angled Narrow Rail,2x4,Round,Standard,90,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-120-C2,Angled,2x4,Diffuse,Standard,90,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-120-C2,Flat,2x4,Diffuse,Standard,90,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-120-C2,Angled,2x4,Slotted,Standard,90,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-120-C2,Flat,2x4,Slotted,Standard,90,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-277-C2,Angled,2x4,Diffuse,Standard,90,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-277-C2,Flat,2x4,Diffuse,Standard,90,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-277-C2,Angled,2x4,Slotted,Standard,90,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-277-C2,Flat,2x4,Slotted,Standard,90,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-120-C2,Angled Narrow Rail,2x4,Diffuse,Standard,90,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-120-C2,Angled Narrow Rail,2x4,Slotted,Standard,90,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-277-C2,Angled Narrow Rail,2x4,Diffuse,Standard,90,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-277-C2,Angled Narrow Rail,2x4,Slotted,Standard,90,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-120-C2,Angled,2x4,Round,Standard,90,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-120-C2,Flat,2x4,Round,Standard,90,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-277-C2,Angled,2x4,Round,Standard,90,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-277-C2,Flat,2x4,Round,Standard,90,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-120-C2,Angled Narrow Rail,2x4,Round,Standard,90,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-277-C2,Angled Narrow Rail,2x4,Round,Standard,90,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-120-C2,Angled,2x4,Diffuse,Standard,90,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-120-C2,Flat,2x4,Diffuse,Standard,90,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-120-C2,Angled,2x4,Slotted,Standard,90,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-120-C2,Flat,2x4,Slotted,Standard,90,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-S -9-277-C2,Angled,2x4,Diffuse,Standard,90,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-S -9-277-C2,Flat,2x4,Diffuse,Standard,90,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-S -9-277-C2,Angled,2x4,Slotted,Standard,90,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-S -9-277-C2,Flat,2x4,Slotted,Standard,90,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-120-C2,Angled Narrow Rail,2x4,Diffuse,Standard,90,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-120-C2,Angled Narrow Rail,2x4,Slotted,Standard,90,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-S -9-277-C2,Angled Narrow Rail,2x4,Diffuse,Standard,90,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-S -9-277-C2,Angled Narrow Rail,2x4,Slotted,Standard,90,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-120-C2,Angled,2x4,Round,Standard,90,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-120-C2,Flat,2x4,Round,Standard,90,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-S -9-277-C2,Angled,2x4,Round,Standard,90,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-S -9-277-C2,Flat,2x4,Round,Standard,90,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-120-C2,Angled Narrow Rail,2x4,Round,Standard,90,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-S -9-277-C2,Angled Narrow Rail,2x4,Round,Standard,90,4000K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-120-C1,Wave,2x4,Diffuse,Standard,90,3500K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-277-C1,Wave,2x4,Diffuse,Standard,90,3500K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-120-C2,Wave,2x4,Diffuse,Standard,90,3500K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-277-C2,Wave,2x4,Diffuse,Standard,90,3500K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-120-C3,Wave,2x4,Diffuse,Standard,90,3500K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-S -9-277-C3,Wave,2x4,Diffuse,Standard,90,3500K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-S -9-120-DW,Wave,2x4,Diffuse,Standard,90,3500K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-S -9-277-DW,Wave,2x4,Diffuse,Standard,90,3500K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-S -9-120-C1,Wave,2x4,Diffuse,Standard,90,3000K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-277-C1,Wave,2x4,Diffuse,Standard,90,3000K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-120-C2,Wave,2x4,Diffuse,Standard,90,3000K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-277-C2,Wave,2x4,Diffuse,Standard,90,3000K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-120-C3,Wave,2x4,Diffuse,Standard,90,3000K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-S -9-277-C3,Wave,2x4,Diffuse,Standard,90,3000K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-S -9-120-DW,Wave,2x4,Diffuse,Standard,90,3000K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-S -9-277-DW,Wave,2x4,Diffuse,Standard,90,3000K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-S -9-120-C1,Wave,2x4,Diffuse,Standard,90,4000K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-277-C1,Wave,2x4,Diffuse,Standard,90,4000K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-120-C2,Wave,2x4,Diffuse,Standard,90,4000K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-277-C2,Wave,2x4,Diffuse,Standard,90,4000K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-120-C3,Wave,2x4,Diffuse,Standard,90,4000K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-S -9-277-C3,Wave,2x4,Diffuse,Standard,90,4000K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-S -9-120-DW,Wave,2x4,Diffuse,Standard,90,4000K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-S -9-277-DW,Wave,2x4,Diffuse,Standard,90,4000K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-S -9-120-C2,Wave,2x4,Diffuse,Standard,90,3500K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-277-C2,Wave,2x4,Diffuse,Standard,90,3500K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-120-C2,Wave,2x4,Diffuse,Standard,90,3000K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-277-C2,Wave,2x4,Diffuse,Standard,90,3000K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-120-C2,Wave,2x4,Diffuse,Standard,90,4000K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-S -9-277-C2,Wave,2x4,Diffuse,Standard,90,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-120-C1,Angled,2x4,Diffuse,Boosted,90,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-120-C1,Flat,2x4,Diffuse,Boosted,90,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-120-C1,Angled,2x4,Slotted,Boosted,90,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-120-C1,Flat,2x4,Slotted,Boosted,90,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-277-C1,Angled,2x4,Diffuse,Boosted,90,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-277-C1,Flat,2x4,Diffuse,Boosted,90,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-277-C1,Angled,2x4,Slotted,Boosted,90,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-277-C1,Flat,2x4,Slotted,Boosted,90,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-120-C2,Angled,2x4,Diffuse,Boosted,90,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-120-C2,Flat,2x4,Diffuse,Boosted,90,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-120-C2,Angled,2x4,Slotted,Boosted,90,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-120-C2,Flat,2x4,Slotted,Boosted,90,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-277-C2,Angled,2x4,Diffuse,Boosted,90,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-277-C2,Flat,2x4,Diffuse,Boosted,90,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-277-C2,Angled,2x4,Slotted,Boosted,90,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-277-C2,Flat,2x4,Slotted,Boosted,90,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-120-C3,Angled,2x4,Diffuse,Boosted,90,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-B-9-120-C3,Flat,2x4,Diffuse,Boosted,90,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-B-9-120-C3,Angled,2x4,Slotted,Boosted,90,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-B-9-120-C3,Flat,2x4,Slotted,Boosted,90,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-B-9-277-C3,Angled,2x4,Diffuse,Boosted,90,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-B-9-277-C3,Flat,2x4,Diffuse,Boosted,90,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-B-9-277-C3,Angled,2x4,Slotted,Boosted,90,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-B-9-277-C3,Flat,2x4,Slotted,Boosted,90,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-B-9-120-DW,Angled,2x4,Diffuse,Boosted,90,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-B-9-120-DW,Flat,2x4,Diffuse,Boosted,90,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-B-9-120-DW,Angled,2x4,Slotted,Boosted,90,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-B-9-120-DW,Flat,2x4,Slotted,Boosted,90,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-B-9-277-DW,Angled,2x4,Diffuse,Boosted,90,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-B-9-277-DW,Flat,2x4,Diffuse,Boosted,90,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-B-9-277-DW,Angled,2x4,Slotted,Boosted,90,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-B-9-277-DW,Flat,2x4,Slotted,Boosted,90,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-B-9-120-C1,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-120-C1,Angled Narrow Rail,2x4,Slotted,Boosted,90,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-277-C1,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-277-C1,Angled Narrow Rail,2x4,Slotted,Boosted,90,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-120-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-120-C2,Angled Narrow Rail,2x4,Slotted,Boosted,90,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-277-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-277-C2,Angled Narrow Rail,2x4,Slotted,Boosted,90,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-120-C3,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-B-9-120-C3,Angled Narrow Rail,2x4,Slotted,Boosted,90,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-B-9-277-C3,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-B-9-277-C3,Angled Narrow Rail,2x4,Slotted,Boosted,90,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-B-9-120-DW,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-B-9-120-DW,Angled Narrow Rail,2x4,Slotted,Boosted,90,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-B-9-277-DW,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-B-9-277-DW,Angled Narrow Rail,2x4,Slotted,Boosted,90,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-B-9-120-C1,Angled,2x4,Round,Boosted,90,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-120-C1,Flat,2x4,Round,Boosted,90,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-277-C1,Angled,2x4,Round,Boosted,90,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-277-C1,Flat,2x4,Round,Boosted,90,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-120-C2,Angled,2x4,Round,Boosted,90,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-120-C2,Flat,2x4,Round,Boosted,90,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-277-C2,Angled,2x4,Round,Boosted,90,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-277-C2,Flat,2x4,Round,Boosted,90,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-120-C3,Angled,2x4,Round,Boosted,90,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-B-9-120-C3,Flat,2x4,Round,Boosted,90,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-B-9-277-C3,Angled,2x4,Round,Boosted,90,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-B-9-277-C3,Flat,2x4,Round,Boosted,90,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-B-9-120-DW,Angled,2x4,Round,Boosted,90,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-B-9-120-DW,Flat,2x4,Round,Boosted,90,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-B-9-277-DW,Angled,2x4,Round,Boosted,90,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-B-9-277-DW,Flat,2x4,Round,Boosted,90,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-B-9-120-C1,Angled Narrow Rail,2x4,Round,Boosted,90,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-277-C1,Angled Narrow Rail,2x4,Round,Boosted,90,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-120-C2,Angled Narrow Rail,2x4,Round,Boosted,90,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-277-C2,Angled Narrow Rail,2x4,Round,Boosted,90,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-120-C3,Angled Narrow Rail,2x4,Round,Boosted,90,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-B-9-277-C3,Angled Narrow Rail,2x4,Round,Boosted,90,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-B-9-120-DW,Angled Narrow Rail,2x4,Round,Boosted,90,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-B-9-277-DW,Angled Narrow Rail,2x4,Round,Boosted,90,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-B-9-120-C1,Angled,2x4,Diffuse,Boosted,90,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-120-C1,Flat,2x4,Diffuse,Boosted,90,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-120-C1,Angled,2x4,Slotted,Boosted,90,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-120-C1,Flat,2x4,Slotted,Boosted,90,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-277-C1,Angled,2x4,Diffuse,Boosted,90,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-277-C1,Flat,2x4,Diffuse,Boosted,90,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-277-C1,Angled,2x4,Slotted,Boosted,90,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-277-C1,Flat,2x4,Slotted,Boosted,90,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-120-C2,Angled,2x4,Diffuse,Boosted,90,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-120-C2,Flat,2x4,Diffuse,Boosted,90,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-120-C2,Angled,2x4,Slotted,Boosted,90,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-120-C2,Flat,2x4,Slotted,Boosted,90,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-277-C2,Angled,2x4,Diffuse,Boosted,90,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-277-C2,Flat,2x4,Diffuse,Boosted,90,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-277-C2,Angled,2x4,Slotted,Boosted,90,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-277-C2,Flat,2x4,Slotted,Boosted,90,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-120-C3,Angled,2x4,Diffuse,Boosted,90,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-B-9-120-C3,Flat,2x4,Diffuse,Boosted,90,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-B-9-120-C3,Angled,2x4,Slotted,Boosted,90,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-B-9-120-C3,Flat,2x4,Slotted,Boosted,90,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-B-9-277-C3,Angled,2x4,Diffuse,Boosted,90,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-B-9-277-C3,Flat,2x4,Diffuse,Boosted,90,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-B-9-277-C3,Angled,2x4,Slotted,Boosted,90,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-B-9-277-C3,Flat,2x4,Slotted,Boosted,90,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-B-9-120-DW,Angled,2x4,Diffuse,Boosted,90,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-B-9-120-DW,Flat,2x4,Diffuse,Boosted,90,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-B-9-120-DW,Angled,2x4,Slotted,Boosted,90,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-B-9-120-DW,Flat,2x4,Slotted,Boosted,90,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-B-9-277-DW,Angled,2x4,Diffuse,Boosted,90,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-B-9-277-DW,Flat,2x4,Diffuse,Boosted,90,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-B-9-277-DW,Angled,2x4,Slotted,Boosted,90,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-B-9-277-DW,Flat,2x4,Slotted,Boosted,90,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-B-9-120-C1,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-120-C1,Angled Narrow Rail,2x4,Slotted,Boosted,90,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-277-C1,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-277-C1,Angled Narrow Rail,2x4,Slotted,Boosted,90,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-120-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-120-C2,Angled Narrow Rail,2x4,Slotted,Boosted,90,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-277-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-277-C2,Angled Narrow Rail,2x4,Slotted,Boosted,90,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-120-C3,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-B-9-120-C3,Angled Narrow Rail,2x4,Slotted,Boosted,90,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-B-9-277-C3,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-B-9-277-C3,Angled Narrow Rail,2x4,Slotted,Boosted,90,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-B-9-120-DW,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-B-9-120-DW,Angled Narrow Rail,2x4,Slotted,Boosted,90,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-B-9-277-DW,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-B-9-277-DW,Angled Narrow Rail,2x4,Slotted,Boosted,90,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-B-9-120-C1,Angled,2x4,Round,Boosted,90,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-120-C1,Flat,2x4,Round,Boosted,90,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-277-C1,Angled,2x4,Round,Boosted,90,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-277-C1,Flat,2x4,Round,Boosted,90,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-120-C2,Angled,2x4,Round,Boosted,90,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-120-C2,Flat,2x4,Round,Boosted,90,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-277-C2,Angled,2x4,Round,Boosted,90,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-277-C2,Flat,2x4,Round,Boosted,90,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-120-C3,Angled,2x4,Round,Boosted,90,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-B-9-120-C3,Flat,2x4,Round,Boosted,90,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-B-9-277-C3,Angled,2x4,Round,Boosted,90,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-B-9-277-C3,Flat,2x4,Round,Boosted,90,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-B-9-120-DW,Angled,2x4,Round,Boosted,90,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-B-9-120-DW,Flat,2x4,Round,Boosted,90,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-B-9-277-DW,Angled,2x4,Round,Boosted,90,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-B-9-277-DW,Flat,2x4,Round,Boosted,90,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-B-9-120-C1,Angled Narrow Rail,2x4,Round,Boosted,90,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-277-C1,Angled Narrow Rail,2x4,Round,Boosted,90,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-120-C2,Angled Narrow Rail,2x4,Round,Boosted,90,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-277-C2,Angled Narrow Rail,2x4,Round,Boosted,90,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-120-C3,Angled Narrow Rail,2x4,Round,Boosted,90,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-B-9-277-C3,Angled Narrow Rail,2x4,Round,Boosted,90,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-B-9-120-DW,Angled Narrow Rail,2x4,Round,Boosted,90,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-B-9-277-DW,Angled Narrow Rail,2x4,Round,Boosted,90,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-B-9-120-C1,Angled,2x4,Diffuse,Boosted,90,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-120-C1,Flat,2x4,Diffuse,Boosted,90,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-120-C1,Angled,2x4,Slotted,Boosted,90,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-120-C1,Flat,2x4,Slotted,Boosted,90,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-277-C1,Angled,2x4,Diffuse,Boosted,90,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-277-C1,Flat,2x4,Diffuse,Boosted,90,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-277-C1,Angled,2x4,Slotted,Boosted,90,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-277-C1,Flat,2x4,Slotted,Boosted,90,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-120-C2,Angled,2x4,Diffuse,Boosted,90,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-120-C2,Flat,2x4,Diffuse,Boosted,90,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-120-C2,Angled,2x4,Slotted,Boosted,90,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-120-C2,Flat,2x4,Slotted,Boosted,90,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-277-C2,Angled,2x4,Diffuse,Boosted,90,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-277-C2,Flat,2x4,Diffuse,Boosted,90,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-277-C2,Angled,2x4,Slotted,Boosted,90,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-277-C2,Flat,2x4,Slotted,Boosted,90,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-120-C3,Angled,2x4,Diffuse,Boosted,90,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-B-9-120-C3,Flat,2x4,Diffuse,Boosted,90,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-B-9-120-C3,Angled,2x4,Slotted,Boosted,90,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-B-9-120-C3,Flat,2x4,Slotted,Boosted,90,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-B-9-277-C3,Angled,2x4,Diffuse,Boosted,90,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-B-9-277-C3,Flat,2x4,Diffuse,Boosted,90,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-B-9-277-C3,Angled,2x4,Slotted,Boosted,90,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-B-9-277-C3,Flat,2x4,Slotted,Boosted,90,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-B-9-120-DW,Angled,2x4,Diffuse,Boosted,90,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-B-9-120-DW,Flat,2x4,Diffuse,Boosted,90,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-B-9-120-DW,Angled,2x4,Slotted,Boosted,90,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-B-9-120-DW,Flat,2x4,Slotted,Boosted,90,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-B-9-277-DW,Angled,2x4,Diffuse,Boosted,90,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-B-9-277-DW,Flat,2x4,Diffuse,Boosted,90,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-B-9-277-DW,Angled,2x4,Slotted,Boosted,90,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-B-9-277-DW,Flat,2x4,Slotted,Boosted,90,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-B-9-120-C1,Angled Narrow Rail,2x4,Diffuse,Boosted,90,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-120-C1,Angled Narrow Rail,2x4,Slotted,Boosted,90,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-277-C1,Angled Narrow Rail,2x4,Diffuse,Boosted,90,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-277-C1,Angled Narrow Rail,2x4,Slotted,Boosted,90,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-120-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,90,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-120-C2,Angled Narrow Rail,2x4,Slotted,Boosted,90,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-277-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,90,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-277-C2,Angled Narrow Rail,2x4,Slotted,Boosted,90,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-120-C3,Angled Narrow Rail,2x4,Diffuse,Boosted,90,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-B-9-120-C3,Angled Narrow Rail,2x4,Slotted,Boosted,90,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-B-9-277-C3,Angled Narrow Rail,2x4,Diffuse,Boosted,90,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-B-9-277-C3,Angled Narrow Rail,2x4,Slotted,Boosted,90,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-B-9-120-DW,Angled Narrow Rail,2x4,Diffuse,Boosted,90,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-B-9-120-DW,Angled Narrow Rail,2x4,Slotted,Boosted,90,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-B-9-277-DW,Angled Narrow Rail,2x4,Diffuse,Boosted,90,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-B-9-277-DW,Angled Narrow Rail,2x4,Slotted,Boosted,90,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-B-9-120-C1,Angled,2x4,Round,Boosted,90,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-120-C1,Flat,2x4,Round,Boosted,90,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-277-C1,Angled,2x4,Round,Boosted,90,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-277-C1,Flat,2x4,Round,Boosted,90,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-120-C2,Angled,2x4,Round,Boosted,90,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-120-C2,Flat,2x4,Round,Boosted,90,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-277-C2,Angled,2x4,Round,Boosted,90,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-277-C2,Flat,2x4,Round,Boosted,90,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-120-C3,Angled,2x4,Round,Boosted,90,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-B-9-120-C3,Flat,2x4,Round,Boosted,90,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-B-9-277-C3,Angled,2x4,Round,Boosted,90,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-B-9-277-C3,Flat,2x4,Round,Boosted,90,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-B-9-120-DW,Angled,2x4,Round,Boosted,90,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-B-9-120-DW,Flat,2x4,Round,Boosted,90,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-B-9-277-DW,Angled,2x4,Round,Boosted,90,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-B-9-277-DW,Flat,2x4,Round,Boosted,90,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-B-9-120-C1,Angled Narrow Rail,2x4,Round,Boosted,90,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-277-C1,Angled Narrow Rail,2x4,Round,Boosted,90,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-120-C2,Angled Narrow Rail,2x4,Round,Boosted,90,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-277-C2,Angled Narrow Rail,2x4,Round,Boosted,90,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-120-C3,Angled Narrow Rail,2x4,Round,Boosted,90,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-B-9-277-C3,Angled Narrow Rail,2x4,Round,Boosted,90,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-B-9-120-DW,Angled Narrow Rail,2x4,Round,Boosted,90,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-B-9-277-DW,Angled Narrow Rail,2x4,Round,Boosted,90,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-B-9-120-C2,Angled,2x4,Diffuse,Boosted,90,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-120-C2,Flat,2x4,Diffuse,Boosted,90,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-120-C2,Angled,2x4,Slotted,Boosted,90,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-120-C2,Flat,2x4,Slotted,Boosted,90,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-277-C2,Angled,2x4,Diffuse,Boosted,90,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-277-C2,Flat,2x4,Diffuse,Boosted,90,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-277-C2,Angled,2x4,Slotted,Boosted,90,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-277-C2,Flat,2x4,Slotted,Boosted,90,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-120-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-120-C2,Angled Narrow Rail,2x4,Slotted,Boosted,90,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-277-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-277-C2,Angled Narrow Rail,2x4,Slotted,Boosted,90,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-120-C2,Angled,2x4,Round,Boosted,90,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-120-C2,Flat,2x4,Round,Boosted,90,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-277-C2,Angled,2x4,Round,Boosted,90,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-277-C2,Flat,2x4,Round,Boosted,90,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-120-C2,Angled Narrow Rail,2x4,Round,Boosted,90,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-277-C2,Angled Narrow Rail,2x4,Round,Boosted,90,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-120-C2,Angled,2x4,Diffuse,Boosted,90,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-120-C2,Flat,2x4,Diffuse,Boosted,90,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-120-C2,Angled,2x4,Slotted,Boosted,90,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-120-C2,Flat,2x4,Slotted,Boosted,90,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-277-C2,Angled,2x4,Diffuse,Boosted,90,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-277-C2,Flat,2x4,Diffuse,Boosted,90,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-277-C2,Angled,2x4,Slotted,Boosted,90,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-277-C2,Flat,2x4,Slotted,Boosted,90,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-120-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-120-C2,Angled Narrow Rail,2x4,Slotted,Boosted,90,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-277-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,90,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-277-C2,Angled Narrow Rail,2x4,Slotted,Boosted,90,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-120-C2,Angled,2x4,Round,Boosted,90,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-120-C2,Flat,2x4,Round,Boosted,90,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-277-C2,Angled,2x4,Round,Boosted,90,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-277-C2,Flat,2x4,Round,Boosted,90,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-120-C2,Angled Narrow Rail,2x4,Round,Boosted,90,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-277-C2,Angled Narrow Rail,2x4,Round,Boosted,90,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-120-C2,Angled,2x4,Diffuse,Boosted,90,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-120-C2,Flat,2x4,Diffuse,Boosted,90,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-120-C2,Angled,2x4,Slotted,Boosted,90,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-120-C2,Flat,2x4,Slotted,Boosted,90,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-B-9-277-C2,Angled,2x4,Diffuse,Boosted,90,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-B-9-277-C2,Flat,2x4,Diffuse,Boosted,90,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-B-9-277-C2,Angled,2x4,Slotted,Boosted,90,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-B-9-277-C2,Flat,2x4,Slotted,Boosted,90,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-120-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,90,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-120-C2,Angled Narrow Rail,2x4,Slotted,Boosted,90,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-B-9-277-C2,Angled Narrow Rail,2x4,Diffuse,Boosted,90,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-B-9-277-C2,Angled Narrow Rail,2x4,Slotted,Boosted,90,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-120-C2,Angled,2x4,Round,Boosted,90,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-120-C2,Flat,2x4,Round,Boosted,90,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-B-9-277-C2,Angled,2x4,Round,Boosted,90,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-B-9-277-C2,Flat,2x4,Round,Boosted,90,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-120-C2,Angled Narrow Rail,2x4,Round,Boosted,90,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-B-9-277-C2,Angled Narrow Rail,2x4,Round,Boosted,90,4000K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-120-C1,Wave,2x4,Diffuse,Boosted,90,3500K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-277-C1,Wave,2x4,Diffuse,Boosted,90,3500K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-120-C2,Wave,2x4,Diffuse,Boosted,90,3500K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-277-C2,Wave,2x4,Diffuse,Boosted,90,3500K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-120-C3,Wave,2x4,Diffuse,Boosted,90,3500K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-B-9-277-C3,Wave,2x4,Diffuse,Boosted,90,3500K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-B-9-120-DW,Wave,2x4,Diffuse,Boosted,90,3500K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-B-9-277-DW,Wave,2x4,Diffuse,Boosted,90,3500K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-B-9-120-C1,Wave,2x4,Diffuse,Boosted,90,3000K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-277-C1,Wave,2x4,Diffuse,Boosted,90,3000K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-120-C2,Wave,2x4,Diffuse,Boosted,90,3000K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-277-C2,Wave,2x4,Diffuse,Boosted,90,3000K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-120-C3,Wave,2x4,Diffuse,Boosted,90,3000K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-B-9-277-C3,Wave,2x4,Diffuse,Boosted,90,3000K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-B-9-120-DW,Wave,2x4,Diffuse,Boosted,90,3000K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-B-9-277-DW,Wave,2x4,Diffuse,Boosted,90,3000K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-B-9-120-C1,Wave,2x4,Diffuse,Boosted,90,4000K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-277-C1,Wave,2x4,Diffuse,Boosted,90,4000K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-120-C2,Wave,2x4,Diffuse,Boosted,90,4000K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-277-C2,Wave,2x4,Diffuse,Boosted,90,4000K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-120-C3,Wave,2x4,Diffuse,Boosted,90,4000K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-B-9-277-C3,Wave,2x4,Diffuse,Boosted,90,4000K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-B-9-120-DW,Wave,2x4,Diffuse,Boosted,90,4000K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-B-9-277-DW,Wave,2x4,Diffuse,Boosted,90,4000K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-B-9-120-C2,Wave,2x4,Diffuse,Boosted,90,3500K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-277-C2,Wave,2x4,Diffuse,Boosted,90,3500K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-120-C2,Wave,2x4,Diffuse,Boosted,90,3000K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-277-C2,Wave,2x4,Diffuse,Boosted,90,3000K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-120-C2,Wave,2x4,Diffuse,Boosted,90,4000K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-B-9-277-C2,Wave,2x4,Diffuse,Boosted,90,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-120-C1,Angled,2x4,Diffuse,High,90,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-120-C1,Flat,2x4,Diffuse,High,90,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-120-C1,Angled,2x4,Slotted,High,90,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-120-C1,Flat,2x4,Slotted,High,90,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-277-C1,Angled,2x4,Diffuse,High,90,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-277-C1,Flat,2x4,Diffuse,High,90,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-277-C1,Angled,2x4,Slotted,High,90,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-277-C1,Flat,2x4,Slotted,High,90,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-120-C2,Angled,2x4,Diffuse,High,90,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-120-C2,Flat,2x4,Diffuse,High,90,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-120-C2,Angled,2x4,Slotted,High,90,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-120-C2,Flat,2x4,Slotted,High,90,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-277-C2,Angled,2x4,Diffuse,High,90,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-277-C2,Flat,2x4,Diffuse,High,90,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-277-C2,Angled,2x4,Slotted,High,90,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-277-C2,Flat,2x4,Slotted,High,90,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-120-C3,Angled,2x4,Diffuse,High,90,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-H -9-120-C3,Flat,2x4,Diffuse,High,90,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-H -9-120-C3,Angled,2x4,Slotted,High,90,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-H -9-120-C3,Flat,2x4,Slotted,High,90,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-H -9-277-C3,Angled,2x4,Diffuse,High,90,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-H -9-277-C3,Flat,2x4,Diffuse,High,90,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-H -9-277-C3,Angled,2x4,Slotted,High,90,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-H -9-277-C3,Flat,2x4,Slotted,High,90,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-H -9-120-DW,Angled,2x4,Diffuse,High,90,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-H -9-120-DW,Flat,2x4,Diffuse,High,90,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-H -9-120-DW,Angled,2x4,Slotted,High,90,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-H -9-120-DW,Flat,2x4,Slotted,High,90,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-H -9-277-DW,Angled,2x4,Diffuse,High,90,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-H -9-277-DW,Flat,2x4,Diffuse,High,90,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-H -9-277-DW,Angled,2x4,Slotted,High,90,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-H -9-277-DW,Flat,2x4,Slotted,High,90,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-H -9-120-C1,Angled Narrow Rail,2x4,Diffuse,High,90,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-120-C1,Angled Narrow Rail,2x4,Slotted,High,90,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-277-C1,Angled Narrow Rail,2x4,Diffuse,High,90,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-277-C1,Angled Narrow Rail,2x4,Slotted,High,90,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-120-C2,Angled Narrow Rail,2x4,Diffuse,High,90,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-120-C2,Angled Narrow Rail,2x4,Slotted,High,90,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-277-C2,Angled Narrow Rail,2x4,Diffuse,High,90,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-277-C2,Angled Narrow Rail,2x4,Slotted,High,90,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-120-C3,Angled Narrow Rail,2x4,Diffuse,High,90,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-H -9-120-C3,Angled Narrow Rail,2x4,Slotted,High,90,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-H -9-277-C3,Angled Narrow Rail,2x4,Diffuse,High,90,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-H -9-277-C3,Angled Narrow Rail,2x4,Slotted,High,90,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-H -9-120-DW,Angled Narrow Rail,2x4,Diffuse,High,90,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-H -9-120-DW,Angled Narrow Rail,2x4,Slotted,High,90,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-H -9-277-DW,Angled Narrow Rail,2x4,Diffuse,High,90,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-H -9-277-DW,Angled Narrow Rail,2x4,Slotted,High,90,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-H -9-120-C1,Angled,2x4,Round,High,90,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-120-C1,Flat,2x4,Round,High,90,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-277-C1,Angled,2x4,Round,High,90,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-277-C1,Flat,2x4,Round,High,90,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-120-C2,Angled,2x4,Round,High,90,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-120-C2,Flat,2x4,Round,High,90,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-277-C2,Angled,2x4,Round,High,90,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-277-C2,Flat,2x4,Round,High,90,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-120-C3,Angled,2x4,Round,High,90,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-H -9-120-C3,Flat,2x4,Round,High,90,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-H -9-277-C3,Angled,2x4,Round,High,90,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-H -9-277-C3,Flat,2x4,Round,High,90,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-H -9-120-DW,Angled,2x4,Round,High,90,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-H -9-120-DW,Flat,2x4,Round,High,90,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-H -9-277-DW,Angled,2x4,Round,High,90,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-H -9-277-DW,Flat,2x4,Round,High,90,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-H -9-120-C1,Angled Narrow Rail,2x4,Round,High,90,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-277-C1,Angled Narrow Rail,2x4,Round,High,90,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-120-C2,Angled Narrow Rail,2x4,Round,High,90,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-277-C2,Angled Narrow Rail,2x4,Round,High,90,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-120-C3,Angled Narrow Rail,2x4,Round,High,90,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-H -9-277-C3,Angled Narrow Rail,2x4,Round,High,90,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-H -9-120-DW,Angled Narrow Rail,2x4,Round,High,90,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-H -9-277-DW,Angled Narrow Rail,2x4,Round,High,90,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-H -9-120-C1,Angled,2x4,Diffuse,High,90,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-120-C1,Flat,2x4,Diffuse,High,90,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-120-C1,Angled,2x4,Slotted,High,90,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-120-C1,Flat,2x4,Slotted,High,90,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-277-C1,Angled,2x4,Diffuse,High,90,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-277-C1,Flat,2x4,Diffuse,High,90,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-277-C1,Angled,2x4,Slotted,High,90,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-277-C1,Flat,2x4,Slotted,High,90,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-120-C2,Angled,2x4,Diffuse,High,90,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-120-C2,Flat,2x4,Diffuse,High,90,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-120-C2,Angled,2x4,Slotted,High,90,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-120-C2,Flat,2x4,Slotted,High,90,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-277-C2,Angled,2x4,Diffuse,High,90,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-277-C2,Flat,2x4,Diffuse,High,90,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-277-C2,Angled,2x4,Slotted,High,90,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-277-C2,Flat,2x4,Slotted,High,90,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-120-C3,Angled,2x4,Diffuse,High,90,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-H -9-120-C3,Flat,2x4,Diffuse,High,90,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-H -9-120-C3,Angled,2x4,Slotted,High,90,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-H -9-120-C3,Flat,2x4,Slotted,High,90,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-H -9-277-C3,Angled,2x4,Diffuse,High,90,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-H -9-277-C3,Flat,2x4,Diffuse,High,90,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-H -9-277-C3,Angled,2x4,Slotted,High,90,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-H -9-277-C3,Flat,2x4,Slotted,High,90,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-H -9-120-DW,Angled,2x4,Diffuse,High,90,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-H -9-120-DW,Flat,2x4,Diffuse,High,90,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-H -9-120-DW,Angled,2x4,Slotted,High,90,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-H -9-120-DW,Flat,2x4,Slotted,High,90,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-H -9-277-DW,Angled,2x4,Diffuse,High,90,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-H -9-277-DW,Flat,2x4,Diffuse,High,90,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-H -9-277-DW,Angled,2x4,Slotted,High,90,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-H -9-277-DW,Flat,2x4,Slotted,High,90,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-H -9-120-C1,Angled Narrow Rail,2x4,Diffuse,High,90,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-120-C1,Angled Narrow Rail,2x4,Slotted,High,90,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-277-C1,Angled Narrow Rail,2x4,Diffuse,High,90,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-277-C1,Angled Narrow Rail,2x4,Slotted,High,90,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-120-C2,Angled Narrow Rail,2x4,Diffuse,High,90,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-120-C2,Angled Narrow Rail,2x4,Slotted,High,90,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-277-C2,Angled Narrow Rail,2x4,Diffuse,High,90,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-277-C2,Angled Narrow Rail,2x4,Slotted,High,90,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-120-C3,Angled Narrow Rail,2x4,Diffuse,High,90,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-H -9-120-C3,Angled Narrow Rail,2x4,Slotted,High,90,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-H -9-277-C3,Angled Narrow Rail,2x4,Diffuse,High,90,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-H -9-277-C3,Angled Narrow Rail,2x4,Slotted,High,90,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-H -9-120-DW,Angled Narrow Rail,2x4,Diffuse,High,90,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-H -9-120-DW,Angled Narrow Rail,2x4,Slotted,High,90,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-H -9-277-DW,Angled Narrow Rail,2x4,Diffuse,High,90,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-H -9-277-DW,Angled Narrow Rail,2x4,Slotted,High,90,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-H -9-120-C1,Angled,2x4,Round,High,90,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-120-C1,Flat,2x4,Round,High,90,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-277-C1,Angled,2x4,Round,High,90,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-277-C1,Flat,2x4,Round,High,90,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-120-C2,Angled,2x4,Round,High,90,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-120-C2,Flat,2x4,Round,High,90,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-277-C2,Angled,2x4,Round,High,90,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-277-C2,Flat,2x4,Round,High,90,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-120-C3,Angled,2x4,Round,High,90,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-H -9-120-C3,Flat,2x4,Round,High,90,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-H -9-277-C3,Angled,2x4,Round,High,90,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-H -9-277-C3,Flat,2x4,Round,High,90,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-H -9-120-DW,Angled,2x4,Round,High,90,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-H -9-120-DW,Flat,2x4,Round,High,90,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-H -9-277-DW,Angled,2x4,Round,High,90,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-H -9-277-DW,Flat,2x4,Round,High,90,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-H -9-120-C1,Angled Narrow Rail,2x4,Round,High,90,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-277-C1,Angled Narrow Rail,2x4,Round,High,90,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-120-C2,Angled Narrow Rail,2x4,Round,High,90,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-277-C2,Angled Narrow Rail,2x4,Round,High,90,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-120-C3,Angled Narrow Rail,2x4,Round,High,90,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-H -9-277-C3,Angled Narrow Rail,2x4,Round,High,90,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-H -9-120-DW,Angled Narrow Rail,2x4,Round,High,90,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-H -9-277-DW,Angled Narrow Rail,2x4,Round,High,90,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-H -9-120-C1,Angled,2x4,Diffuse,High,90,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-120-C1,Flat,2x4,Diffuse,High,90,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-120-C1,Angled,2x4,Slotted,High,90,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-120-C1,Flat,2x4,Slotted,High,90,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-277-C1,Angled,2x4,Diffuse,High,90,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-277-C1,Flat,2x4,Diffuse,High,90,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-277-C1,Angled,2x4,Slotted,High,90,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-277-C1,Flat,2x4,Slotted,High,90,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-120-C2,Angled,2x4,Diffuse,High,90,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-120-C2,Flat,2x4,Diffuse,High,90,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-120-C2,Angled,2x4,Slotted,High,90,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-120-C2,Flat,2x4,Slotted,High,90,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-277-C2,Angled,2x4,Diffuse,High,90,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-277-C2,Flat,2x4,Diffuse,High,90,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-277-C2,Angled,2x4,Slotted,High,90,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-277-C2,Flat,2x4,Slotted,High,90,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-120-C3,Angled,2x4,Diffuse,High,90,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-H -9-120-C3,Flat,2x4,Diffuse,High,90,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-H -9-120-C3,Angled,2x4,Slotted,High,90,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-H -9-120-C3,Flat,2x4,Slotted,High,90,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-H -9-277-C3,Angled,2x4,Diffuse,High,90,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-H -9-277-C3,Flat,2x4,Diffuse,High,90,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-H -9-277-C3,Angled,2x4,Slotted,High,90,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-H -9-277-C3,Flat,2x4,Slotted,High,90,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-H -9-120-DW,Angled,2x4,Diffuse,High,90,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-H -9-120-DW,Flat,2x4,Diffuse,High,90,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-H -9-120-DW,Angled,2x4,Slotted,High,90,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-H -9-120-DW,Flat,2x4,Slotted,High,90,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-H -9-277-DW,Angled,2x4,Diffuse,High,90,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-H -9-277-DW,Flat,2x4,Diffuse,High,90,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-H -9-277-DW,Angled,2x4,Slotted,High,90,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-H -9-277-DW,Flat,2x4,Slotted,High,90,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-H -9-120-C1,Angled Narrow Rail,2x4,Diffuse,High,90,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-120-C1,Angled Narrow Rail,2x4,Slotted,High,90,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-277-C1,Angled Narrow Rail,2x4,Diffuse,High,90,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-277-C1,Angled Narrow Rail,2x4,Slotted,High,90,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-120-C2,Angled Narrow Rail,2x4,Diffuse,High,90,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-120-C2,Angled Narrow Rail,2x4,Slotted,High,90,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-277-C2,Angled Narrow Rail,2x4,Diffuse,High,90,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-277-C2,Angled Narrow Rail,2x4,Slotted,High,90,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-120-C3,Angled Narrow Rail,2x4,Diffuse,High,90,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-H -9-120-C3,Angled Narrow Rail,2x4,Slotted,High,90,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-H -9-277-C3,Angled Narrow Rail,2x4,Diffuse,High,90,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-H -9-277-C3,Angled Narrow Rail,2x4,Slotted,High,90,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-H -9-120-DW,Angled Narrow Rail,2x4,Diffuse,High,90,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-H -9-120-DW,Angled Narrow Rail,2x4,Slotted,High,90,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-H -9-277-DW,Angled Narrow Rail,2x4,Diffuse,High,90,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-H -9-277-DW,Angled Narrow Rail,2x4,Slotted,High,90,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-H -9-120-C1,Angled,2x4,Round,High,90,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-120-C1,Flat,2x4,Round,High,90,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-277-C1,Angled,2x4,Round,High,90,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-277-C1,Flat,2x4,Round,High,90,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-120-C2,Angled,2x4,Round,High,90,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-120-C2,Flat,2x4,Round,High,90,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-277-C2,Angled,2x4,Round,High,90,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-277-C2,Flat,2x4,Round,High,90,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-120-C3,Angled,2x4,Round,High,90,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-H -9-120-C3,Flat,2x4,Round,High,90,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-H -9-277-C3,Angled,2x4,Round,High,90,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-H -9-277-C3,Flat,2x4,Round,High,90,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-H -9-120-DW,Angled,2x4,Round,High,90,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-H -9-120-DW,Flat,2x4,Round,High,90,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-H -9-277-DW,Angled,2x4,Round,High,90,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-H -9-277-DW,Flat,2x4,Round,High,90,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-H -9-120-C1,Angled Narrow Rail,2x4,Round,High,90,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-277-C1,Angled Narrow Rail,2x4,Round,High,90,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-120-C2,Angled Narrow Rail,2x4,Round,High,90,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-277-C2,Angled Narrow Rail,2x4,Round,High,90,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-120-C3,Angled Narrow Rail,2x4,Round,High,90,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-H -9-277-C3,Angled Narrow Rail,2x4,Round,High,90,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-H -9-120-DW,Angled Narrow Rail,2x4,Round,High,90,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-H -9-277-DW,Angled Narrow Rail,2x4,Round,High,90,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-H -9-120-C2,Angled,2x4,Diffuse,High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-120-C2,Flat,2x4,Diffuse,High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-120-C2,Angled,2x4,Slotted,High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-120-C2,Flat,2x4,Slotted,High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-277-C2,Angled,2x4,Diffuse,High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-277-C2,Flat,2x4,Diffuse,High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-277-C2,Angled,2x4,Slotted,High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-277-C2,Flat,2x4,Slotted,High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-120-C2,Angled Narrow Rail,2x4,Diffuse,High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-120-C2,Angled Narrow Rail,2x4,Slotted,High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-277-C2,Angled Narrow Rail,2x4,Diffuse,High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-277-C2,Angled Narrow Rail,2x4,Slotted,High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-120-C2,Angled,2x4,Round,High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-120-C2,Flat,2x4,Round,High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-277-C2,Angled,2x4,Round,High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-277-C2,Flat,2x4,Round,High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-120-C2,Angled Narrow Rail,2x4,Round,High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-277-C2,Angled Narrow Rail,2x4,Round,High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-120-C2,Angled,2x4,Diffuse,High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-120-C2,Flat,2x4,Diffuse,High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-120-C2,Angled,2x4,Slotted,High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-120-C2,Flat,2x4,Slotted,High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-277-C2,Angled,2x4,Diffuse,High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-277-C2,Flat,2x4,Diffuse,High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-277-C2,Angled,2x4,Slotted,High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-277-C2,Flat,2x4,Slotted,High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-120-C2,Angled Narrow Rail,2x4,Diffuse,High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-120-C2,Angled Narrow Rail,2x4,Slotted,High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-277-C2,Angled Narrow Rail,2x4,Diffuse,High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-277-C2,Angled Narrow Rail,2x4,Slotted,High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-120-C2,Angled,2x4,Round,High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-120-C2,Flat,2x4,Round,High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-277-C2,Angled,2x4,Round,High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-277-C2,Flat,2x4,Round,High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-120-C2,Angled Narrow Rail,2x4,Round,High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-277-C2,Angled Narrow Rail,2x4,Round,High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-120-C2,Angled,2x4,Diffuse,High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-120-C2,Flat,2x4,Diffuse,High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-120-C2,Angled,2x4,Slotted,High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-120-C2,Flat,2x4,Slotted,High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-H -9-277-C2,Angled,2x4,Diffuse,High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-H -9-277-C2,Flat,2x4,Diffuse,High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-H -9-277-C2,Angled,2x4,Slotted,High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-H -9-277-C2,Flat,2x4,Slotted,High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-120-C2,Angled Narrow Rail,2x4,Diffuse,High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-120-C2,Angled Narrow Rail,2x4,Slotted,High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-H -9-277-C2,Angled Narrow Rail,2x4,Diffuse,High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-H -9-277-C2,Angled Narrow Rail,2x4,Slotted,High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-120-C2,Angled,2x4,Round,High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-120-C2,Flat,2x4,Round,High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-H -9-277-C2,Angled,2x4,Round,High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-H -9-277-C2,Flat,2x4,Round,High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-120-C2,Angled Narrow Rail,2x4,Round,High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-H -9-277-C2,Angled Narrow Rail,2x4,Round,High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-120-C1,Wave,2x4,Diffuse,High,90,3500K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-277-C1,Wave,2x4,Diffuse,High,90,3500K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-120-C2,Wave,2x4,Diffuse,High,90,3500K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-277-C2,Wave,2x4,Diffuse,High,90,3500K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-120-C3,Wave,2x4,Diffuse,High,90,3500K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-H -9-277-C3,Wave,2x4,Diffuse,High,90,3500K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-H -9-120-DW,Wave,2x4,Diffuse,High,90,3500K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-H -9-277-DW,Wave,2x4,Diffuse,High,90,3500K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-H -9-120-C1,Wave,2x4,Diffuse,High,90,3000K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-277-C1,Wave,2x4,Diffuse,High,90,3000K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-120-C2,Wave,2x4,Diffuse,High,90,3000K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-277-C2,Wave,2x4,Diffuse,High,90,3000K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-120-C3,Wave,2x4,Diffuse,High,90,3000K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-H -9-277-C3,Wave,2x4,Diffuse,High,90,3000K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-H -9-120-DW,Wave,2x4,Diffuse,High,90,3000K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-H -9-277-DW,Wave,2x4,Diffuse,High,90,3000K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-H -9-120-C1,Wave,2x4,Diffuse,High,90,4000K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-277-C1,Wave,2x4,Diffuse,High,90,4000K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-120-C2,Wave,2x4,Diffuse,High,90,4000K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-277-C2,Wave,2x4,Diffuse,High,90,4000K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-120-C3,Wave,2x4,Diffuse,High,90,4000K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-H -9-277-C3,Wave,2x4,Diffuse,High,90,4000K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-H -9-120-DW,Wave,2x4,Diffuse,High,90,4000K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-H -9-277-DW,Wave,2x4,Diffuse,High,90,4000K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-H -9-120-C2,Wave,2x4,Diffuse,High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-277-C2,Wave,2x4,Diffuse,High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-120-C2,Wave,2x4,Diffuse,High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-277-C2,Wave,2x4,Diffuse,High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-120-C2,Wave,2x4,Diffuse,High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-H -9-277-C2,Wave,2x4,Diffuse,High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-120-C1,Angled,2x4,Diffuse,Very High,90,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-120-C1,Flat,2x4,Diffuse,Very High,90,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-120-C1,Angled,2x4,Slotted,Very High,90,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-120-C1,Flat,2x4,Slotted,Very High,90,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-277-C1,Angled,2x4,Diffuse,Very High,90,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-277-C1,Flat,2x4,Diffuse,Very High,90,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-277-C1,Angled,2x4,Slotted,Very High,90,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-277-C1,Flat,2x4,Slotted,Very High,90,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-120-C2,Angled,2x4,Diffuse,Very High,90,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-120-C2,Flat,2x4,Diffuse,Very High,90,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-120-C2,Angled,2x4,Slotted,Very High,90,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-120-C2,Flat,2x4,Slotted,Very High,90,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-277-C2,Angled,2x4,Diffuse,Very High,90,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-277-C2,Flat,2x4,Diffuse,Very High,90,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-277-C2,Angled,2x4,Slotted,Very High,90,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-277-C2,Flat,2x4,Slotted,Very High,90,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-120-C3,Angled,2x4,Diffuse,Very High,90,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-V-9-120-C3,Flat,2x4,Diffuse,Very High,90,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-V-9-120-C3,Angled,2x4,Slotted,Very High,90,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-V-9-120-C3,Flat,2x4,Slotted,Very High,90,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-V-9-277-C3,Angled,2x4,Diffuse,Very High,90,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-V-9-277-C3,Flat,2x4,Diffuse,Very High,90,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-V-9-277-C3,Angled,2x4,Slotted,Very High,90,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-V-9-277-C3,Flat,2x4,Slotted,Very High,90,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-V-9-120-DW,Angled,2x4,Diffuse,Very High,90,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-V-9-120-DW,Flat,2x4,Diffuse,Very High,90,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-V-9-120-DW,Angled,2x4,Slotted,Very High,90,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-V-9-120-DW,Flat,2x4,Slotted,Very High,90,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-V-9-277-DW,Angled,2x4,Diffuse,Very High,90,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-V-9-277-DW,Flat,2x4,Diffuse,Very High,90,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-V-9-277-DW,Angled,2x4,Slotted,Very High,90,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-V-9-277-DW,Flat,2x4,Slotted,Very High,90,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-V-9-120-C1,Angled Narrow Rail,2x4,Diffuse,Very High,90,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-120-C1,Angled Narrow Rail,2x4,Slotted,Very High,90,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-277-C1,Angled Narrow Rail,2x4,Diffuse,Very High,90,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-277-C1,Angled Narrow Rail,2x4,Slotted,Very High,90,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-120-C2,Angled Narrow Rail,2x4,Diffuse,Very High,90,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-120-C2,Angled Narrow Rail,2x4,Slotted,Very High,90,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-277-C2,Angled Narrow Rail,2x4,Diffuse,Very High,90,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-277-C2,Angled Narrow Rail,2x4,Slotted,Very High,90,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-120-C3,Angled Narrow Rail,2x4,Diffuse,Very High,90,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-V-9-120-C3,Angled Narrow Rail,2x4,Slotted,Very High,90,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-V-9-277-C3,Angled Narrow Rail,2x4,Diffuse,Very High,90,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-V-9-277-C3,Angled Narrow Rail,2x4,Slotted,Very High,90,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-V-9-120-DW,Angled Narrow Rail,2x4,Diffuse,Very High,90,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-V-9-120-DW,Angled Narrow Rail,2x4,Slotted,Very High,90,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-V-9-277-DW,Angled Narrow Rail,2x4,Diffuse,Very High,90,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-V-9-277-DW,Angled Narrow Rail,2x4,Slotted,Very High,90,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-V-9-120-C1,Angled,2x4,Round,Very High,90,3500K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-120-C1,Flat,2x4,Round,Very High,90,3500K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-277-C1,Angled,2x4,Round,Very High,90,3500K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-277-C1,Flat,2x4,Round,Very High,90,3500K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-120-C2,Angled,2x4,Round,Very High,90,3500K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-120-C2,Flat,2x4,Round,Very High,90,3500K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-277-C2,Angled,2x4,Round,Very High,90,3500K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-277-C2,Flat,2x4,Round,Very High,90,3500K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-120-C3,Angled,2x4,Round,Very High,90,3500K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-V-9-120-C3,Flat,2x4,Round,Very High,90,3500K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-V-9-277-C3,Angled,2x4,Round,Very High,90,3500K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-V-9-277-C3,Flat,2x4,Round,Very High,90,3500K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-V-9-120-DW,Angled,2x4,Round,Very High,90,3500K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-V-9-120-DW,Flat,2x4,Round,Very High,90,3500K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-V-9-277-DW,Angled,2x4,Round,Very High,90,3500K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-V-9-277-DW,Flat,2x4,Round,Very High,90,3500K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-V-9-120-C1,Angled Narrow Rail,2x4,Round,Very High,90,3500K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-277-C1,Angled Narrow Rail,2x4,Round,Very High,90,3500K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-120-C2,Angled Narrow Rail,2x4,Round,Very High,90,3500K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-277-C2,Angled Narrow Rail,2x4,Round,Very High,90,3500K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-120-C3,Angled Narrow Rail,2x4,Round,Very High,90,3500K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-V-9-277-C3,Angled Narrow Rail,2x4,Round,Very High,90,3500K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-V-9-120-DW,Angled Narrow Rail,2x4,Round,Very High,90,3500K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-V-9-277-DW,Angled Narrow Rail,2x4,Round,Very High,90,3500K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-V-9-120-C1,Angled,2x4,Diffuse,Very High,90,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-120-C1,Flat,2x4,Diffuse,Very High,90,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-120-C1,Angled,2x4,Slotted,Very High,90,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-120-C1,Flat,2x4,Slotted,Very High,90,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-277-C1,Angled,2x4,Diffuse,Very High,90,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-277-C1,Flat,2x4,Diffuse,Very High,90,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-277-C1,Angled,2x4,Slotted,Very High,90,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-277-C1,Flat,2x4,Slotted,Very High,90,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-120-C2,Angled,2x4,Diffuse,Very High,90,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-120-C2,Flat,2x4,Diffuse,Very High,90,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-120-C2,Angled,2x4,Slotted,Very High,90,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-120-C2,Flat,2x4,Slotted,Very High,90,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-277-C2,Angled,2x4,Diffuse,Very High,90,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-277-C2,Flat,2x4,Diffuse,Very High,90,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-277-C2,Angled,2x4,Slotted,Very High,90,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-277-C2,Flat,2x4,Slotted,Very High,90,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-120-C3,Angled,2x4,Diffuse,Very High,90,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-V-9-120-C3,Flat,2x4,Diffuse,Very High,90,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-V-9-120-C3,Angled,2x4,Slotted,Very High,90,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-V-9-120-C3,Flat,2x4,Slotted,Very High,90,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-V-9-277-C3,Angled,2x4,Diffuse,Very High,90,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-V-9-277-C3,Flat,2x4,Diffuse,Very High,90,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-V-9-277-C3,Angled,2x4,Slotted,Very High,90,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-V-9-277-C3,Flat,2x4,Slotted,Very High,90,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-V-9-120-DW,Angled,2x4,Diffuse,Very High,90,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-V-9-120-DW,Flat,2x4,Diffuse,Very High,90,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-V-9-120-DW,Angled,2x4,Slotted,Very High,90,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-V-9-120-DW,Flat,2x4,Slotted,Very High,90,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-V-9-277-DW,Angled,2x4,Diffuse,Very High,90,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-V-9-277-DW,Flat,2x4,Diffuse,Very High,90,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-V-9-277-DW,Angled,2x4,Slotted,Very High,90,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-V-9-277-DW,Flat,2x4,Slotted,Very High,90,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-V-9-120-C1,Angled Narrow Rail,2x4,Diffuse,Very High,90,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-120-C1,Angled Narrow Rail,2x4,Slotted,Very High,90,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-277-C1,Angled Narrow Rail,2x4,Diffuse,Very High,90,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-277-C1,Angled Narrow Rail,2x4,Slotted,Very High,90,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-120-C2,Angled Narrow Rail,2x4,Diffuse,Very High,90,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-120-C2,Angled Narrow Rail,2x4,Slotted,Very High,90,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-277-C2,Angled Narrow Rail,2x4,Diffuse,Very High,90,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-277-C2,Angled Narrow Rail,2x4,Slotted,Very High,90,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-120-C3,Angled Narrow Rail,2x4,Diffuse,Very High,90,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-V-9-120-C3,Angled Narrow Rail,2x4,Slotted,Very High,90,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-V-9-277-C3,Angled Narrow Rail,2x4,Diffuse,Very High,90,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-V-9-277-C3,Angled Narrow Rail,2x4,Slotted,Very High,90,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-V-9-120-DW,Angled Narrow Rail,2x4,Diffuse,Very High,90,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-V-9-120-DW,Angled Narrow Rail,2x4,Slotted,Very High,90,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-V-9-277-DW,Angled Narrow Rail,2x4,Diffuse,Very High,90,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-V-9-277-DW,Angled Narrow Rail,2x4,Slotted,Very High,90,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-V-9-120-C1,Angled,2x4,Round,Very High,90,3000K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-120-C1,Flat,2x4,Round,Very High,90,3000K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-277-C1,Angled,2x4,Round,Very High,90,3000K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-277-C1,Flat,2x4,Round,Very High,90,3000K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-120-C2,Angled,2x4,Round,Very High,90,3000K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-120-C2,Flat,2x4,Round,Very High,90,3000K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-277-C2,Angled,2x4,Round,Very High,90,3000K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-277-C2,Flat,2x4,Round,Very High,90,3000K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-120-C3,Angled,2x4,Round,Very High,90,3000K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-V-9-120-C3,Flat,2x4,Round,Very High,90,3000K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-V-9-277-C3,Angled,2x4,Round,Very High,90,3000K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-V-9-277-C3,Flat,2x4,Round,Very High,90,3000K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-V-9-120-DW,Angled,2x4,Round,Very High,90,3000K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-V-9-120-DW,Flat,2x4,Round,Very High,90,3000K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-V-9-277-DW,Angled,2x4,Round,Very High,90,3000K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-V-9-277-DW,Flat,2x4,Round,Very High,90,3000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-V-9-120-C1,Angled Narrow Rail,2x4,Round,Very High,90,3000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-277-C1,Angled Narrow Rail,2x4,Round,Very High,90,3000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-120-C2,Angled Narrow Rail,2x4,Round,Very High,90,3000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-277-C2,Angled Narrow Rail,2x4,Round,Very High,90,3000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-120-C3,Angled Narrow Rail,2x4,Round,Very High,90,3000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-V-9-277-C3,Angled Narrow Rail,2x4,Round,Very High,90,3000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-V-9-120-DW,Angled Narrow Rail,2x4,Round,Very High,90,3000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-V-9-277-DW,Angled Narrow Rail,2x4,Round,Very High,90,3000K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-V-9-120-C1,Angled,2x4,Diffuse,Very High,90,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-120-C1,Flat,2x4,Diffuse,Very High,90,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-120-C1,Angled,2x4,Slotted,Very High,90,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-120-C1,Flat,2x4,Slotted,Very High,90,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-277-C1,Angled,2x4,Diffuse,Very High,90,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-277-C1,Flat,2x4,Diffuse,Very High,90,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-277-C1,Angled,2x4,Slotted,Very High,90,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-277-C1,Flat,2x4,Slotted,Very High,90,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-120-C2,Angled,2x4,Diffuse,Very High,90,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-120-C2,Flat,2x4,Diffuse,Very High,90,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-120-C2,Angled,2x4,Slotted,Very High,90,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-120-C2,Flat,2x4,Slotted,Very High,90,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-277-C2,Angled,2x4,Diffuse,Very High,90,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-277-C2,Flat,2x4,Diffuse,Very High,90,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-277-C2,Angled,2x4,Slotted,Very High,90,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-277-C2,Flat,2x4,Slotted,Very High,90,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-120-C3,Angled,2x4,Diffuse,Very High,90,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-DCO-V-9-120-C3,Flat,2x4,Diffuse,Very High,90,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-SCO-V-9-120-C3,Angled,2x4,Slotted,Very High,90,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-SCO-V-9-120-C3,Flat,2x4,Slotted,Very High,90,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-DCO-V-9-277-C3,Angled,2x4,Diffuse,Very High,90,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-DCO-V-9-277-C3,Flat,2x4,Diffuse,Very High,90,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-SCO-V-9-277-C3,Angled,2x4,Slotted,Very High,90,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-SCO-V-9-277-C3,Flat,2x4,Slotted,Very High,90,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-DCO-V-9-120-DW,Angled,2x4,Diffuse,Very High,90,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-DCO-V-9-120-DW,Flat,2x4,Diffuse,Very High,90,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-SCO-V-9-120-DW,Angled,2x4,Slotted,Very High,90,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-SCO-V-9-120-DW,Flat,2x4,Slotted,Very High,90,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-DCO-V-9-277-DW,Angled,2x4,Diffuse,Very High,90,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-DCO-V-9-277-DW,Flat,2x4,Diffuse,Very High,90,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-SCO-V-9-277-DW,Angled,2x4,Slotted,Very High,90,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-SCO-V-9-277-DW,Flat,2x4,Slotted,Very High,90,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-V-9-120-C1,Angled Narrow Rail,2x4,Diffuse,Very High,90,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-120-C1,Angled Narrow Rail,2x4,Slotted,Very High,90,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-277-C1,Angled Narrow Rail,2x4,Diffuse,Very High,90,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-277-C1,Angled Narrow Rail,2x4,Slotted,Very High,90,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-120-C2,Angled Narrow Rail,2x4,Diffuse,Very High,90,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-120-C2,Angled Narrow Rail,2x4,Slotted,Very High,90,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-277-C2,Angled Narrow Rail,2x4,Diffuse,Very High,90,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-277-C2,Angled Narrow Rail,2x4,Slotted,Very High,90,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-120-C3,Angled Narrow Rail,2x4,Diffuse,Very High,90,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-V-9-120-C3,Angled Narrow Rail,2x4,Slotted,Very High,90,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-V-9-277-C3,Angled Narrow Rail,2x4,Diffuse,Very High,90,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-SCO-V-9-277-C3,Angled Narrow Rail,2x4,Slotted,Very High,90,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-DCO-V-9-120-DW,Angled Narrow Rail,2x4,Diffuse,Very High,90,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-V-9-120-DW,Angled Narrow Rail,2x4,Slotted,Very High,90,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-DCO-V-9-277-DW,Angled Narrow Rail,2x4,Diffuse,Very High,90,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-SCO-V-9-277-DW,Angled Narrow Rail,2x4,Slotted,Very High,90,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-RCO-V-9-120-C1,Angled,2x4,Round,Very High,90,4000K,120,1” T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-120-C1,Flat,2x4,Round,Very High,90,4000K,120,1” T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-277-C1,Angled,2x4,Round,Very High,90,4000K,277,1” T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-277-C1,Flat,2x4,Round,Very High,90,4000K,277,1” T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-120-C2,Angled,2x4,Round,Very High,90,4000K,120,16” T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-120-C2,Flat,2x4,Round,Very High,90,4000K,120,16” T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-277-C2,Angled,2x4,Round,Very High,90,4000K,277,16” T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-277-C2,Flat,2x4,Round,Very High,90,4000K,277,16” T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-120-C3,Angled,2x4,Round,Very High,90,4000K,120,Screw Slot,24,48
HPR LED-F-2x4-RCO-V-9-120-C3,Flat,2x4,Round,Very High,90,4000K,120,Screw Slot,24,48
HPR LED-A-2x4-RCO-V-9-277-C3,Angled,2x4,Round,Very High,90,4000K,277,Screw Slot,24,48
HPR LED-F-2x4-RCO-V-9-277-C3,Flat,2x4,Round,Very High,90,4000K,277,Screw Slot,24,48
HPR LED-A-2x4-RCO-V-9-120-DW,Angled,2x4,Round,Very High,90,4000K,120,Drywall Kit,24,48
HPR LED-F-2x4-RCO-V-9-120-DW,Flat,2x4,Round,Very High,90,4000K,120,Drywall Kit,24,48
HPR LED-A-2x4-RCO-V-9-277-DW,Angled,2x4,Round,Very High,90,4000K,277,Drywall Kit,24,48
HPR LED-F-2x4-RCO-V-9-277-DW,Flat,2x4,Round,Very High,90,4000K,277,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-V-9-120-C1,Angled Narrow Rail,2x4,Round,Very High,90,4000K,120,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-277-C1,Angled Narrow Rail,2x4,Round,Very High,90,4000K,277,1” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-120-C2,Angled Narrow Rail,2x4,Round,Very High,90,4000K,120,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-277-C2,Angled Narrow Rail,2x4,Round,Very High,90,4000K,277,16” T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-120-C3,Angled Narrow Rail,2x4,Round,Very High,90,4000K,120,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-V-9-277-C3,Angled Narrow Rail,2x4,Round,Very High,90,4000K,277,Screw Slot,24,48
HPR LED-ANR-2x4-RCO-V-9-120-DW,Angled Narrow Rail,2x4,Round,Very High,90,4000K,120,Drywall Kit,24,48
HPR LED-ANR-2x4-RCO-V-9-277-DW,Angled Narrow Rail,2x4,Round,Very High,90,4000K,277,Drywall Kit,24,48
HPR LED-A-2x4-DCO-V-9-120-C2,Angled,2x4,Diffuse,Very High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-120-C2,Flat,2x4,Diffuse,Very High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-120-C2,Angled,2x4,Slotted,Very High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-120-C2,Flat,2x4,Slotted,Very High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-277-C2,Angled,2x4,Diffuse,Very High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-277-C2,Flat,2x4,Diffuse,Very High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-277-C2,Angled,2x4,Slotted,Very High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-277-C2,Flat,2x4,Slotted,Very High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-120-C2,Angled Narrow Rail,2x4,Diffuse,Very High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-120-C2,Angled Narrow Rail,2x4,Slotted,Very High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-277-C2,Angled Narrow Rail,2x4,Diffuse,Very High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-277-C2,Angled Narrow Rail,2x4,Slotted,Very High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-120-C2,Angled,2x4,Round,Very High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-120-C2,Flat,2x4,Round,Very High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-277-C2,Angled,2x4,Round,Very High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-277-C2,Flat,2x4,Round,Very High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-120-C2,Angled Narrow Rail,2x4,Round,Very High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-277-C2,Angled Narrow Rail,2x4,Round,Very High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-120-C2,Angled,2x4,Diffuse,Very High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-120-C2,Flat,2x4,Diffuse,Very High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-120-C2,Angled,2x4,Slotted,Very High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-120-C2,Flat,2x4,Slotted,Very High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-277-C2,Angled,2x4,Diffuse,Very High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-277-C2,Flat,2x4,Diffuse,Very High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-277-C2,Angled,2x4,Slotted,Very High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-277-C2,Flat,2x4,Slotted,Very High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-120-C2,Angled Narrow Rail,2x4,Diffuse,Very High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-120-C2,Angled Narrow Rail,2x4,Slotted,Very High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-277-C2,Angled Narrow Rail,2x4,Diffuse,Very High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-277-C2,Angled Narrow Rail,2x4,Slotted,Very High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-120-C2,Angled,2x4,Round,Very High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-120-C2,Flat,2x4,Round,Very High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-277-C2,Angled,2x4,Round,Very High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-277-C2,Flat,2x4,Round,Very High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-120-C2,Angled Narrow Rail,2x4,Round,Very High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-277-C2,Angled Narrow Rail,2x4,Round,Very High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-120-C2,Angled,2x4,Diffuse,Very High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-120-C2,Flat,2x4,Diffuse,Very High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-120-C2,Angled,2x4,Slotted,Very High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-120-C2,Flat,2x4,Slotted,Very High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-DCO-V-9-277-C2,Angled,2x4,Diffuse,Very High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-DCO-V-9-277-C2,Flat,2x4,Diffuse,Very High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-SCO-V-9-277-C2,Angled,2x4,Slotted,Very High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-SCO-V-9-277-C2,Flat,2x4,Slotted,Very High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-120-C2,Angled Narrow Rail,2x4,Diffuse,Very High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-120-C2,Angled Narrow Rail,2x4,Slotted,Very High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-DCO-V-9-277-C2,Angled Narrow Rail,2x4,Diffuse,Very High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-SCO-V-9-277-C2,Angled Narrow Rail,2x4,Slotted,Very High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-120-C2,Angled,2x4,Round,Very High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-120-C2,Flat,2x4,Round,Very High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-A-2x4-RCO-V-9-277-C2,Angled,2x4,Round,Very High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-F-2x4-RCO-V-9-277-C2,Flat,2x4,Round,Very High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-120-C2,Angled Narrow Rail,2x4,Round,Very High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-ANR-2x4-RCO-V-9-277-C2,Angled Narrow Rail,2x4,Round,Very High,90,4000K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-120-C1,Wave,2x4,Diffuse,Very High,90,3500K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-277-C1,Wave,2x4,Diffuse,Very High,90,3500K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-120-C2,Wave,2x4,Diffuse,Very High,90,3500K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-277-C2,Wave,2x4,Diffuse,Very High,90,3500K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-120-C3,Wave,2x4,Diffuse,Very High,90,3500K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-V-9-277-C3,Wave,2x4,Diffuse,Very High,90,3500K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-V-9-120-DW,Wave,2x4,Diffuse,Very High,90,3500K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-V-9-277-DW,Wave,2x4,Diffuse,Very High,90,3500K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-V-9-120-C1,Wave,2x4,Diffuse,Very High,90,3000K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-277-C1,Wave,2x4,Diffuse,Very High,90,3000K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-120-C2,Wave,2x4,Diffuse,Very High,90,3000K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-277-C2,Wave,2x4,Diffuse,Very High,90,3000K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-120-C3,Wave,2x4,Diffuse,Very High,90,3000K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-V-9-277-C3,Wave,2x4,Diffuse,Very High,90,3000K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-V-9-120-DW,Wave,2x4,Diffuse,Very High,90,3000K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-V-9-277-DW,Wave,2x4,Diffuse,Very High,90,3000K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-V-9-120-C1,Wave,2x4,Diffuse,Very High,90,4000K,120,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-277-C1,Wave,2x4,Diffuse,Very High,90,4000K,277,1” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-120-C2,Wave,2x4,Diffuse,Very High,90,4000K,120,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-277-C2,Wave,2x4,Diffuse,Very High,90,4000K,277,16” T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-120-C3,Wave,2x4,Diffuse,Very High,90,4000K,120,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-V-9-277-C3,Wave,2x4,Diffuse,Very High,90,4000K,277,Screw Slot,24,48
HPR LED-WAV-2x4-DCO-V-9-120-DW,Wave,2x4,Diffuse,Very High,90,4000K,120,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-V-9-277-DW,Wave,2x4,Diffuse,Very High,90,4000K,277,Drywall Kit,24,48
HPR LED-WAV-2x4-DCO-V-9-120-C2,Wave,2x4,Diffuse,Very High,90,3500K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-277-C2,Wave,2x4,Diffuse,Very High,90,3500K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-120-C2,Wave,2x4,Diffuse,Very High,90,3000K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-277-C2,Wave,2x4,Diffuse,Very High,90,3000K,277,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-120-C2,Wave,2x4,Diffuse,Very High,90,4000K,120,9/16' T-Bar,24,48
HPR LED-WAV-2x4-DCO-V-9-277-C2,Wave,2x4,Diffuse,Very High,90,4000K,277,9/16' T-Bar,24,48
