,Size##length##inches,Uplight Engine##other##,Downlight Engine##other##,Color Temperature##other##,Voltage##electrical_potential##volts,Circuiting##other##,Ceiling Type##other##,Integrated Sensor##other##,Model Number##other##
HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C1-OBO,48,Standard,Standard,3000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C1-OBO
HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C1-OBO,96,Standard,Standard,3000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C1-OBO
HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C1-OBO,48,Standard,High Output,3000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C1-OBO
HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C1-OBO,96,Standard,High Output,3000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C1-OBO
HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C1-OBO,48,Standard,Standard,3500K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C1-OBO
HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C1-OBO,96,Standard,Standard,3500K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C1-OBO
HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C1-OBO,48,Standard,High Output,3500K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C1-OBO
HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C1-OBO,96,Standard,High Output,3500K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C1-OBO
HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C1-OBO,48,Standard,Standard,4000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C1-OBO
HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C1-OBO,96,Standard,Standard,4000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C1-OBO
HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C1-OBO,48,Standard,High Output,4000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C1-OBO
HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C1-OBO,96,Standard,High Output,4000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C1-OBO
HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C1-OBO,48,Standard,Standard,3000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C1-OBO
HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C1-OBO,96,Standard,Standard,3000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C1-OBO
HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C1-OBO,48,Standard,High Output,3000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C1-OBO
HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C1-OBO,96,Standard,High Output,3000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C1-OBO
HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C1-OBO,48,Standard,Standard,3500K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C1-OBO
HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C1-OBO,96,Standard,Standard,3500K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C1-OBO
HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C1-OBO,48,Standard,High Output,3500K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C1-OBO
HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C1-OBO,96,Standard,High Output,3500K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C1-OBO
HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C1-OBO,48,Standard,Standard,4000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C1-OBO
HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C1-OBO,96,Standard,Standard,4000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C1-OBO
HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C1-OBO,48,Standard,High Output,4000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C1-OBO
HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C1-OBO,96,Standard,High Output,4000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C1-OBO
HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C2-OBO,48,Standard,Standard,3000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C2-OBO
HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C2-OBO,96,Standard,Standard,3000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C2-OBO
HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C2-OBO,48,Standard,High Output,3000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C2-OBO
HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C2-OBO,96,Standard,High Output,3000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C2-OBO
HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C2-OBO,48,Standard,Standard,3500K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C2-OBO
HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C2-OBO,96,Standard,Standard,3500K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C2-OBO
HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C2-OBO,48,Standard,High Output,3500K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C2-OBO
HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C2-OBO,96,Standard,High Output,3500K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C2-OBO
HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C2-OBO,48,Standard,Standard,4000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C2-OBO
HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C2-OBO,96,Standard,Standard,4000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C2-OBO
HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C2-OBO,48,Standard,High Output,4000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C2-OBO
HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C2-OBO,96,Standard,High Output,4000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C2-OBO
HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C2-OBO,48,Standard,Standard,3000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C2-OBO
HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C2-OBO,96,Standard,Standard,3000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C2-OBO
HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C2-OBO,48,Standard,High Output,3000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C2-OBO
HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C2-OBO,96,Standard,High Output,3000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C2-OBO
HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C2-OBO,48,Standard,Standard,3500K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C2-OBO
HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C2-OBO,96,Standard,Standard,3500K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C2-OBO
HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C2-OBO,48,Standard,High Output,3500K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C2-OBO
HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C2-OBO,96,Standard,High Output,3500K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C2-OBO
HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C2-OBO,48,Standard,Standard,4000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C2-OBO
HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C2-OBO,96,Standard,Standard,4000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C2-OBO
HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C2-OBO,48,Standard,High Output,4000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C2-OBO
HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C2-OBO,96,Standard,High Output,4000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C2-OBO
HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C3-OBO,48,Standard,Standard,3000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C3-OBO
HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C3-OBO,96,Standard,Standard,3000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C3-OBO
HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C3-OBO,48,Standard,High Output,3000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C3-OBO
HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C3-OBO,96,Standard,High Output,3000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C3-OBO
HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C3-OBO,48,Standard,Standard,3500K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C3-OBO
HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C3-OBO,96,Standard,Standard,3500K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C3-OBO
HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C3-OBO,48,Standard,High Output,3500K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C3-OBO
HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C3-OBO,96,Standard,High Output,3500K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C3-OBO
HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C3-OBO,48,Standard,Standard,4000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C3-OBO
HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C3-OBO,96,Standard,Standard,4000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C3-OBO
HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C3-OBO,48,Standard,High Output,4000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C3-OBO
HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C3-OBO,96,Standard,High Output,4000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C3-OBO
HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C3-OBO,48,Standard,Standard,3000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C3-OBO
HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C3-OBO,96,Standard,Standard,3000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C3-OBO
HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C3-OBO,48,Standard,High Output,3000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C3-OBO
HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C3-OBO,96,Standard,High Output,3000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C3-OBO
HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C3-OBO,48,Standard,Standard,3500K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C3-OBO
HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C3-OBO,96,Standard,Standard,3500K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C3-OBO
HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C3-OBO,48,Standard,High Output,3500K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C3-OBO
HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C3-OBO,96,Standard,High Output,3500K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C3-OBO
HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C3-OBO,48,Standard,Standard,4000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C3-OBO
HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C3-OBO,96,Standard,Standard,4000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C3-OBO
HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C3-OBO,48,Standard,High Output,4000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C3-OBO
HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C3-OBO,96,Standard,High Output,4000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C3-OBO
HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C4-OBO,48,Standard,Standard,3000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C4-OBO
HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C4-OBO,96,Standard,Standard,3000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C4-OBO
HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C4-OBO,48,Standard,High Output,3000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C4-OBO
HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C4-OBO,96,Standard,High Output,3000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C4-OBO
HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C4-OBO,48,Standard,Standard,3500K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C4-OBO
HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C4-OBO,96,Standard,Standard,3500K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C4-OBO
HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C4-OBO,48,Standard,High Output,3500K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C4-OBO
HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C4-OBO,96,Standard,High Output,3500K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C4-OBO
HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C4-OBO,48,Standard,Standard,4000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C4-OBO
HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C4-OBO,96,Standard,Standard,4000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C4-OBO
HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C4-OBO,48,Standard,High Output,4000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C4-OBO
HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C4-OBO,96,Standard,High Output,4000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C4-OBO
HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C4-OBO,48,Standard,Standard,3000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C4-OBO
HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C4-OBO,96,Standard,Standard,3000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C4-OBO
HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C4-OBO,48,Standard,High Output,3000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C4-OBO
HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C4-OBO,96,Standard,High Output,3000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C4-OBO
HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C4-OBO,48,Standard,Standard,3500K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C4-OBO
HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C4-OBO,96,Standard,Standard,3500K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C4-OBO
HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C4-OBO,48,Standard,High Output,3500K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C4-OBO
HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C4-OBO,96,Standard,High Output,3500K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C4-OBO
HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C4-OBO,48,Standard,Standard,4000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C4-OBO
HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C4-OBO,96,Standard,Standard,4000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C4-OBO
HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C4-OBO,48,Standard,High Output,4000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C4-OBO
HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C4-OBO,96,Standard,High Output,4000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C4-OBO
HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C1-OBO,144,Standard,Standard,3000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C1-OBO
HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C1-OBO,144,Standard,High Output,3000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C1-OBO
HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C1-OBO,144,Standard,Standard,3500K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C1-OBO
HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C1-OBO,144,Standard,High Output,3500K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C1-OBO
HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C1-OBO,144,Standard,Standard,4000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C1-OBO
HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C1-OBO,144,Standard,High Output,4000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C1-OBO
HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C1-OBO,144,Standard,Standard,3000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C1-OBO
HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C1-OBO,144,Standard,High Output,3000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C1-OBO
HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C1-OBO,144,Standard,Standard,3500K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C1-OBO
HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C1-OBO,144,Standard,High Output,3500K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C1-OBO
HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C1-OBO,144,Standard,Standard,4000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C1-OBO
HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C1-OBO,144,Standard,High Output,4000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C1-OBO
HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C2-OBO,144,Standard,Standard,3000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C2-OBO
HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C2-OBO,144,Standard,High Output,3000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C2-OBO
HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C2-OBO,144,Standard,Standard,3500K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C2-OBO
HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C2-OBO,144,Standard,High Output,3500K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C2-OBO
HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C2-OBO,144,Standard,Standard,4000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C2-OBO
HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C2-OBO,144,Standard,High Output,4000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C2-OBO
HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C2-OBO,144,Standard,Standard,3000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C2-OBO
HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C2-OBO,144,Standard,High Output,3000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C2-OBO
HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C2-OBO,144,Standard,Standard,3500K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C2-OBO
HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C2-OBO,144,Standard,High Output,3500K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C2-OBO
HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C2-OBO,144,Standard,Standard,4000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C2-OBO
HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C2-OBO,144,Standard,High Output,4000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C2-OBO
HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C3-OBO,144,Standard,Standard,3000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C3-OBO
HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C3-OBO,144,Standard,High Output,3000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C3-OBO
HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C3-OBO,144,Standard,Standard,3500K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C3-OBO
HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C3-OBO,144,Standard,High Output,3500K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C3-OBO
HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C3-OBO,144,Standard,Standard,4000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C3-OBO
HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C3-OBO,144,Standard,High Output,4000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C3-OBO
HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C3-OBO,144,Standard,Standard,3000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C3-OBO
HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C3-OBO,144,Standard,High Output,3000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C3-OBO
HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C3-OBO,144,Standard,Standard,3500K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C3-OBO
HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C3-OBO,144,Standard,High Output,3500K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C3-OBO
HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C3-OBO,144,Standard,Standard,4000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C3-OBO
HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C3-OBO,144,Standard,High Output,4000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C3-OBO
HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C4-OBO,144,Standard,Standard,3000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C4-OBO
HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C4-OBO,144,Standard,High Output,3000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C4-OBO
HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C4-OBO,144,Standard,Standard,3500K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C4-OBO
HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C4-OBO,144,Standard,High Output,3500K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C4-OBO
HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C4-OBO,144,Standard,Standard,4000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C4-OBO
HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C4-OBO,144,Standard,High Output,4000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C4-OBO
HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C4-OBO,144,Standard,Standard,3000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C4-OBO
HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C4-OBO,144,Standard,High Output,3000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C4-OBO
HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C4-OBO,144,Standard,Standard,3500K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C4-OBO
HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C4-OBO,144,Standard,High Output,3500K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C4-OBO
HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C4-OBO,144,Standard,Standard,4000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C4-OBO
HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C4-OBO,144,Standard,High Output,4000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C4-OBO
HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C1-OBD,48,Standard,Standard,3000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C1-OBD
HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C1-OBD,96,Standard,Standard,3000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C1-OBD
HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C1-OBD,48,Standard,High Output,3000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C1-OBD
HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C1-OBD,96,Standard,High Output,3000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C1-OBD
HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C1-OBD,48,Standard,Standard,3500K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C1-OBD
HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C1-OBD,96,Standard,Standard,3500K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C1-OBD
HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C1-OBD,48,Standard,High Output,3500K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C1-OBD
HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C1-OBD,96,Standard,High Output,3500K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C1-OBD
HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C1-OBD,48,Standard,Standard,4000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C1-OBD
HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C1-OBD,96,Standard,Standard,4000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C1-OBD
HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C1-OBD,48,Standard,High Output,4000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C1-OBD
HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C1-OBD,96,Standard,High Output,4000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C1-OBD
HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C1-OBD,48,Standard,Standard,3000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C1-OBD
HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C1-OBD,96,Standard,Standard,3000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C1-OBD
HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C1-OBD,48,Standard,High Output,3000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C1-OBD
HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C1-OBD,96,Standard,High Output,3000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C1-OBD
HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C1-OBD,48,Standard,Standard,3500K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C1-OBD
HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C1-OBD,96,Standard,Standard,3500K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C1-OBD
HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C1-OBD,48,Standard,High Output,3500K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C1-OBD
HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C1-OBD,96,Standard,High Output,3500K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C1-OBD
HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C1-OBD,48,Standard,Standard,4000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C1-OBD
HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C1-OBD,96,Standard,Standard,4000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C1-OBD
HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C1-OBD,48,Standard,High Output,4000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C1-OBD
HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C1-OBD,96,Standard,High Output,4000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C1-OBD
HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C2-OBD,48,Standard,Standard,3000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C2-OBD
HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C2-OBD,96,Standard,Standard,3000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C2-OBD
HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C2-OBD,48,Standard,High Output,3000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C2-OBD
HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C2-OBD,96,Standard,High Output,3000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C2-OBD
HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C2-OBD,48,Standard,Standard,3500K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C2-OBD
HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C2-OBD,96,Standard,Standard,3500K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C2-OBD
HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C2-OBD,48,Standard,High Output,3500K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C2-OBD
HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C2-OBD,96,Standard,High Output,3500K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C2-OBD
HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C2-OBD,48,Standard,Standard,4000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C2-OBD
HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C2-OBD,96,Standard,Standard,4000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C2-OBD
HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C2-OBD,48,Standard,High Output,4000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C2-OBD
HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C2-OBD,96,Standard,High Output,4000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C2-OBD
HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C2-OBD,48,Standard,Standard,3000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C2-OBD
HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C2-OBD,96,Standard,Standard,3000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C2-OBD
HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C2-OBD,48,Standard,High Output,3000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C2-OBD
HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C2-OBD,96,Standard,High Output,3000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C2-OBD
HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C2-OBD,48,Standard,Standard,3500K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C2-OBD
HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C2-OBD,96,Standard,Standard,3500K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C2-OBD
HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C2-OBD,48,Standard,High Output,3500K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C2-OBD
HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C2-OBD,96,Standard,High Output,3500K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C2-OBD
HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C2-OBD,48,Standard,Standard,4000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C2-OBD
HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C2-OBD,96,Standard,Standard,4000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C2-OBD
HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C2-OBD,48,Standard,High Output,4000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C2-OBD
HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C2-OBD,96,Standard,High Output,4000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C2-OBD
HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C3-OBD,48,Standard,Standard,3000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C3-OBD
HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C3-OBD,96,Standard,Standard,3000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C3-OBD
HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C3-OBD,48,Standard,High Output,3000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C3-OBD
HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C3-OBD,96,Standard,High Output,3000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C3-OBD
HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C3-OBD,48,Standard,Standard,3500K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C3-OBD
HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C3-OBD,96,Standard,Standard,3500K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C3-OBD
HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C3-OBD,48,Standard,High Output,3500K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C3-OBD
HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C3-OBD,96,Standard,High Output,3500K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C3-OBD
HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C3-OBD,48,Standard,Standard,4000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C3-OBD
HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C3-OBD,96,Standard,Standard,4000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C3-OBD
HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C3-OBD,48,Standard,High Output,4000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C3-OBD
HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C3-OBD,96,Standard,High Output,4000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C3-OBD
HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C3-OBD,48,Standard,Standard,3000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C3-OBD
HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C3-OBD,96,Standard,Standard,3000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C3-OBD
HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C3-OBD,48,Standard,High Output,3000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C3-OBD
HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C3-OBD,96,Standard,High Output,3000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C3-OBD
HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C3-OBD,48,Standard,Standard,3500K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C3-OBD
HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C3-OBD,96,Standard,Standard,3500K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C3-OBD
HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C3-OBD,48,Standard,High Output,3500K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C3-OBD
HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C3-OBD,96,Standard,High Output,3500K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C3-OBD
HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C3-OBD,48,Standard,Standard,4000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C3-OBD
HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C3-OBD,96,Standard,Standard,4000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C3-OBD
HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C3-OBD,48,Standard,High Output,4000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C3-OBD
HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C3-OBD,96,Standard,High Output,4000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C3-OBD
HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C4-OBD,48,Standard,Standard,3000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C4-OBD
HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C4-OBD,96,Standard,Standard,3000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C4-OBD
HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C4-OBD,48,Standard,High Output,3000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C4-OBD
HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C4-OBD,96,Standard,High Output,3000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C4-OBD
HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C4-OBD,48,Standard,Standard,3500K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C4-OBD
HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C4-OBD,96,Standard,Standard,3500K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C4-OBD
HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C4-OBD,48,Standard,High Output,3500K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C4-OBD
HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C4-OBD,96,Standard,High Output,3500K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C4-OBD
HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C4-OBD,48,Standard,Standard,4000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C4-OBD
HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C4-OBD,96,Standard,Standard,4000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C4-OBD
HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C4-OBD,48,Standard,High Output,4000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C4-OBD
HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C4-OBD,96,Standard,High Output,4000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C4-OBD
HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C4-OBD,48,Standard,Standard,3000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C4-OBD
HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C4-OBD,96,Standard,Standard,3000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C4-OBD
HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C4-OBD,48,Standard,High Output,3000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C4-OBD
HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C4-OBD,96,Standard,High Output,3000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C4-OBD
HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C4-OBD,48,Standard,Standard,3500K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C4-OBD
HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C4-OBD,96,Standard,Standard,3500K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C4-OBD
HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C4-OBD,48,Standard,High Output,3500K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C4-OBD
HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C4-OBD,96,Standard,High Output,3500K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C4-OBD
HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C4-OBD,48,Standard,Standard,4000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C4-OBD
HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C4-OBD,96,Standard,Standard,4000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C4-OBD
HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C4-OBD,48,Standard,High Output,4000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C4-OBD
HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C4-OBD,96,Standard,High Output,4000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C4-OBD
HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C1-OBD,144,Standard,Standard,3000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C1-OBD
HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C1-OBD,144,Standard,High Output,3000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C1-OBD
HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C1-OBD,144,Standard,Standard,3500K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C1-OBD
HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C1-OBD,144,Standard,High Output,3500K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C1-OBD
HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C1-OBD,144,Standard,Standard,4000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C1-OBD
HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C1-OBD,144,Standard,High Output,4000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C1-OBD
HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C1-OBD,144,Standard,Standard,3000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C1-OBD
HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C1-OBD,144,Standard,High Output,3000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C1-OBD
HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C1-OBD,144,Standard,Standard,3500K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C1-OBD
HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C1-OBD,144,Standard,High Output,3500K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C1-OBD
HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C1-OBD,144,Standard,Standard,4000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C1-OBD
HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C1-OBD,144,Standard,High Output,4000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C1-OBD
HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C2-OBD,144,Standard,Standard,3000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C2-OBD
HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C2-OBD,144,Standard,High Output,3000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C2-OBD
HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C2-OBD,144,Standard,Standard,3500K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C2-OBD
HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C2-OBD,144,Standard,High Output,3500K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C2-OBD
HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C2-OBD,144,Standard,Standard,4000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C2-OBD
HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C2-OBD,144,Standard,High Output,4000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C2-OBD
HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C2-OBD,144,Standard,Standard,3000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C2-OBD
HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C2-OBD,144,Standard,High Output,3000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C2-OBD
HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C2-OBD,144,Standard,Standard,3500K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C2-OBD
HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C2-OBD,144,Standard,High Output,3500K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C2-OBD
HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C2-OBD,144,Standard,Standard,4000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C2-OBD
HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C2-OBD,144,Standard,High Output,4000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C2-OBD
HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C3-OBD,144,Standard,Standard,3000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C3-OBD
HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C3-OBD,144,Standard,High Output,3000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C3-OBD
HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C3-OBD,144,Standard,Standard,3500K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C3-OBD
HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C3-OBD,144,Standard,High Output,3500K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C3-OBD
HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C3-OBD,144,Standard,Standard,4000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C3-OBD
HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C3-OBD,144,Standard,High Output,4000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C3-OBD
HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C3-OBD,144,Standard,Standard,3000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C3-OBD
HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C3-OBD,144,Standard,High Output,3000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C3-OBD
HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C3-OBD,144,Standard,Standard,3500K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C3-OBD
HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C3-OBD,144,Standard,High Output,3500K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C3-OBD
HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C3-OBD,144,Standard,Standard,4000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C3-OBD
HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C3-OBD,144,Standard,High Output,4000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C3-OBD
HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C4-OBD,144,Standard,Standard,3000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C4-OBD
HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C4-OBD,144,Standard,High Output,3000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C4-OBD
HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C4-OBD,144,Standard,Standard,3500K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C4-OBD
HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C4-OBD,144,Standard,High Output,3500K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C4-OBD
HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C4-OBD,144,Standard,Standard,4000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C4-OBD
HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C4-OBD,144,Standard,High Output,4000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C4-OBD
HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C4-OBD,144,Standard,Standard,3000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C4-OBD
HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C4-OBD,144,Standard,High Output,3000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C4-OBD
HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C4-OBD,144,Standard,Standard,3500K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C4-OBD
HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C4-OBD,144,Standard,High Output,3500K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C4-OBD
HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C4-OBD,144,Standard,Standard,4000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C4-OBD
HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C4-OBD,144,Standard,High Output,4000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C4-OBD
HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C1-OBB,48,Standard,Standard,3000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C1-OBB
HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C1-OBB,96,Standard,Standard,3000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C1-OBB
HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C1-OBB,48,Standard,High Output,3000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C1-OBB
HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C1-OBB,96,Standard,High Output,3000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C1-OBB
HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C1-OBB,48,Standard,Standard,3500K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C1-OBB
HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C1-OBB,96,Standard,Standard,3500K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C1-OBB
HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C1-OBB,48,Standard,High Output,3500K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C1-OBB
HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C1-OBB,96,Standard,High Output,3500K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C1-OBB
HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C1-OBB,48,Standard,Standard,4000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C1-OBB
HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C1-OBB,96,Standard,Standard,4000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C1-OBB
HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C1-OBB,48,Standard,High Output,4000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C1-OBB
HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C1-OBB,96,Standard,High Output,4000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C1-OBB
HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C1-OBB,48,Standard,Standard,3000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C1-OBB
HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C1-OBB,96,Standard,Standard,3000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C1-OBB
HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C1-OBB,48,Standard,High Output,3000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C1-OBB
HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C1-OBB,96,Standard,High Output,3000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C1-OBB
HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C1-OBB,48,Standard,Standard,3500K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C1-OBB
HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C1-OBB,96,Standard,Standard,3500K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C1-OBB
HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C1-OBB,48,Standard,High Output,3500K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C1-OBB
HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C1-OBB,96,Standard,High Output,3500K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C1-OBB
HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C1-OBB,48,Standard,Standard,4000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C1-OBB
HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C1-OBB,96,Standard,Standard,4000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C1-OBB
HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C1-OBB,48,Standard,High Output,4000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C1-OBB
HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C1-OBB,96,Standard,High Output,4000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C1-OBB
HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C2-OBB,48,Standard,Standard,3000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C2-OBB
HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C2-OBB,96,Standard,Standard,3000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C2-OBB
HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C2-OBB,48,Standard,High Output,3000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C2-OBB
HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C2-OBB,96,Standard,High Output,3000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C2-OBB
HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C2-OBB,48,Standard,Standard,3500K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C2-OBB
HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C2-OBB,96,Standard,Standard,3500K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C2-OBB
HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C2-OBB,48,Standard,High Output,3500K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C2-OBB
HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C2-OBB,96,Standard,High Output,3500K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C2-OBB
HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C2-OBB,48,Standard,Standard,4000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C2-OBB
HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C2-OBB,96,Standard,Standard,4000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C2-OBB
HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C2-OBB,48,Standard,High Output,4000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C2-OBB
HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C2-OBB,96,Standard,High Output,4000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C2-OBB
HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C2-OBB,48,Standard,Standard,3000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C2-OBB
HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C2-OBB,96,Standard,Standard,3000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C2-OBB
HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C2-OBB,48,Standard,High Output,3000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C2-OBB
HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C2-OBB,96,Standard,High Output,3000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C2-OBB
HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C2-OBB,48,Standard,Standard,3500K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C2-OBB
HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C2-OBB,96,Standard,Standard,3500K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C2-OBB
HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C2-OBB,48,Standard,High Output,3500K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C2-OBB
HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C2-OBB,96,Standard,High Output,3500K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C2-OBB
HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C2-OBB,48,Standard,Standard,4000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C2-OBB
HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C2-OBB,96,Standard,Standard,4000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C2-OBB
HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C2-OBB,48,Standard,High Output,4000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C2-OBB
HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C2-OBB,96,Standard,High Output,4000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C2-OBB
HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C3-OBB,48,Standard,Standard,3000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C3-OBB
HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C3-OBB,96,Standard,Standard,3000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C3-OBB
HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C3-OBB,48,Standard,High Output,3000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C3-OBB
HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C3-OBB,96,Standard,High Output,3000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C3-OBB
HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C3-OBB,48,Standard,Standard,3500K,120,Single Circuit,Slot Grid,Both,HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C3-OBB
HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C3-OBB,96,Standard,Standard,3500K,120,Single Circuit,Slot Grid,Both,HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C3-OBB
HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C3-OBB,48,Standard,High Output,3500K,120,Single Circuit,Slot Grid,Both,HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C3-OBB
HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C3-OBB,96,Standard,High Output,3500K,120,Single Circuit,Slot Grid,Both,HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C3-OBB
HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C3-OBB,48,Standard,Standard,4000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C3-OBB
HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C3-OBB,96,Standard,Standard,4000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C3-OBB
HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C3-OBB,48,Standard,High Output,4000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C3-OBB
HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C3-OBB,96,Standard,High Output,4000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C3-OBB
HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C3-OBB,48,Standard,Standard,3000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C3-OBB
HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C3-OBB,96,Standard,Standard,3000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C3-OBB
HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C3-OBB,48,Standard,High Output,3000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C3-OBB
HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C3-OBB,96,Standard,High Output,3000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C3-OBB
HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C3-OBB,48,Standard,Standard,3500K,277,Single Circuit,Slot Grid,Both,HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C3-OBB
HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C3-OBB,96,Standard,Standard,3500K,277,Single Circuit,Slot Grid,Both,HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C3-OBB
HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C3-OBB,48,Standard,High Output,3500K,277,Single Circuit,Slot Grid,Both,HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C3-OBB
HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C3-OBB,96,Standard,High Output,3500K,277,Single Circuit,Slot Grid,Both,HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C3-OBB
HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C3-OBB,48,Standard,Standard,4000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C3-OBB
HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C3-OBB,96,Standard,Standard,4000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C3-OBB
HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C3-OBB,48,Standard,High Output,4000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C3-OBB
HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C3-OBB,96,Standard,High Output,4000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C3-OBB
HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C4-OBB,48,Standard,Standard,3000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-SO-3000K-120-FA-SC-C4-OBB
HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C4-OBB,96,Standard,Standard,3000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-SO-3000K-120-FA-SC-C4-OBB
HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C4-OBB,48,Standard,High Output,3000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-HO-3000K-120-FA-SC-C4-OBB
HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C4-OBB,96,Standard,High Output,3000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-HO-3000K-120-FA-SC-C4-OBB
HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C4-OBB,48,Standard,Standard,3500K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-SO-3500K-120-FA-SC-C4-OBB
HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C4-OBB,96,Standard,Standard,3500K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-SO-3500K-120-FA-SC-C4-OBB
HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C4-OBB,48,Standard,High Output,3500K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-HO-3500K-120-FA-SC-C4-OBB
HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C4-OBB,96,Standard,High Output,3500K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-HO-3500K-120-FA-SC-C4-OBB
HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C4-OBB,48,Standard,Standard,4000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-SO-4000K-120-FA-SC-C4-OBB
HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C4-OBB,96,Standard,Standard,4000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-SO-4000K-120-FA-SC-C4-OBB
HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C4-OBB,48,Standard,High Output,4000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-HO-4000K-120-FA-SC-C4-OBB
HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C4-OBB,96,Standard,High Output,4000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-HO-4000K-120-FA-SC-C4-OBB
HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C4-OBB,48,Standard,Standard,3000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-SO-3000K-277-FA-SC-C4-OBB
HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C4-OBB,96,Standard,Standard,3000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-SO-3000K-277-FA-SC-C4-OBB
HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C4-OBB,48,Standard,High Output,3000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-HO-3000K-277-FA-SC-C4-OBB
HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C4-OBB,96,Standard,High Output,3000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-HO-3000K-277-FA-SC-C4-OBB
HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C4-OBB,48,Standard,Standard,3500K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-SO-3500K-277-FA-SC-C4-OBB
HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C4-OBB,96,Standard,Standard,3500K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-SO-3500K-277-FA-SC-C4-OBB
HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C4-OBB,48,Standard,High Output,3500K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-HO-3500K-277-FA-SC-C4-OBB
HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C4-OBB,96,Standard,High Output,3500K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-HO-3500K-277-FA-SC-C4-OBB
HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C4-OBB,48,Standard,Standard,4000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-SO-4000K-277-FA-SC-C4-OBB
HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C4-OBB,96,Standard,Standard,4000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-SO-4000K-277-FA-SC-C4-OBB
HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C4-OBB,48,Standard,High Output,4000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-HO-4000K-277-FA-SC-C4-OBB
HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C4-OBB,96,Standard,High Output,4000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-HO-4000K-277-FA-SC-C4-OBB
HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C1-OBB,144,Standard,Standard,3000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C1-OBB
HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C1-OBB,144,Standard,High Output,3000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C1-OBB
HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C1-OBB,144,Standard,Standard,3500K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C1-OBB
HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C1-OBB,144,Standard,High Output,3500K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C1-OBB
HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C1-OBB,144,Standard,Standard,4000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C1-OBB
HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C1-OBB,144,Standard,High Output,4000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C1-OBB
HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C1-OBB,144,Standard,Standard,3000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C1-OBB
HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C1-OBB,144,Standard,High Output,3000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C1-OBB
HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C1-OBB,144,Standard,Standard,3500K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C1-OBB
HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C1-OBB,144,Standard,High Output,3500K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C1-OBB
HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C1-OBB,144,Standard,Standard,4000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C1-OBB
HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C1-OBB,144,Standard,High Output,4000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C1-OBB
HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C2-OBB,144,Standard,Standard,3000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C2-OBB
HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C2-OBB,144,Standard,High Output,3000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C2-OBB
HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C2-OBB,144,Standard,Standard,3500K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C2-OBB
HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C2-OBB,144,Standard,High Output,3500K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C2-OBB
HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C2-OBB,144,Standard,Standard,4000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C2-OBB
HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C2-OBB,144,Standard,High Output,4000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C2-OBB
HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C2-OBB,144,Standard,Standard,3000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C2-OBB
HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C2-OBB,144,Standard,High Output,3000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C2-OBB
HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C2-OBB,144,Standard,Standard,3500K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C2-OBB
HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C2-OBB,144,Standard,High Output,3500K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C2-OBB
HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C2-OBB,144,Standard,Standard,4000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C2-OBB
HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C2-OBB,144,Standard,High Output,4000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C2-OBB
HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C3-OBB,144,Standard,Standard,3000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C3-OBB
HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C3-OBB,144,Standard,High Output,3000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C3-OBB
HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C3-OBB,144,Standard,Standard,3500K,120,Single Circuit,Slot Grid,Both,HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C3-OBB
HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C3-OBB,144,Standard,High Output,3500K,120,Single Circuit,Slot Grid,Both,HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C3-OBB
HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C3-OBB,144,Standard,Standard,4000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C3-OBB
HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C3-OBB,144,Standard,High Output,4000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C3-OBB
HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C3-OBB,144,Standard,Standard,3000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C3-OBB
HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C3-OBB,144,Standard,High Output,3000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C3-OBB
HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C3-OBB,144,Standard,Standard,3500K,277,Single Circuit,Slot Grid,Both,HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C3-OBB
HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C3-OBB,144,Standard,High Output,3500K,277,Single Circuit,Slot Grid,Both,HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C3-OBB
HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C3-OBB,144,Standard,Standard,4000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C3-OBB
HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C3-OBB,144,Standard,High Output,4000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C3-OBB
HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C4-OBB,144,Standard,Standard,3000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-SO-3000K-120-FA-SC-C4-OBB
HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C4-OBB,144,Standard,High Output,3000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-HO-3000K-120-FA-SC-C4-OBB
HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C4-OBB,144,Standard,Standard,3500K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-SO-3500K-120-FA-SC-C4-OBB
HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C4-OBB,144,Standard,High Output,3500K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-HO-3500K-120-FA-SC-C4-OBB
HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C4-OBB,144,Standard,Standard,4000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-SO-4000K-120-FA-SC-C4-OBB
HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C4-OBB,144,Standard,High Output,4000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-HO-4000K-120-FA-SC-C4-OBB
HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C4-OBB,144,Standard,Standard,3000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-SO-3000K-277-FA-SC-C4-OBB
HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C4-OBB,144,Standard,High Output,3000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-HO-3000K-277-FA-SC-C4-OBB
HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C4-OBB,144,Standard,Standard,3500K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-SO-3500K-277-FA-SC-C4-OBB
HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C4-OBB,144,Standard,High Output,3500K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-HO-3500K-277-FA-SC-C4-OBB
HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C4-OBB,144,Standard,Standard,4000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-SO-4000K-277-FA-SC-C4-OBB
HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C4-OBB,144,Standard,High Output,4000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-HO-4000K-277-FA-SC-C4-OBB
HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C1-OBO,48,High Output,Standard,3000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C1-OBO
HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C1-OBO,96,High Output,Standard,3000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C1-OBO
HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C1-OBO,48,High Output,High Output,3000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C1-OBO
HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C1-OBO,96,High Output,High Output,3000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C1-OBO
HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C1-OBO,48,High Output,Standard,3500K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C1-OBO
HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C1-OBO,96,High Output,Standard,3500K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C1-OBO
HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C1-OBO,48,High Output,High Output,3500K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C1-OBO
HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C1-OBO,96,High Output,High Output,3500K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C1-OBO
HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C1-OBO,48,High Output,Standard,4000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C1-OBO
HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C1-OBO,96,High Output,Standard,4000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C1-OBO
HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C1-OBO,48,High Output,High Output,4000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C1-OBO
HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C1-OBO,96,High Output,High Output,4000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C1-OBO
HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C1-OBO,48,High Output,Standard,3000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C1-OBO
HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C1-OBO,96,High Output,Standard,3000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C1-OBO
HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C1-OBO,48,High Output,High Output,3000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C1-OBO
HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C1-OBO,96,High Output,High Output,3000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C1-OBO
HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C1-OBO,48,High Output,Standard,3500K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C1-OBO
HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C1-OBO,96,High Output,Standard,3500K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C1-OBO
HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C1-OBO,48,High Output,High Output,3500K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C1-OBO
HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C1-OBO,96,High Output,High Output,3500K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C1-OBO
HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C1-OBO,48,High Output,Standard,4000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C1-OBO
HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C1-OBO,96,High Output,Standard,4000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C1-OBO
HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C1-OBO,48,High Output,High Output,4000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C1-OBO
HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C1-OBO,96,High Output,High Output,4000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C1-OBO
HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C2-OBO,48,High Output,Standard,3000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C2-OBO
HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C2-OBO,96,High Output,Standard,3000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C2-OBO
HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C2-OBO,48,High Output,High Output,3000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C2-OBO
HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C2-OBO,96,High Output,High Output,3000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C2-OBO
HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C2-OBO,48,High Output,Standard,3500K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C2-OBO
HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C2-OBO,96,High Output,Standard,3500K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C2-OBO
HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C2-OBO,48,High Output,High Output,3500K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C2-OBO
HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C2-OBO,96,High Output,High Output,3500K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C2-OBO
HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C2-OBO,48,High Output,Standard,4000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C2-OBO
HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C2-OBO,96,High Output,Standard,4000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C2-OBO
HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C2-OBO,48,High Output,High Output,4000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C2-OBO
HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C2-OBO,96,High Output,High Output,4000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C2-OBO
HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C2-OBO,48,High Output,Standard,3000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C2-OBO
HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C2-OBO,96,High Output,Standard,3000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C2-OBO
HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C2-OBO,48,High Output,High Output,3000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C2-OBO
HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C2-OBO,96,High Output,High Output,3000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C2-OBO
HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C2-OBO,48,High Output,Standard,3500K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C2-OBO
HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C2-OBO,96,High Output,Standard,3500K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C2-OBO
HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C2-OBO,48,High Output,High Output,3500K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C2-OBO
HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C2-OBO,96,High Output,High Output,3500K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C2-OBO
HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C2-OBO,48,High Output,Standard,4000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C2-OBO
HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C2-OBO,96,High Output,Standard,4000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C2-OBO
HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C2-OBO,48,High Output,High Output,4000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C2-OBO
HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C2-OBO,96,High Output,High Output,4000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C2-OBO
HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C3-OBO,48,High Output,Standard,3000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C3-OBO
HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C3-OBO,96,High Output,Standard,3000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C3-OBO
HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C3-OBO,48,High Output,High Output,3000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C3-OBO
HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C3-OBO,96,High Output,High Output,3000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C3-OBO
HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C3-OBO,48,High Output,Standard,3500K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C3-OBO
HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C3-OBO,96,High Output,Standard,3500K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C3-OBO
HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C3-OBO,48,High Output,High Output,3500K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C3-OBO
HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C3-OBO,96,High Output,High Output,3500K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C3-OBO
HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C3-OBO,48,High Output,Standard,4000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C3-OBO
HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C3-OBO,96,High Output,Standard,4000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C3-OBO
HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C3-OBO,48,High Output,High Output,4000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C3-OBO
HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C3-OBO,96,High Output,High Output,4000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C3-OBO
HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C3-OBO,48,High Output,Standard,3000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C3-OBO
HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C3-OBO,96,High Output,Standard,3000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C3-OBO
HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C3-OBO,48,High Output,High Output,3000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C3-OBO
HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C3-OBO,96,High Output,High Output,3000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C3-OBO
HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C3-OBO,48,High Output,Standard,3500K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C3-OBO
HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C3-OBO,96,High Output,Standard,3500K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C3-OBO
HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C3-OBO,48,High Output,High Output,3500K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C3-OBO
HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C3-OBO,96,High Output,High Output,3500K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C3-OBO
HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C3-OBO,48,High Output,Standard,4000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C3-OBO
HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C3-OBO,96,High Output,Standard,4000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C3-OBO
HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C3-OBO,48,High Output,High Output,4000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C3-OBO
HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C3-OBO,96,High Output,High Output,4000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C3-OBO
HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C4-OBO,48,High Output,Standard,3000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C4-OBO
HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C4-OBO,96,High Output,Standard,3000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C4-OBO
HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C4-OBO,48,High Output,High Output,3000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C4-OBO
HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C4-OBO,96,High Output,High Output,3000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C4-OBO
HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C4-OBO,48,High Output,Standard,3500K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C4-OBO
HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C4-OBO,96,High Output,Standard,3500K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C4-OBO
HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C4-OBO,48,High Output,High Output,3500K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C4-OBO
HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C4-OBO,96,High Output,High Output,3500K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C4-OBO
HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C4-OBO,48,High Output,Standard,4000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C4-OBO
HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C4-OBO,96,High Output,Standard,4000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C4-OBO
HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C4-OBO,48,High Output,High Output,4000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C4-OBO
HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C4-OBO,96,High Output,High Output,4000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C4-OBO
HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C4-OBO,48,High Output,Standard,3000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C4-OBO
HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C4-OBO,96,High Output,Standard,3000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C4-OBO
HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C4-OBO,48,High Output,High Output,3000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C4-OBO
HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C4-OBO,96,High Output,High Output,3000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C4-OBO
HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C4-OBO,48,High Output,Standard,3500K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C4-OBO
HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C4-OBO,96,High Output,Standard,3500K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C4-OBO
HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C4-OBO,48,High Output,High Output,3500K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C4-OBO
HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C4-OBO,96,High Output,High Output,3500K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C4-OBO
HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C4-OBO,48,High Output,Standard,4000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C4-OBO
HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C4-OBO,96,High Output,Standard,4000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C4-OBO
HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C4-OBO,48,High Output,High Output,4000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C4-OBO
HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C4-OBO,96,High Output,High Output,4000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C4-OBO
HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C1-OBO,144,High Output,Standard,3000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C1-OBO
HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C1-OBO,144,High Output,High Output,3000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C1-OBO
HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C1-OBO,144,High Output,Standard,3500K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C1-OBO
HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C1-OBO,144,High Output,High Output,3500K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C1-OBO
HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C1-OBO,144,High Output,Standard,4000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C1-OBO
HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C1-OBO,144,High Output,High Output,4000K,120,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C1-OBO
HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C1-OBO,144,High Output,Standard,3000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C1-OBO
HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C1-OBO,144,High Output,High Output,3000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C1-OBO
HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C1-OBO,144,High Output,Standard,3500K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C1-OBO
HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C1-OBO,144,High Output,High Output,3500K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C1-OBO
HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C1-OBO,144,High Output,Standard,4000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C1-OBO
HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C1-OBO,144,High Output,High Output,4000K,277,Single Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C1-OBO
HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C2-OBO,144,High Output,Standard,3000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C2-OBO
HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C2-OBO,144,High Output,High Output,3000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C2-OBO
HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C2-OBO,144,High Output,Standard,3500K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C2-OBO
HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C2-OBO,144,High Output,High Output,3500K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C2-OBO
HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C2-OBO,144,High Output,Standard,4000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C2-OBO
HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C2-OBO,144,High Output,High Output,4000K,120,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C2-OBO
HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C2-OBO,144,High Output,Standard,3000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C2-OBO
HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C2-OBO,144,High Output,High Output,3000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C2-OBO
HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C2-OBO,144,High Output,Standard,3500K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C2-OBO
HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C2-OBO,144,High Output,High Output,3500K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C2-OBO
HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C2-OBO,144,High Output,Standard,4000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C2-OBO
HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C2-OBO,144,High Output,High Output,4000K,277,Single Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C2-OBO
HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C3-OBO,144,High Output,Standard,3000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C3-OBO
HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C3-OBO,144,High Output,High Output,3000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C3-OBO
HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C3-OBO,144,High Output,Standard,3500K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C3-OBO
HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C3-OBO,144,High Output,High Output,3500K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C3-OBO
HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C3-OBO,144,High Output,Standard,4000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C3-OBO
HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C3-OBO,144,High Output,High Output,4000K,120,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C3-OBO
HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C3-OBO,144,High Output,Standard,3000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C3-OBO
HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C3-OBO,144,High Output,High Output,3000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C3-OBO
HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C3-OBO,144,High Output,Standard,3500K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C3-OBO
HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C3-OBO,144,High Output,High Output,3500K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C3-OBO
HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C3-OBO,144,High Output,Standard,4000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C3-OBO
HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C3-OBO,144,High Output,High Output,4000K,277,Single Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C3-OBO
HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C4-OBO,144,High Output,Standard,3000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C4-OBO
HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C4-OBO,144,High Output,High Output,3000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C4-OBO
HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C4-OBO,144,High Output,Standard,3500K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C4-OBO
HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C4-OBO,144,High Output,High Output,3500K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C4-OBO
HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C4-OBO,144,High Output,Standard,4000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C4-OBO
HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C4-OBO,144,High Output,High Output,4000K,120,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C4-OBO
HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C4-OBO,144,High Output,Standard,3000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C4-OBO
HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C4-OBO,144,High Output,High Output,3000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C4-OBO
HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C4-OBO,144,High Output,Standard,3500K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C4-OBO
HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C4-OBO,144,High Output,High Output,3500K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C4-OBO
HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C4-OBO,144,High Output,Standard,4000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C4-OBO
HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C4-OBO,144,High Output,High Output,4000K,277,Single Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C4-OBO
HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C1-OBD,48,High Output,Standard,3000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C1-OBD
HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C1-OBD,96,High Output,Standard,3000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C1-OBD
HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C1-OBD,48,High Output,High Output,3000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C1-OBD
HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C1-OBD,96,High Output,High Output,3000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C1-OBD
HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C1-OBD,48,High Output,Standard,3500K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C1-OBD
HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C1-OBD,96,High Output,Standard,3500K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C1-OBD
HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C1-OBD,48,High Output,High Output,3500K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C1-OBD
HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C1-OBD,96,High Output,High Output,3500K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C1-OBD
HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C1-OBD,48,High Output,Standard,4000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C1-OBD
HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C1-OBD,96,High Output,Standard,4000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C1-OBD
HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C1-OBD,48,High Output,High Output,4000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C1-OBD
HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C1-OBD,96,High Output,High Output,4000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C1-OBD
HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C1-OBD,48,High Output,Standard,3000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C1-OBD
HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C1-OBD,96,High Output,Standard,3000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C1-OBD
HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C1-OBD,48,High Output,High Output,3000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C1-OBD
HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C1-OBD,96,High Output,High Output,3000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C1-OBD
HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C1-OBD,48,High Output,Standard,3500K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C1-OBD
HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C1-OBD,96,High Output,Standard,3500K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C1-OBD
HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C1-OBD,48,High Output,High Output,3500K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C1-OBD
HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C1-OBD,96,High Output,High Output,3500K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C1-OBD
HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C1-OBD,48,High Output,Standard,4000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C1-OBD
HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C1-OBD,96,High Output,Standard,4000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C1-OBD
HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C1-OBD,48,High Output,High Output,4000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C1-OBD
HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C1-OBD,96,High Output,High Output,4000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C1-OBD
HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C2-OBD,48,High Output,Standard,3000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C2-OBD
HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C2-OBD,96,High Output,Standard,3000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C2-OBD
HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C2-OBD,48,High Output,High Output,3000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C2-OBD
HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C2-OBD,96,High Output,High Output,3000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C2-OBD
HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C2-OBD,48,High Output,Standard,3500K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C2-OBD
HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C2-OBD,96,High Output,Standard,3500K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C2-OBD
HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C2-OBD,48,High Output,High Output,3500K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C2-OBD
HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C2-OBD,96,High Output,High Output,3500K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C2-OBD
HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C2-OBD,48,High Output,Standard,4000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C2-OBD
HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C2-OBD,96,High Output,Standard,4000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C2-OBD
HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C2-OBD,48,High Output,High Output,4000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C2-OBD
HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C2-OBD,96,High Output,High Output,4000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C2-OBD
HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C2-OBD,48,High Output,Standard,3000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C2-OBD
HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C2-OBD,96,High Output,Standard,3000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C2-OBD
HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C2-OBD,48,High Output,High Output,3000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C2-OBD
HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C2-OBD,96,High Output,High Output,3000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C2-OBD
HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C2-OBD,48,High Output,Standard,3500K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C2-OBD
HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C2-OBD,96,High Output,Standard,3500K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C2-OBD
HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C2-OBD,48,High Output,High Output,3500K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C2-OBD
HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C2-OBD,96,High Output,High Output,3500K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C2-OBD
HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C2-OBD,48,High Output,Standard,4000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C2-OBD
HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C2-OBD,96,High Output,Standard,4000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C2-OBD
HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C2-OBD,48,High Output,High Output,4000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C2-OBD
HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C2-OBD,96,High Output,High Output,4000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C2-OBD
HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C3-OBD,48,High Output,Standard,3000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C3-OBD
HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C3-OBD,96,High Output,Standard,3000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C3-OBD
HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C3-OBD,48,High Output,High Output,3000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C3-OBD
HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C3-OBD,96,High Output,High Output,3000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C3-OBD
HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C3-OBD,48,High Output,Standard,3500K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C3-OBD
HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C3-OBD,96,High Output,Standard,3500K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C3-OBD
HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C3-OBD,48,High Output,High Output,3500K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C3-OBD
HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C3-OBD,96,High Output,High Output,3500K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C3-OBD
HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C3-OBD,48,High Output,Standard,4000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C3-OBD
HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C3-OBD,96,High Output,Standard,4000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C3-OBD
HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C3-OBD,48,High Output,High Output,4000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C3-OBD
HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C3-OBD,96,High Output,High Output,4000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C3-OBD
HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C3-OBD,48,High Output,Standard,3000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C3-OBD
HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C3-OBD,96,High Output,Standard,3000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C3-OBD
HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C3-OBD,48,High Output,High Output,3000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C3-OBD
HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C3-OBD,96,High Output,High Output,3000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C3-OBD
HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C3-OBD,48,High Output,Standard,3500K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C3-OBD
HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C3-OBD,96,High Output,Standard,3500K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C3-OBD
HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C3-OBD,48,High Output,High Output,3500K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C3-OBD
HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C3-OBD,96,High Output,High Output,3500K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C3-OBD
HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C3-OBD,48,High Output,Standard,4000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C3-OBD
HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C3-OBD,96,High Output,Standard,4000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C3-OBD
HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C3-OBD,48,High Output,High Output,4000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C3-OBD
HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C3-OBD,96,High Output,High Output,4000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C3-OBD
HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C4-OBD,48,High Output,Standard,3000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C4-OBD
HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C4-OBD,96,High Output,Standard,3000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C4-OBD
HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C4-OBD,48,High Output,High Output,3000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C4-OBD
HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C4-OBD,96,High Output,High Output,3000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C4-OBD
HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C4-OBD,48,High Output,Standard,3500K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C4-OBD
HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C4-OBD,96,High Output,Standard,3500K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C4-OBD
HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C4-OBD,48,High Output,High Output,3500K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C4-OBD
HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C4-OBD,96,High Output,High Output,3500K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C4-OBD
HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C4-OBD,48,High Output,Standard,4000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C4-OBD
HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C4-OBD,96,High Output,Standard,4000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C4-OBD
HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C4-OBD,48,High Output,High Output,4000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C4-OBD
HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C4-OBD,96,High Output,High Output,4000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C4-OBD
HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C4-OBD,48,High Output,Standard,3000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C4-OBD
HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C4-OBD,96,High Output,Standard,3000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C4-OBD
HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C4-OBD,48,High Output,High Output,3000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C4-OBD
HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C4-OBD,96,High Output,High Output,3000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C4-OBD
HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C4-OBD,48,High Output,Standard,3500K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C4-OBD
HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C4-OBD,96,High Output,Standard,3500K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C4-OBD
HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C4-OBD,48,High Output,High Output,3500K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C4-OBD
HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C4-OBD,96,High Output,High Output,3500K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C4-OBD
HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C4-OBD,48,High Output,Standard,4000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C4-OBD
HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C4-OBD,96,High Output,Standard,4000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C4-OBD
HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C4-OBD,48,High Output,High Output,4000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C4-OBD
HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C4-OBD,96,High Output,High Output,4000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C4-OBD
HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C1-OBD,144,High Output,Standard,3000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C1-OBD
HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C1-OBD,144,High Output,High Output,3000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C1-OBD
HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C1-OBD,144,High Output,Standard,3500K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C1-OBD
HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C1-OBD,144,High Output,High Output,3500K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C1-OBD
HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C1-OBD,144,High Output,Standard,4000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C1-OBD
HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C1-OBD,144,High Output,High Output,4000K,120,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C1-OBD
HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C1-OBD,144,High Output,Standard,3000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C1-OBD
HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C1-OBD,144,High Output,High Output,3000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C1-OBD
HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C1-OBD,144,High Output,Standard,3500K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C1-OBD
HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C1-OBD,144,High Output,High Output,3500K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C1-OBD
HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C1-OBD,144,High Output,Standard,4000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C1-OBD
HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C1-OBD,144,High Output,High Output,4000K,277,Single Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C1-OBD
HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C2-OBD,144,High Output,Standard,3000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C2-OBD
HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C2-OBD,144,High Output,High Output,3000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C2-OBD
HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C2-OBD,144,High Output,Standard,3500K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C2-OBD
HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C2-OBD,144,High Output,High Output,3500K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C2-OBD
HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C2-OBD,144,High Output,Standard,4000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C2-OBD
HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C2-OBD,144,High Output,High Output,4000K,120,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C2-OBD
HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C2-OBD,144,High Output,Standard,3000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C2-OBD
HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C2-OBD,144,High Output,High Output,3000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C2-OBD
HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C2-OBD,144,High Output,Standard,3500K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C2-OBD
HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C2-OBD,144,High Output,High Output,3500K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C2-OBD
HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C2-OBD,144,High Output,Standard,4000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C2-OBD
HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C2-OBD,144,High Output,High Output,4000K,277,Single Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C2-OBD
HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C3-OBD,144,High Output,Standard,3000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C3-OBD
HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C3-OBD,144,High Output,High Output,3000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C3-OBD
HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C3-OBD,144,High Output,Standard,3500K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C3-OBD
HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C3-OBD,144,High Output,High Output,3500K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C3-OBD
HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C3-OBD,144,High Output,Standard,4000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C3-OBD
HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C3-OBD,144,High Output,High Output,4000K,120,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C3-OBD
HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C3-OBD,144,High Output,Standard,3000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C3-OBD
HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C3-OBD,144,High Output,High Output,3000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C3-OBD
HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C3-OBD,144,High Output,Standard,3500K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C3-OBD
HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C3-OBD,144,High Output,High Output,3500K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C3-OBD
HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C3-OBD,144,High Output,Standard,4000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C3-OBD
HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C3-OBD,144,High Output,High Output,4000K,277,Single Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C3-OBD
HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C4-OBD,144,High Output,Standard,3000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C4-OBD
HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C4-OBD,144,High Output,High Output,3000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C4-OBD
HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C4-OBD,144,High Output,Standard,3500K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C4-OBD
HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C4-OBD,144,High Output,High Output,3500K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C4-OBD
HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C4-OBD,144,High Output,Standard,4000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C4-OBD
HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C4-OBD,144,High Output,High Output,4000K,120,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C4-OBD
HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C4-OBD,144,High Output,Standard,3000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C4-OBD
HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C4-OBD,144,High Output,High Output,3000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C4-OBD
HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C4-OBD,144,High Output,Standard,3500K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C4-OBD
HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C4-OBD,144,High Output,High Output,3500K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C4-OBD
HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C4-OBD,144,High Output,Standard,4000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C4-OBD
HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C4-OBD,144,High Output,High Output,4000K,277,Single Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C4-OBD
HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C1-OBB,48,High Output,Standard,3000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C1-OBB
HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C1-OBB,96,High Output,Standard,3000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C1-OBB
HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C1-OBB,48,High Output,High Output,3000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C1-OBB
HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C1-OBB,96,High Output,High Output,3000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C1-OBB
HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C1-OBB,48,High Output,Standard,3500K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C1-OBB
HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C1-OBB,96,High Output,Standard,3500K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C1-OBB
HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C1-OBB,48,High Output,High Output,3500K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C1-OBB
HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C1-OBB,96,High Output,High Output,3500K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C1-OBB
HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C1-OBB,48,High Output,Standard,4000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C1-OBB
HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C1-OBB,96,High Output,Standard,4000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C1-OBB
HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C1-OBB,48,High Output,High Output,4000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C1-OBB
HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C1-OBB,96,High Output,High Output,4000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C1-OBB
HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C1-OBB,48,High Output,Standard,3000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C1-OBB
HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C1-OBB,96,High Output,Standard,3000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C1-OBB
HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C1-OBB,48,High Output,High Output,3000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C1-OBB
HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C1-OBB,96,High Output,High Output,3000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C1-OBB
HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C1-OBB,48,High Output,Standard,3500K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C1-OBB
HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C1-OBB,96,High Output,Standard,3500K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C1-OBB
HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C1-OBB,48,High Output,High Output,3500K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C1-OBB
HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C1-OBB,96,High Output,High Output,3500K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C1-OBB
HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C1-OBB,48,High Output,Standard,4000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C1-OBB
HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C1-OBB,96,High Output,Standard,4000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C1-OBB
HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C1-OBB,48,High Output,High Output,4000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C1-OBB
HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C1-OBB,96,High Output,High Output,4000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C1-OBB
HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C2-OBB,48,High Output,Standard,3000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C2-OBB
HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C2-OBB,96,High Output,Standard,3000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C2-OBB
HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C2-OBB,48,High Output,High Output,3000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C2-OBB
HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C2-OBB,96,High Output,High Output,3000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C2-OBB
HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C2-OBB,48,High Output,Standard,3500K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C2-OBB
HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C2-OBB,96,High Output,Standard,3500K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C2-OBB
HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C2-OBB,48,High Output,High Output,3500K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C2-OBB
HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C2-OBB,96,High Output,High Output,3500K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C2-OBB
HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C2-OBB,48,High Output,Standard,4000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C2-OBB
HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C2-OBB,96,High Output,Standard,4000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C2-OBB
HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C2-OBB,48,High Output,High Output,4000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C2-OBB
HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C2-OBB,96,High Output,High Output,4000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C2-OBB
HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C2-OBB,48,High Output,Standard,3000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C2-OBB
HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C2-OBB,96,High Output,Standard,3000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C2-OBB
HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C2-OBB,48,High Output,High Output,3000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C2-OBB
HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C2-OBB,96,High Output,High Output,3000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C2-OBB
HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C2-OBB,48,High Output,Standard,3500K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C2-OBB
HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C2-OBB,96,High Output,Standard,3500K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C2-OBB
HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C2-OBB,48,High Output,High Output,3500K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C2-OBB
HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C2-OBB,96,High Output,High Output,3500K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C2-OBB
HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C2-OBB,48,High Output,Standard,4000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C2-OBB
HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C2-OBB,96,High Output,Standard,4000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C2-OBB
HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C2-OBB,48,High Output,High Output,4000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C2-OBB
HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C2-OBB,96,High Output,High Output,4000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C2-OBB
HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C3-OBB,48,High Output,Standard,3000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C3-OBB
HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C3-OBB,96,High Output,Standard,3000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C3-OBB
HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C3-OBB,48,High Output,High Output,3000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C3-OBB
HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C3-OBB,96,High Output,High Output,3000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C3-OBB
HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C3-OBB,48,High Output,Standard,3500K,120,Single Circuit,Slot Grid,Both,HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C3-OBB
HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C3-OBB,96,High Output,Standard,3500K,120,Single Circuit,Slot Grid,Both,HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C3-OBB
HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C3-OBB,48,High Output,High Output,3500K,120,Single Circuit,Slot Grid,Both,HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C3-OBB
HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C3-OBB,96,High Output,High Output,3500K,120,Single Circuit,Slot Grid,Both,HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C3-OBB
HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C3-OBB,48,High Output,Standard,4000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C3-OBB
HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C3-OBB,96,High Output,Standard,4000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C3-OBB
HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C3-OBB,48,High Output,High Output,4000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C3-OBB
HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C3-OBB,96,High Output,High Output,4000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C3-OBB
HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C3-OBB,48,High Output,Standard,3000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C3-OBB
HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C3-OBB,96,High Output,Standard,3000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C3-OBB
HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C3-OBB,48,High Output,High Output,3000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C3-OBB
HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C3-OBB,96,High Output,High Output,3000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C3-OBB
HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C3-OBB,48,High Output,Standard,3500K,277,Single Circuit,Slot Grid,Both,HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C3-OBB
HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C3-OBB,96,High Output,Standard,3500K,277,Single Circuit,Slot Grid,Both,HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C3-OBB
HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C3-OBB,48,High Output,High Output,3500K,277,Single Circuit,Slot Grid,Both,HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C3-OBB
HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C3-OBB,96,High Output,High Output,3500K,277,Single Circuit,Slot Grid,Both,HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C3-OBB
HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C3-OBB,48,High Output,Standard,4000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C3-OBB
HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C3-OBB,96,High Output,Standard,4000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C3-OBB
HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C3-OBB,48,High Output,High Output,4000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C3-OBB
HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C3-OBB,96,High Output,High Output,4000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C3-OBB
HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C4-OBB,48,High Output,Standard,3000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-SO-3000K-120-FA-SC-C4-OBB
HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C4-OBB,96,High Output,Standard,3000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-SO-3000K-120-FA-SC-C4-OBB
HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C4-OBB,48,High Output,High Output,3000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-HO-3000K-120-FA-SC-C4-OBB
HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C4-OBB,96,High Output,High Output,3000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-HO-3000K-120-FA-SC-C4-OBB
HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C4-OBB,48,High Output,Standard,3500K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-SO-3500K-120-FA-SC-C4-OBB
HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C4-OBB,96,High Output,Standard,3500K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-SO-3500K-120-FA-SC-C4-OBB
HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C4-OBB,48,High Output,High Output,3500K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-HO-3500K-120-FA-SC-C4-OBB
HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C4-OBB,96,High Output,High Output,3500K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-HO-3500K-120-FA-SC-C4-OBB
HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C4-OBB,48,High Output,Standard,4000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-SO-4000K-120-FA-SC-C4-OBB
HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C4-OBB,96,High Output,Standard,4000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-SO-4000K-120-FA-SC-C4-OBB
HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C4-OBB,48,High Output,High Output,4000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-HO-4000K-120-FA-SC-C4-OBB
HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C4-OBB,96,High Output,High Output,4000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-HO-4000K-120-FA-SC-C4-OBB
HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C4-OBB,48,High Output,Standard,3000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-SO-3000K-277-FA-SC-C4-OBB
HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C4-OBB,96,High Output,Standard,3000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-SO-3000K-277-FA-SC-C4-OBB
HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C4-OBB,48,High Output,High Output,3000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-HO-3000K-277-FA-SC-C4-OBB
HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C4-OBB,96,High Output,High Output,3000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-HO-3000K-277-FA-SC-C4-OBB
HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C4-OBB,48,High Output,Standard,3500K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-SO-3500K-277-FA-SC-C4-OBB
HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C4-OBB,96,High Output,Standard,3500K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-SO-3500K-277-FA-SC-C4-OBB
HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C4-OBB,48,High Output,High Output,3500K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-HO-3500K-277-FA-SC-C4-OBB
HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C4-OBB,96,High Output,High Output,3500K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-HO-3500K-277-FA-SC-C4-OBB
HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C4-OBB,48,High Output,Standard,4000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-SO-4000K-277-FA-SC-C4-OBB
HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C4-OBB,96,High Output,Standard,4000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-SO-4000K-277-FA-SC-C4-OBB
HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C4-OBB,48,High Output,High Output,4000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-HO-4000K-277-FA-SC-C4-OBB
HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C4-OBB,96,High Output,High Output,4000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-HO-4000K-277-FA-SC-C4-OBB
HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C1-OBB,144,High Output,Standard,3000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C1-OBB
HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C1-OBB,144,High Output,High Output,3000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C1-OBB
HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C1-OBB,144,High Output,Standard,3500K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C1-OBB
HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C1-OBB,144,High Output,High Output,3500K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C1-OBB
HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C1-OBB,144,High Output,Standard,4000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C1-OBB
HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C1-OBB,144,High Output,High Output,4000K,120,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C1-OBB
HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C1-OBB,144,High Output,Standard,3000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C1-OBB
HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C1-OBB,144,High Output,High Output,3000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C1-OBB
HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C1-OBB,144,High Output,Standard,3500K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C1-OBB
HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C1-OBB,144,High Output,High Output,3500K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C1-OBB
HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C1-OBB,144,High Output,Standard,4000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C1-OBB
HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C1-OBB,144,High Output,High Output,4000K,277,Single Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C1-OBB
HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C2-OBB,144,High Output,Standard,3000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C2-OBB
HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C2-OBB,144,High Output,High Output,3000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C2-OBB
HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C2-OBB,144,High Output,Standard,3500K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C2-OBB
HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C2-OBB,144,High Output,High Output,3500K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C2-OBB
HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C2-OBB,144,High Output,Standard,4000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C2-OBB
HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C2-OBB,144,High Output,High Output,4000K,120,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C2-OBB
HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C2-OBB,144,High Output,Standard,3000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C2-OBB
HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C2-OBB,144,High Output,High Output,3000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C2-OBB
HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C2-OBB,144,High Output,Standard,3500K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C2-OBB
HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C2-OBB,144,High Output,High Output,3500K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C2-OBB
HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C2-OBB,144,High Output,Standard,4000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C2-OBB
HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C2-OBB,144,High Output,High Output,4000K,277,Single Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C2-OBB
HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C3-OBB,144,High Output,Standard,3000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C3-OBB
HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C3-OBB,144,High Output,High Output,3000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C3-OBB
HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C3-OBB,144,High Output,Standard,3500K,120,Single Circuit,Slot Grid,Both,HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C3-OBB
HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C3-OBB,144,High Output,High Output,3500K,120,Single Circuit,Slot Grid,Both,HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C3-OBB
HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C3-OBB,144,High Output,Standard,4000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C3-OBB
HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C3-OBB,144,High Output,High Output,4000K,120,Single Circuit,Slot Grid,Both,HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C3-OBB
HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C3-OBB,144,High Output,Standard,3000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C3-OBB
HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C3-OBB,144,High Output,High Output,3000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C3-OBB
HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C3-OBB,144,High Output,Standard,3500K,277,Single Circuit,Slot Grid,Both,HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C3-OBB
HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C3-OBB,144,High Output,High Output,3500K,277,Single Circuit,Slot Grid,Both,HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C3-OBB
HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C3-OBB,144,High Output,Standard,4000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C3-OBB
HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C3-OBB,144,High Output,High Output,4000K,277,Single Circuit,Slot Grid,Both,HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C3-OBB
HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C4-OBB,144,High Output,Standard,3000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-SO-3000K-120-FA-SC-C4-OBB
HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C4-OBB,144,High Output,High Output,3000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-HO-3000K-120-FA-SC-C4-OBB
HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C4-OBB,144,High Output,Standard,3500K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-SO-3500K-120-FA-SC-C4-OBB
HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C4-OBB,144,High Output,High Output,3500K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-HO-3500K-120-FA-SC-C4-OBB
HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C4-OBB,144,High Output,Standard,4000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-SO-4000K-120-FA-SC-C4-OBB
HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C4-OBB,144,High Output,High Output,4000K,120,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-HO-4000K-120-FA-SC-C4-OBB
HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C4-OBB,144,High Output,Standard,3000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-SO-3000K-277-FA-SC-C4-OBB
HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C4-OBB,144,High Output,High Output,3000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-HO-3000K-277-FA-SC-C4-OBB
HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C4-OBB,144,High Output,Standard,3500K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-SO-3500K-277-FA-SC-C4-OBB
HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C4-OBB,144,High Output,High Output,3500K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-HO-3500K-277-FA-SC-C4-OBB
HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C4-OBB,144,High Output,Standard,4000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-SO-4000K-277-FA-SC-C4-OBB
HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C4-OBB,144,High Output,High Output,4000K,277,Single Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-HO-4000K-277-FA-SC-C4-OBB
HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C1-OBO,48,Standard,Standard,3000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C1-OBO
HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C1-OBO,96,Standard,Standard,3000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C1-OBO
HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C1-OBO,48,Standard,High Output,3000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C1-OBO
HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C1-OBO,96,Standard,High Output,3000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C1-OBO
HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C1-OBO,48,Standard,Standard,3500K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C1-OBO
HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C1-OBO,96,Standard,Standard,3500K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C1-OBO
HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C1-OBO,48,Standard,High Output,3500K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C1-OBO
HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C1-OBO,96,Standard,High Output,3500K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C1-OBO
HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C1-OBO,48,Standard,Standard,4000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C1-OBO
HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C1-OBO,96,Standard,Standard,4000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C1-OBO
HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C1-OBO,48,Standard,High Output,4000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C1-OBO
HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C1-OBO,96,Standard,High Output,4000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C1-OBO
HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C1-OBO,48,Standard,Standard,3000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C1-OBO
HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C1-OBO,96,Standard,Standard,3000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C1-OBO
HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C1-OBO,48,Standard,High Output,3000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C1-OBO
HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C1-OBO,96,Standard,High Output,3000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C1-OBO
HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C1-OBO,48,Standard,Standard,3500K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C1-OBO
HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C1-OBO,96,Standard,Standard,3500K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C1-OBO
HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C1-OBO,48,Standard,High Output,3500K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C1-OBO
HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C1-OBO,96,Standard,High Output,3500K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C1-OBO
HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C1-OBO,48,Standard,Standard,4000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C1-OBO
HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C1-OBO,96,Standard,Standard,4000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C1-OBO
HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C1-OBO,48,Standard,High Output,4000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C1-OBO
HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C1-OBO,96,Standard,High Output,4000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C1-OBO
HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C2-OBO,48,Standard,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C2-OBO
HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C2-OBO,96,Standard,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C2-OBO
HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C2-OBO,48,Standard,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C2-OBO
HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C2-OBO,96,Standard,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C2-OBO
HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C2-OBO,48,Standard,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C2-OBO
HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C2-OBO,96,Standard,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C2-OBO
HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C2-OBO,48,Standard,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C2-OBO
HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C2-OBO,96,Standard,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C2-OBO
HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C2-OBO,48,Standard,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C2-OBO
HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C2-OBO,96,Standard,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C2-OBO
HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C2-OBO,48,Standard,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C2-OBO
HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C2-OBO,96,Standard,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C2-OBO
HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C2-OBO,48,Standard,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C2-OBO
HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C2-OBO,96,Standard,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C2-OBO
HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C2-OBO,48,Standard,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C2-OBO
HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C2-OBO,96,Standard,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C2-OBO
HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C2-OBO,48,Standard,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C2-OBO
HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C2-OBO,96,Standard,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C2-OBO
HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C2-OBO,48,Standard,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C2-OBO
HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C2-OBO,96,Standard,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C2-OBO
HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C2-OBO,48,Standard,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C2-OBO
HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C2-OBO,96,Standard,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C2-OBO
HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C2-OBO,48,Standard,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C2-OBO
HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C2-OBO,96,Standard,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C2-OBO
HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C3-OBO,48,Standard,Standard,3000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C3-OBO
HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C3-OBO,96,Standard,Standard,3000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C3-OBO
HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C3-OBO,48,Standard,High Output,3000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C3-OBO
HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C3-OBO,96,Standard,High Output,3000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C3-OBO
HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C3-OBO,48,Standard,Standard,3500K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C3-OBO
HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C3-OBO,96,Standard,Standard,3500K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C3-OBO
HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C3-OBO,48,Standard,High Output,3500K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C3-OBO
HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C3-OBO,96,Standard,High Output,3500K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C3-OBO
HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C3-OBO,48,Standard,Standard,4000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C3-OBO
HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C3-OBO,96,Standard,Standard,4000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C3-OBO
HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C3-OBO,48,Standard,High Output,4000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C3-OBO
HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C3-OBO,96,Standard,High Output,4000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C3-OBO
HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C3-OBO,48,Standard,Standard,3000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C3-OBO
HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C3-OBO,96,Standard,Standard,3000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C3-OBO
HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C3-OBO,48,Standard,High Output,3000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C3-OBO
HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C3-OBO,96,Standard,High Output,3000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C3-OBO
HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C3-OBO,48,Standard,Standard,3500K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C3-OBO
HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C3-OBO,96,Standard,Standard,3500K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C3-OBO
HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C3-OBO,48,Standard,High Output,3500K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C3-OBO
HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C3-OBO,96,Standard,High Output,3500K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C3-OBO
HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C3-OBO,48,Standard,Standard,4000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C3-OBO
HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C3-OBO,96,Standard,Standard,4000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C3-OBO
HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C3-OBO,48,Standard,High Output,4000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C3-OBO
HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C3-OBO,96,Standard,High Output,4000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C3-OBO
HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C4-OBO,48,Standard,Standard,3000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C4-OBO
HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C4-OBO,96,Standard,Standard,3000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C4-OBO
HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C4-OBO,48,Standard,High Output,3000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C4-OBO
HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C4-OBO,96,Standard,High Output,3000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C4-OBO
HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C4-OBO,48,Standard,Standard,3500K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C4-OBO
HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C4-OBO,96,Standard,Standard,3500K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C4-OBO
HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C4-OBO,48,Standard,High Output,3500K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C4-OBO
HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C4-OBO,96,Standard,High Output,3500K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C4-OBO
HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C4-OBO,48,Standard,Standard,4000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C4-OBO
HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C4-OBO,96,Standard,Standard,4000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C4-OBO
HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C4-OBO,48,Standard,High Output,4000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C4-OBO
HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C4-OBO,96,Standard,High Output,4000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C4-OBO
HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C4-OBO,48,Standard,Standard,3000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C4-OBO
HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C4-OBO,96,Standard,Standard,3000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C4-OBO
HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C4-OBO,48,Standard,High Output,3000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C4-OBO
HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C4-OBO,96,Standard,High Output,3000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C4-OBO
HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C4-OBO,48,Standard,Standard,3500K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C4-OBO
HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C4-OBO,96,Standard,Standard,3500K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C4-OBO
HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C4-OBO,48,Standard,High Output,3500K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C4-OBO
HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C4-OBO,96,Standard,High Output,3500K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C4-OBO
HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C4-OBO,48,Standard,Standard,4000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C4-OBO
HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C4-OBO,96,Standard,Standard,4000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C4-OBO
HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C4-OBO,48,Standard,High Output,4000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C4-OBO
HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C4-OBO,96,Standard,High Output,4000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C4-OBO
HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C1-OBO,144,Standard,Standard,3000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C1-OBO
HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C1-OBO,144,Standard,High Output,3000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C1-OBO
HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C1-OBO,144,Standard,Standard,3500K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C1-OBO
HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C1-OBO,144,Standard,High Output,3500K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C1-OBO
HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C1-OBO,144,Standard,Standard,4000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C1-OBO
HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C1-OBO,144,Standard,High Output,4000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C1-OBO
HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C1-OBO,144,Standard,Standard,3000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C1-OBO
HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C1-OBO,144,Standard,High Output,3000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C1-OBO
HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C1-OBO,144,Standard,Standard,3500K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C1-OBO
HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C1-OBO,144,Standard,High Output,3500K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C1-OBO
HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C1-OBO,144,Standard,Standard,4000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C1-OBO
HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C1-OBO,144,Standard,High Output,4000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C1-OBO
HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C2-OBO,144,Standard,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C2-OBO
HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C2-OBO,144,Standard,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C2-OBO
HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C2-OBO,144,Standard,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C2-OBO
HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C2-OBO,144,Standard,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C2-OBO
HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C2-OBO,144,Standard,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C2-OBO
HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C2-OBO,144,Standard,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C2-OBO
HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C2-OBO,144,Standard,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C2-OBO
HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C2-OBO,144,Standard,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C2-OBO
HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C2-OBO,144,Standard,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C2-OBO
HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C2-OBO,144,Standard,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C2-OBO
HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C2-OBO,144,Standard,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C2-OBO
HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C2-OBO,144,Standard,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C2-OBO
HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C3-OBO,144,Standard,Standard,3000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C3-OBO
HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C3-OBO,144,Standard,High Output,3000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C3-OBO
HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C3-OBO,144,Standard,Standard,3500K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C3-OBO
HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C3-OBO,144,Standard,High Output,3500K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C3-OBO
HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C3-OBO,144,Standard,Standard,4000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C3-OBO
HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C3-OBO,144,Standard,High Output,4000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C3-OBO
HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C3-OBO,144,Standard,Standard,3000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C3-OBO
HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C3-OBO,144,Standard,High Output,3000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C3-OBO
HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C3-OBO,144,Standard,Standard,3500K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C3-OBO
HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C3-OBO,144,Standard,High Output,3500K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C3-OBO
HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C3-OBO,144,Standard,Standard,4000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C3-OBO
HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C3-OBO,144,Standard,High Output,4000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C3-OBO
HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C4-OBO,144,Standard,Standard,3000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C4-OBO
HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C4-OBO,144,Standard,High Output,3000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C4-OBO
HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C4-OBO,144,Standard,Standard,3500K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C4-OBO
HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C4-OBO,144,Standard,High Output,3500K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C4-OBO
HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C4-OBO,144,Standard,Standard,4000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C4-OBO
HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C4-OBO,144,Standard,High Output,4000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C4-OBO
HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C4-OBO,144,Standard,Standard,3000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C4-OBO
HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C4-OBO,144,Standard,High Output,3000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C4-OBO
HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C4-OBO,144,Standard,Standard,3500K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C4-OBO
HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C4-OBO,144,Standard,High Output,3500K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C4-OBO
HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C4-OBO,144,Standard,Standard,4000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C4-OBO
HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C4-OBO,144,Standard,High Output,4000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C4-OBO
HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C1-OBD,48,Standard,Standard,3000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C1-OBD
HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C1-OBD,96,Standard,Standard,3000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C1-OBD
HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C1-OBD,48,Standard,High Output,3000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C1-OBD
HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C1-OBD,96,Standard,High Output,3000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C1-OBD
HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C1-OBD,48,Standard,Standard,3500K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C1-OBD
HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C1-OBD,96,Standard,Standard,3500K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C1-OBD
HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C1-OBD,48,Standard,High Output,3500K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C1-OBD
HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C1-OBD,96,Standard,High Output,3500K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C1-OBD
HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C1-OBD,48,Standard,Standard,4000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C1-OBD
HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C1-OBD,96,Standard,Standard,4000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C1-OBD
HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C1-OBD,48,Standard,High Output,4000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C1-OBD
HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C1-OBD,96,Standard,High Output,4000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C1-OBD
HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C1-OBD,48,Standard,Standard,3000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C1-OBD
HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C1-OBD,96,Standard,Standard,3000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C1-OBD
HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C1-OBD,48,Standard,High Output,3000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C1-OBD
HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C1-OBD,96,Standard,High Output,3000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C1-OBD
HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C1-OBD,48,Standard,Standard,3500K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C1-OBD
HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C1-OBD,96,Standard,Standard,3500K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C1-OBD
HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C1-OBD,48,Standard,High Output,3500K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C1-OBD
HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C1-OBD,96,Standard,High Output,3500K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C1-OBD
HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C1-OBD,48,Standard,Standard,4000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C1-OBD
HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C1-OBD,96,Standard,Standard,4000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C1-OBD
HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C1-OBD,48,Standard,High Output,4000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C1-OBD
HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C1-OBD,96,Standard,High Output,4000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C1-OBD
HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C2-OBD,48,Standard,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C2-OBD
HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C2-OBD,96,Standard,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C2-OBD
HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C2-OBD,48,Standard,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C2-OBD
HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C2-OBD,96,Standard,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C2-OBD
HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C2-OBD,48,Standard,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C2-OBD
HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C2-OBD,96,Standard,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C2-OBD
HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C2-OBD,48,Standard,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C2-OBD
HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C2-OBD,96,Standard,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C2-OBD
HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C2-OBD,48,Standard,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C2-OBD
HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C2-OBD,96,Standard,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C2-OBD
HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C2-OBD,48,Standard,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C2-OBD
HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C2-OBD,96,Standard,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C2-OBD
HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C2-OBD,48,Standard,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C2-OBD
HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C2-OBD,96,Standard,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C2-OBD
HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C2-OBD,48,Standard,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C2-OBD
HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C2-OBD,96,Standard,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C2-OBD
HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C2-OBD,48,Standard,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C2-OBD
HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C2-OBD,96,Standard,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C2-OBD
HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C2-OBD,48,Standard,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C2-OBD
HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C2-OBD,96,Standard,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C2-OBD
HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C2-OBD,48,Standard,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C2-OBD
HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C2-OBD,96,Standard,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C2-OBD
HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C2-OBD,48,Standard,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C2-OBD
HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C2-OBD,96,Standard,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C2-OBD
HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C3-OBD,48,Standard,Standard,3000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C3-OBD
HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C3-OBD,96,Standard,Standard,3000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C3-OBD
HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C3-OBD,48,Standard,High Output,3000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C3-OBD
HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C3-OBD,96,Standard,High Output,3000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C3-OBD
HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C3-OBD,48,Standard,Standard,3500K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C3-OBD
HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C3-OBD,96,Standard,Standard,3500K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C3-OBD
HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C3-OBD,48,Standard,High Output,3500K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C3-OBD
HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C3-OBD,96,Standard,High Output,3500K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C3-OBD
HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C3-OBD,48,Standard,Standard,4000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C3-OBD
HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C3-OBD,96,Standard,Standard,4000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C3-OBD
HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C3-OBD,48,Standard,High Output,4000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C3-OBD
HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C3-OBD,96,Standard,High Output,4000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C3-OBD
HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C3-OBD,48,Standard,Standard,3000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C3-OBD
HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C3-OBD,96,Standard,Standard,3000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C3-OBD
HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C3-OBD,48,Standard,High Output,3000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C3-OBD
HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C3-OBD,96,Standard,High Output,3000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C3-OBD
HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C3-OBD,48,Standard,Standard,3500K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C3-OBD
HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C3-OBD,96,Standard,Standard,3500K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C3-OBD
HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C3-OBD,48,Standard,High Output,3500K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C3-OBD
HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C3-OBD,96,Standard,High Output,3500K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C3-OBD
HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C3-OBD,48,Standard,Standard,4000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C3-OBD
HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C3-OBD,96,Standard,Standard,4000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C3-OBD
HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C3-OBD,48,Standard,High Output,4000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C3-OBD
HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C3-OBD,96,Standard,High Output,4000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C3-OBD
HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C4-OBD,48,Standard,Standard,3000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C4-OBD
HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C4-OBD,96,Standard,Standard,3000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C4-OBD
HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C4-OBD,48,Standard,High Output,3000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C4-OBD
HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C4-OBD,96,Standard,High Output,3000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C4-OBD
HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C4-OBD,48,Standard,Standard,3500K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C4-OBD
HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C4-OBD,96,Standard,Standard,3500K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C4-OBD
HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C4-OBD,48,Standard,High Output,3500K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C4-OBD
HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C4-OBD,96,Standard,High Output,3500K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C4-OBD
HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C4-OBD,48,Standard,Standard,4000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C4-OBD
HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C4-OBD,96,Standard,Standard,4000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C4-OBD
HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C4-OBD,48,Standard,High Output,4000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C4-OBD
HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C4-OBD,96,Standard,High Output,4000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C4-OBD
HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C4-OBD,48,Standard,Standard,3000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C4-OBD
HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C4-OBD,96,Standard,Standard,3000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C4-OBD
HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C4-OBD,48,Standard,High Output,3000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C4-OBD
HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C4-OBD,96,Standard,High Output,3000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C4-OBD
HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C4-OBD,48,Standard,Standard,3500K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C4-OBD
HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C4-OBD,96,Standard,Standard,3500K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C4-OBD
HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C4-OBD,48,Standard,High Output,3500K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C4-OBD
HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C4-OBD,96,Standard,High Output,3500K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C4-OBD
HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C4-OBD,48,Standard,Standard,4000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C4-OBD
HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C4-OBD,96,Standard,Standard,4000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C4-OBD
HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C4-OBD,48,Standard,High Output,4000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C4-OBD
HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C4-OBD,96,Standard,High Output,4000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C4-OBD
HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C1-OBD,144,Standard,Standard,3000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C1-OBD
HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C1-OBD,144,Standard,High Output,3000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C1-OBD
HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C1-OBD,144,Standard,Standard,3500K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C1-OBD
HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C1-OBD,144,Standard,High Output,3500K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C1-OBD
HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C1-OBD,144,Standard,Standard,4000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C1-OBD
HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C1-OBD,144,Standard,High Output,4000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C1-OBD
HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C1-OBD,144,Standard,Standard,3000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C1-OBD
HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C1-OBD,144,Standard,High Output,3000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C1-OBD
HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C1-OBD,144,Standard,Standard,3500K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C1-OBD
HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C1-OBD,144,Standard,High Output,3500K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C1-OBD
HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C1-OBD,144,Standard,Standard,4000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C1-OBD
HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C1-OBD,144,Standard,High Output,4000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C1-OBD
HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C2-OBD,144,Standard,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C2-OBD
HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C2-OBD,144,Standard,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C2-OBD
HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C2-OBD,144,Standard,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C2-OBD
HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C2-OBD,144,Standard,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C2-OBD
HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C2-OBD,144,Standard,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C2-OBD
HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C2-OBD,144,Standard,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C2-OBD
HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C2-OBD,144,Standard,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C2-OBD
HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C2-OBD,144,Standard,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C2-OBD
HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C2-OBD,144,Standard,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C2-OBD
HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C2-OBD,144,Standard,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C2-OBD
HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C2-OBD,144,Standard,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C2-OBD
HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C2-OBD,144,Standard,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C2-OBD
HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C3-OBD,144,Standard,Standard,3000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C3-OBD
HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C3-OBD,144,Standard,High Output,3000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C3-OBD
HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C3-OBD,144,Standard,Standard,3500K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C3-OBD
HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C3-OBD,144,Standard,High Output,3500K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C3-OBD
HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C3-OBD,144,Standard,Standard,4000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C3-OBD
HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C3-OBD,144,Standard,High Output,4000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C3-OBD
HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C3-OBD,144,Standard,Standard,3000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C3-OBD
HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C3-OBD,144,Standard,High Output,3000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C3-OBD
HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C3-OBD,144,Standard,Standard,3500K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C3-OBD
HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C3-OBD,144,Standard,High Output,3500K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C3-OBD
HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C3-OBD,144,Standard,Standard,4000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C3-OBD
HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C3-OBD,144,Standard,High Output,4000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C3-OBD
HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C4-OBD,144,Standard,Standard,3000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C4-OBD
HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C4-OBD,144,Standard,High Output,3000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C4-OBD
HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C4-OBD,144,Standard,Standard,3500K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C4-OBD
HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C4-OBD,144,Standard,High Output,3500K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C4-OBD
HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C4-OBD,144,Standard,Standard,4000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C4-OBD
HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C4-OBD,144,Standard,High Output,4000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C4-OBD
HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C4-OBD,144,Standard,Standard,3000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C4-OBD
HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C4-OBD,144,Standard,High Output,3000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C4-OBD
HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C4-OBD,144,Standard,Standard,3500K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C4-OBD
HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C4-OBD,144,Standard,High Output,3500K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C4-OBD
HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C4-OBD,144,Standard,Standard,4000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C4-OBD
HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C4-OBD,144,Standard,High Output,4000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C4-OBD
HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C1-OBB,48,Standard,Standard,3000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C1-OBB
HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C1-OBB,96,Standard,Standard,3000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C1-OBB
HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C1-OBB,48,Standard,High Output,3000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C1-OBB
HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C1-OBB,96,Standard,High Output,3000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C1-OBB
HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C1-OBB,48,Standard,Standard,3500K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C1-OBB
HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C1-OBB,96,Standard,Standard,3500K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C1-OBB
HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C1-OBB,48,Standard,High Output,3500K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C1-OBB
HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C1-OBB,96,Standard,High Output,3500K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C1-OBB
HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C1-OBB,48,Standard,Standard,4000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C1-OBB
HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C1-OBB,96,Standard,Standard,4000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C1-OBB
HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C1-OBB,48,Standard,High Output,4000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C1-OBB
HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C1-OBB,96,Standard,High Output,4000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C1-OBB
HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C1-OBB,48,Standard,Standard,3000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C1-OBB
HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C1-OBB,96,Standard,Standard,3000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C1-OBB
HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C1-OBB,48,Standard,High Output,3000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C1-OBB
HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C1-OBB,96,Standard,High Output,3000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C1-OBB
HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C1-OBB,48,Standard,Standard,3500K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C1-OBB
HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C1-OBB,96,Standard,Standard,3500K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C1-OBB
HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C1-OBB,48,Standard,High Output,3500K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C1-OBB
HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C1-OBB,96,Standard,High Output,3500K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C1-OBB
HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C1-OBB,48,Standard,Standard,4000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C1-OBB
HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C1-OBB,96,Standard,Standard,4000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C1-OBB
HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C1-OBB,48,Standard,High Output,4000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C1-OBB
HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C1-OBB,96,Standard,High Output,4000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C1-OBB
HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C2-OBB,48,Standard,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C2-OBB
HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C2-OBB,96,Standard,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C2-OBB
HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C2-OBB,48,Standard,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C2-OBB
HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C2-OBB,96,Standard,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C2-OBB
HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C2-OBB,48,Standard,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C2-OBB
HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C2-OBB,96,Standard,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C2-OBB
HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C2-OBB,48,Standard,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C2-OBB
HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C2-OBB,96,Standard,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C2-OBB
HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C2-OBB,48,Standard,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C2-OBB
HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C2-OBB,96,Standard,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C2-OBB
HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C2-OBB,48,Standard,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C2-OBB
HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C2-OBB,96,Standard,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C2-OBB
HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C2-OBB,48,Standard,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C2-OBB
HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C2-OBB,96,Standard,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C2-OBB
HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C2-OBB,48,Standard,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C2-OBB
HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C2-OBB,96,Standard,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C2-OBB
HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C2-OBB,48,Standard,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C2-OBB
HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C2-OBB,96,Standard,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C2-OBB
HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C2-OBB,48,Standard,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C2-OBB
HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C2-OBB,96,Standard,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C2-OBB
HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C2-OBB,48,Standard,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C2-OBB
HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C2-OBB,96,Standard,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C2-OBB
HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C2-OBB,48,Standard,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C2-OBB
HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C2-OBB,96,Standard,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C2-OBB
HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C3-OBB,48,Standard,Standard,3000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C3-OBB
HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C3-OBB,96,Standard,Standard,3000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C3-OBB
HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C3-OBB,48,Standard,High Output,3000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C3-OBB
HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C3-OBB,96,Standard,High Output,3000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C3-OBB
HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C3-OBB,48,Standard,Standard,3500K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C3-OBB
HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C3-OBB,96,Standard,Standard,3500K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C3-OBB
HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C3-OBB,48,Standard,High Output,3500K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C3-OBB
HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C3-OBB,96,Standard,High Output,3500K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C3-OBB
HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C3-OBB,48,Standard,Standard,4000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C3-OBB
HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C3-OBB,96,Standard,Standard,4000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C3-OBB
HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C3-OBB,48,Standard,High Output,4000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C3-OBB
HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C3-OBB,96,Standard,High Output,4000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C3-OBB
HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C3-OBB,48,Standard,Standard,3000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C3-OBB
HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C3-OBB,96,Standard,Standard,3000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C3-OBB
HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C3-OBB,48,Standard,High Output,3000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C3-OBB
HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C3-OBB,96,Standard,High Output,3000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C3-OBB
HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C3-OBB,48,Standard,Standard,3500K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C3-OBB
HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C3-OBB,96,Standard,Standard,3500K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C3-OBB
HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C3-OBB,48,Standard,High Output,3500K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C3-OBB
HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C3-OBB,96,Standard,High Output,3500K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C3-OBB
HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C3-OBB,48,Standard,Standard,4000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C3-OBB
HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C3-OBB,96,Standard,Standard,4000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C3-OBB
HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C3-OBB,48,Standard,High Output,4000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C3-OBB
HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C3-OBB,96,Standard,High Output,4000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C3-OBB
HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C4-OBB,48,Standard,Standard,3000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-SO-3000K-120-FA-DC-C4-OBB
HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C4-OBB,96,Standard,Standard,3000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-SO-3000K-120-FA-DC-C4-OBB
HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C4-OBB,48,Standard,High Output,3000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-HO-3000K-120-FA-DC-C4-OBB
HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C4-OBB,96,Standard,High Output,3000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-HO-3000K-120-FA-DC-C4-OBB
HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C4-OBB,48,Standard,Standard,3500K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-SO-3500K-120-FA-DC-C4-OBB
HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C4-OBB,96,Standard,Standard,3500K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-SO-3500K-120-FA-DC-C4-OBB
HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C4-OBB,48,Standard,High Output,3500K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-HO-3500K-120-FA-DC-C4-OBB
HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C4-OBB,96,Standard,High Output,3500K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-HO-3500K-120-FA-DC-C4-OBB
HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C4-OBB,48,Standard,Standard,4000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-SO-4000K-120-FA-DC-C4-OBB
HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C4-OBB,96,Standard,Standard,4000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-SO-4000K-120-FA-DC-C4-OBB
HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C4-OBB,48,Standard,High Output,4000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-HO-4000K-120-FA-DC-C4-OBB
HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C4-OBB,96,Standard,High Output,4000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-HO-4000K-120-FA-DC-C4-OBB
HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C4-OBB,48,Standard,Standard,3000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-SO-3000K-277-FA-DC-C4-OBB
HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C4-OBB,96,Standard,Standard,3000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-SO-3000K-277-FA-DC-C4-OBB
HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C4-OBB,48,Standard,High Output,3000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-HO-3000K-277-FA-DC-C4-OBB
HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C4-OBB,96,Standard,High Output,3000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-HO-3000K-277-FA-DC-C4-OBB
HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C4-OBB,48,Standard,Standard,3500K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-SO-3500K-277-FA-DC-C4-OBB
HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C4-OBB,96,Standard,Standard,3500K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-SO-3500K-277-FA-DC-C4-OBB
HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C4-OBB,48,Standard,High Output,3500K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-HO-3500K-277-FA-DC-C4-OBB
HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C4-OBB,96,Standard,High Output,3500K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-HO-3500K-277-FA-DC-C4-OBB
HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C4-OBB,48,Standard,Standard,4000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-SO-4000K-277-FA-DC-C4-OBB
HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C4-OBB,96,Standard,Standard,4000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-SO-4000K-277-FA-DC-C4-OBB
HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C4-OBB,48,Standard,High Output,4000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-SO-HO-4000K-277-FA-DC-C4-OBB
HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C4-OBB,96,Standard,High Output,4000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-SO-HO-4000K-277-FA-DC-C4-OBB
HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C1-OBB,144,Standard,Standard,3000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C1-OBB
HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C1-OBB,144,Standard,High Output,3000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C1-OBB
HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C1-OBB,144,Standard,Standard,3500K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C1-OBB
HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C1-OBB,144,Standard,High Output,3500K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C1-OBB
HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C1-OBB,144,Standard,Standard,4000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C1-OBB
HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C1-OBB,144,Standard,High Output,4000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C1-OBB
HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C1-OBB,144,Standard,Standard,3000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C1-OBB
HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C1-OBB,144,Standard,High Output,3000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C1-OBB
HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C1-OBB,144,Standard,Standard,3500K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C1-OBB
HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C1-OBB,144,Standard,High Output,3500K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C1-OBB
HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C1-OBB,144,Standard,Standard,4000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C1-OBB
HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C1-OBB,144,Standard,High Output,4000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C1-OBB
HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C2-OBB,144,Standard,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C2-OBB
HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C2-OBB,144,Standard,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C2-OBB
HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C2-OBB,144,Standard,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C2-OBB
HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C2-OBB,144,Standard,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C2-OBB
HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C2-OBB,144,Standard,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C2-OBB
HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C2-OBB,144,Standard,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C2-OBB
HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C2-OBB,144,Standard,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C2-OBB
HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C2-OBB,144,Standard,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C2-OBB
HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C2-OBB,144,Standard,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C2-OBB
HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C2-OBB,144,Standard,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C2-OBB
HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C2-OBB,144,Standard,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C2-OBB
HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C2-OBB,144,Standard,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C2-OBB
HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C3-OBB,144,Standard,Standard,3000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C3-OBB
HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C3-OBB,144,Standard,High Output,3000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C3-OBB
HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C3-OBB,144,Standard,Standard,3500K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C3-OBB
HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C3-OBB,144,Standard,High Output,3500K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C3-OBB
HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C3-OBB,144,Standard,Standard,4000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C3-OBB
HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C3-OBB,144,Standard,High Output,4000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C3-OBB
HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C3-OBB,144,Standard,Standard,3000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C3-OBB
HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C3-OBB,144,Standard,High Output,3000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C3-OBB
HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C3-OBB,144,Standard,Standard,3500K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C3-OBB
HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C3-OBB,144,Standard,High Output,3500K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C3-OBB
HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C3-OBB,144,Standard,Standard,4000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C3-OBB
HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C3-OBB,144,Standard,High Output,4000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C3-OBB
HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C4-OBB,144,Standard,Standard,3000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-SO-3000K-120-FA-DC-C4-OBB
HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C4-OBB,144,Standard,High Output,3000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-HO-3000K-120-FA-DC-C4-OBB
HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C4-OBB,144,Standard,Standard,3500K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-SO-3500K-120-FA-DC-C4-OBB
HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C4-OBB,144,Standard,High Output,3500K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-HO-3500K-120-FA-DC-C4-OBB
HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C4-OBB,144,Standard,Standard,4000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-SO-4000K-120-FA-DC-C4-OBB
HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C4-OBB,144,Standard,High Output,4000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-HO-4000K-120-FA-DC-C4-OBB
HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C4-OBB,144,Standard,Standard,3000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-SO-3000K-277-FA-DC-C4-OBB
HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C4-OBB,144,Standard,High Output,3000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-HO-3000K-277-FA-DC-C4-OBB
HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C4-OBB,144,Standard,Standard,3500K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-SO-3500K-277-FA-DC-C4-OBB
HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C4-OBB,144,Standard,High Output,3500K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-HO-3500K-277-FA-DC-C4-OBB
HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C4-OBB,144,Standard,Standard,4000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-SO-4000K-277-FA-DC-C4-OBB
HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C4-OBB,144,Standard,High Output,4000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-SO-HO-4000K-277-FA-DC-C4-OBB
HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C1-OBO,48,High Output,Standard,3000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C1-OBO
HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C1-OBO,96,High Output,Standard,3000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C1-OBO
HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C1-OBO,48,High Output,High Output,3000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C1-OBO
HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C1-OBO,96,High Output,High Output,3000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C1-OBO
HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C1-OBO,48,High Output,Standard,3500K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C1-OBO
HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C1-OBO,96,High Output,Standard,3500K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C1-OBO
HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C1-OBO,48,High Output,High Output,3500K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C1-OBO
HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C1-OBO,96,High Output,High Output,3500K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C1-OBO
HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C1-OBO,48,High Output,Standard,4000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C1-OBO
HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C1-OBO,96,High Output,Standard,4000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C1-OBO
HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C1-OBO,48,High Output,High Output,4000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C1-OBO
HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C1-OBO,96,High Output,High Output,4000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C1-OBO
HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C1-OBO,48,High Output,Standard,3000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C1-OBO
HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C1-OBO,96,High Output,Standard,3000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C1-OBO
HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C1-OBO,48,High Output,High Output,3000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C1-OBO
HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C1-OBO,96,High Output,High Output,3000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C1-OBO
HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C1-OBO,48,High Output,Standard,3500K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C1-OBO
HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C1-OBO,96,High Output,Standard,3500K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C1-OBO
HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C1-OBO,48,High Output,High Output,3500K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C1-OBO
HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C1-OBO,96,High Output,High Output,3500K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C1-OBO
HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C1-OBO,48,High Output,Standard,4000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C1-OBO
HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C1-OBO,96,High Output,Standard,4000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C1-OBO
HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C1-OBO,48,High Output,High Output,4000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C1-OBO
HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C1-OBO,96,High Output,High Output,4000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C1-OBO
HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C2-OBO,48,High Output,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C2-OBO
HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C2-OBO,96,High Output,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C2-OBO
HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C2-OBO,48,High Output,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C2-OBO
HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C2-OBO,96,High Output,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C2-OBO
HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C2-OBO,48,High Output,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C2-OBO
HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C2-OBO,96,High Output,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C2-OBO
HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C2-OBO,48,High Output,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C2-OBO
HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C2-OBO,96,High Output,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C2-OBO
HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C2-OBO,48,High Output,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C2-OBO
HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C2-OBO,96,High Output,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C2-OBO
HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C2-OBO,48,High Output,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C2-OBO
HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C2-OBO,96,High Output,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C2-OBO
HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C2-OBO,48,High Output,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C2-OBO
HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C2-OBO,96,High Output,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C2-OBO
HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C2-OBO,48,High Output,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C2-OBO
HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C2-OBO,96,High Output,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C2-OBO
HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C2-OBO,48,High Output,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C2-OBO
HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C2-OBO,96,High Output,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C2-OBO
HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C2-OBO,48,High Output,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C2-OBO
HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C2-OBO,96,High Output,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C2-OBO
HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C2-OBO,48,High Output,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C2-OBO
HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C2-OBO,96,High Output,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C2-OBO
HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C2-OBO,48,High Output,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C2-OBO
HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C2-OBO,96,High Output,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C2-OBO
HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C3-OBO,48,High Output,Standard,3000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C3-OBO
HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C3-OBO,96,High Output,Standard,3000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C3-OBO
HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C3-OBO,48,High Output,High Output,3000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C3-OBO
HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C3-OBO,96,High Output,High Output,3000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C3-OBO
HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C3-OBO,48,High Output,Standard,3500K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C3-OBO
HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C3-OBO,96,High Output,Standard,3500K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C3-OBO
HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C3-OBO,48,High Output,High Output,3500K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C3-OBO
HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C3-OBO,96,High Output,High Output,3500K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C3-OBO
HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C3-OBO,48,High Output,Standard,4000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C3-OBO
HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C3-OBO,96,High Output,Standard,4000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C3-OBO
HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C3-OBO,48,High Output,High Output,4000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C3-OBO
HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C3-OBO,96,High Output,High Output,4000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C3-OBO
HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C3-OBO,48,High Output,Standard,3000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C3-OBO
HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C3-OBO,96,High Output,Standard,3000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C3-OBO
HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C3-OBO,48,High Output,High Output,3000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C3-OBO
HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C3-OBO,96,High Output,High Output,3000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C3-OBO
HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C3-OBO,48,High Output,Standard,3500K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C3-OBO
HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C3-OBO,96,High Output,Standard,3500K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C3-OBO
HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C3-OBO,48,High Output,High Output,3500K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C3-OBO
HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C3-OBO,96,High Output,High Output,3500K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C3-OBO
HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C3-OBO,48,High Output,Standard,4000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C3-OBO
HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C3-OBO,96,High Output,Standard,4000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C3-OBO
HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C3-OBO,48,High Output,High Output,4000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C3-OBO
HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C3-OBO,96,High Output,High Output,4000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C3-OBO
HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C4-OBO,48,High Output,Standard,3000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C4-OBO
HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C4-OBO,96,High Output,Standard,3000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C4-OBO
HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C4-OBO,48,High Output,High Output,3000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C4-OBO
HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C4-OBO,96,High Output,High Output,3000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C4-OBO
HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C4-OBO,48,High Output,Standard,3500K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C4-OBO
HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C4-OBO,96,High Output,Standard,3500K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C4-OBO
HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C4-OBO,48,High Output,High Output,3500K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C4-OBO
HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C4-OBO,96,High Output,High Output,3500K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C4-OBO
HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C4-OBO,48,High Output,Standard,4000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C4-OBO
HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C4-OBO,96,High Output,Standard,4000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C4-OBO
HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C4-OBO,48,High Output,High Output,4000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C4-OBO
HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C4-OBO,96,High Output,High Output,4000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C4-OBO
HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C4-OBO,48,High Output,Standard,3000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C4-OBO
HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C4-OBO,96,High Output,Standard,3000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C4-OBO
HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C4-OBO,48,High Output,High Output,3000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C4-OBO
HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C4-OBO,96,High Output,High Output,3000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C4-OBO
HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C4-OBO,48,High Output,Standard,3500K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C4-OBO
HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C4-OBO,96,High Output,Standard,3500K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C4-OBO
HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C4-OBO,48,High Output,High Output,3500K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C4-OBO
HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C4-OBO,96,High Output,High Output,3500K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C4-OBO
HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C4-OBO,48,High Output,Standard,4000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C4-OBO
HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C4-OBO,96,High Output,Standard,4000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C4-OBO
HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C4-OBO,48,High Output,High Output,4000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C4-OBO
HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C4-OBO,96,High Output,High Output,4000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C4-OBO
HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C1-OBO,144,High Output,Standard,3000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C1-OBO
HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C1-OBO,144,High Output,High Output,3000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C1-OBO
HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C1-OBO,144,High Output,Standard,3500K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C1-OBO
HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C1-OBO,144,High Output,High Output,3500K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C1-OBO
HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C1-OBO,144,High Output,Standard,4000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C1-OBO
HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C1-OBO,144,High Output,High Output,4000K,120,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C1-OBO
HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C1-OBO,144,High Output,Standard,3000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C1-OBO
HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C1-OBO,144,High Output,High Output,3000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C1-OBO
HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C1-OBO,144,High Output,Standard,3500K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C1-OBO
HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C1-OBO,144,High Output,High Output,3500K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C1-OBO
HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C1-OBO,144,High Output,Standard,4000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C1-OBO
HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C1-OBO,144,High Output,High Output,4000K,277,Dual Circuit,1” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C1-OBO
HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C2-OBO,144,High Output,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C2-OBO
HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C2-OBO,144,High Output,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C2-OBO
HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C2-OBO,144,High Output,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C2-OBO
HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C2-OBO,144,High Output,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C2-OBO
HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C2-OBO,144,High Output,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C2-OBO
HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C2-OBO,144,High Output,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C2-OBO
HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C2-OBO,144,High Output,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C2-OBO
HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C2-OBO,144,High Output,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C2-OBO
HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C2-OBO,144,High Output,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C2-OBO
HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C2-OBO,144,High Output,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C2-OBO
HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C2-OBO,144,High Output,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C2-OBO
HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C2-OBO,144,High Output,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Occupancy,HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C2-OBO
HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C3-OBO,144,High Output,Standard,3000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C3-OBO
HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C3-OBO,144,High Output,High Output,3000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C3-OBO
HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C3-OBO,144,High Output,Standard,3500K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C3-OBO
HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C3-OBO,144,High Output,High Output,3500K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C3-OBO
HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C3-OBO,144,High Output,Standard,4000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C3-OBO
HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C3-OBO,144,High Output,High Output,4000K,120,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C3-OBO
HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C3-OBO,144,High Output,Standard,3000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C3-OBO
HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C3-OBO,144,High Output,High Output,3000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C3-OBO
HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C3-OBO,144,High Output,Standard,3500K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C3-OBO
HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C3-OBO,144,High Output,High Output,3500K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C3-OBO
HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C3-OBO,144,High Output,Standard,4000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C3-OBO
HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C3-OBO,144,High Output,High Output,4000K,277,Dual Circuit,Slot Grid,Occupancy,HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C3-OBO
HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C4-OBO,144,High Output,Standard,3000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C4-OBO
HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C4-OBO,144,High Output,High Output,3000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C4-OBO
HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C4-OBO,144,High Output,Standard,3500K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C4-OBO
HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C4-OBO,144,High Output,High Output,3500K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C4-OBO
HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C4-OBO,144,High Output,Standard,4000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C4-OBO
HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C4-OBO,144,High Output,High Output,4000K,120,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C4-OBO
HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C4-OBO,144,High Output,Standard,3000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C4-OBO
HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C4-OBO,144,High Output,High Output,3000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C4-OBO
HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C4-OBO,144,High Output,Standard,3500K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C4-OBO
HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C4-OBO,144,High Output,High Output,3500K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C4-OBO
HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C4-OBO,144,High Output,Standard,4000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C4-OBO
HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C4-OBO,144,High Output,High Output,4000K,277,Dual Circuit,Hard Ceiling,Occupancy,HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C4-OBO
HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C1-OBD,48,High Output,Standard,3000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C1-OBD
HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C1-OBD,96,High Output,Standard,3000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C1-OBD
HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C1-OBD,48,High Output,High Output,3000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C1-OBD
HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C1-OBD,96,High Output,High Output,3000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C1-OBD
HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C1-OBD,48,High Output,Standard,3500K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C1-OBD
HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C1-OBD,96,High Output,Standard,3500K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C1-OBD
HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C1-OBD,48,High Output,High Output,3500K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C1-OBD
HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C1-OBD,96,High Output,High Output,3500K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C1-OBD
HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C1-OBD,48,High Output,Standard,4000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C1-OBD
HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C1-OBD,96,High Output,Standard,4000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C1-OBD
HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C1-OBD,48,High Output,High Output,4000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C1-OBD
HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C1-OBD,96,High Output,High Output,4000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C1-OBD
HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C1-OBD,48,High Output,Standard,3000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C1-OBD
HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C1-OBD,96,High Output,Standard,3000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C1-OBD
HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C1-OBD,48,High Output,High Output,3000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C1-OBD
HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C1-OBD,96,High Output,High Output,3000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C1-OBD
HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C1-OBD,48,High Output,Standard,3500K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C1-OBD
HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C1-OBD,96,High Output,Standard,3500K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C1-OBD
HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C1-OBD,48,High Output,High Output,3500K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C1-OBD
HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C1-OBD,96,High Output,High Output,3500K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C1-OBD
HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C1-OBD,48,High Output,Standard,4000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C1-OBD
HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C1-OBD,96,High Output,Standard,4000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C1-OBD
HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C1-OBD,48,High Output,High Output,4000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C1-OBD
HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C1-OBD,96,High Output,High Output,4000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C1-OBD
HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C2-OBD,48,High Output,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C2-OBD
HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C2-OBD,96,High Output,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C2-OBD
HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C2-OBD,48,High Output,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C2-OBD
HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C2-OBD,96,High Output,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C2-OBD
HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C2-OBD,48,High Output,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C2-OBD
HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C2-OBD,96,High Output,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C2-OBD
HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C2-OBD,48,High Output,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C2-OBD
HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C2-OBD,96,High Output,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C2-OBD
HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C2-OBD,48,High Output,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C2-OBD
HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C2-OBD,96,High Output,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C2-OBD
HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C2-OBD,48,High Output,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C2-OBD
HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C2-OBD,96,High Output,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C2-OBD
HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C2-OBD,48,High Output,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C2-OBD
HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C2-OBD,96,High Output,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C2-OBD
HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C2-OBD,48,High Output,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C2-OBD
HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C2-OBD,96,High Output,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C2-OBD
HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C2-OBD,48,High Output,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C2-OBD
HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C2-OBD,96,High Output,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C2-OBD
HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C2-OBD,48,High Output,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C2-OBD
HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C2-OBD,96,High Output,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C2-OBD
HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C2-OBD,48,High Output,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C2-OBD
HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C2-OBD,96,High Output,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C2-OBD
HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C2-OBD,48,High Output,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C2-OBD
HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C2-OBD,96,High Output,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C2-OBD
HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C3-OBD,48,High Output,Standard,3000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C3-OBD
HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C3-OBD,96,High Output,Standard,3000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C3-OBD
HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C3-OBD,48,High Output,High Output,3000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C3-OBD
HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C3-OBD,96,High Output,High Output,3000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C3-OBD
HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C3-OBD,48,High Output,Standard,3500K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C3-OBD
HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C3-OBD,96,High Output,Standard,3500K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C3-OBD
HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C3-OBD,48,High Output,High Output,3500K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C3-OBD
HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C3-OBD,96,High Output,High Output,3500K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C3-OBD
HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C3-OBD,48,High Output,Standard,4000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C3-OBD
HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C3-OBD,96,High Output,Standard,4000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C3-OBD
HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C3-OBD,48,High Output,High Output,4000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C3-OBD
HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C3-OBD,96,High Output,High Output,4000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C3-OBD
HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C3-OBD,48,High Output,Standard,3000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C3-OBD
HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C3-OBD,96,High Output,Standard,3000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C3-OBD
HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C3-OBD,48,High Output,High Output,3000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C3-OBD
HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C3-OBD,96,High Output,High Output,3000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C3-OBD
HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C3-OBD,48,High Output,Standard,3500K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C3-OBD
HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C3-OBD,96,High Output,Standard,3500K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C3-OBD
HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C3-OBD,48,High Output,High Output,3500K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C3-OBD
HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C3-OBD,96,High Output,High Output,3500K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C3-OBD
HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C3-OBD,48,High Output,Standard,4000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C3-OBD
HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C3-OBD,96,High Output,Standard,4000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C3-OBD
HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C3-OBD,48,High Output,High Output,4000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C3-OBD
HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C3-OBD,96,High Output,High Output,4000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C3-OBD
HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C4-OBD,48,High Output,Standard,3000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C4-OBD
HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C4-OBD,96,High Output,Standard,3000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C4-OBD
HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C4-OBD,48,High Output,High Output,3000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C4-OBD
HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C4-OBD,96,High Output,High Output,3000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C4-OBD
HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C4-OBD,48,High Output,Standard,3500K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C4-OBD
HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C4-OBD,96,High Output,Standard,3500K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C4-OBD
HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C4-OBD,48,High Output,High Output,3500K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C4-OBD
HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C4-OBD,96,High Output,High Output,3500K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C4-OBD
HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C4-OBD,48,High Output,Standard,4000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C4-OBD
HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C4-OBD,96,High Output,Standard,4000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C4-OBD
HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C4-OBD,48,High Output,High Output,4000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C4-OBD
HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C4-OBD,96,High Output,High Output,4000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C4-OBD
HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C4-OBD,48,High Output,Standard,3000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C4-OBD
HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C4-OBD,96,High Output,Standard,3000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C4-OBD
HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C4-OBD,48,High Output,High Output,3000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C4-OBD
HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C4-OBD,96,High Output,High Output,3000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C4-OBD
HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C4-OBD,48,High Output,Standard,3500K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C4-OBD
HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C4-OBD,96,High Output,Standard,3500K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C4-OBD
HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C4-OBD,48,High Output,High Output,3500K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C4-OBD
HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C4-OBD,96,High Output,High Output,3500K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C4-OBD
HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C4-OBD,48,High Output,Standard,4000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C4-OBD
HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C4-OBD,96,High Output,Standard,4000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C4-OBD
HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C4-OBD,48,High Output,High Output,4000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C4-OBD
HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C4-OBD,96,High Output,High Output,4000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C4-OBD
HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C1-OBD,144,High Output,Standard,3000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C1-OBD
HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C1-OBD,144,High Output,High Output,3000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C1-OBD
HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C1-OBD,144,High Output,Standard,3500K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C1-OBD
HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C1-OBD,144,High Output,High Output,3500K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C1-OBD
HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C1-OBD,144,High Output,Standard,4000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C1-OBD
HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C1-OBD,144,High Output,High Output,4000K,120,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C1-OBD
HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C1-OBD,144,High Output,Standard,3000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C1-OBD
HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C1-OBD,144,High Output,High Output,3000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C1-OBD
HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C1-OBD,144,High Output,Standard,3500K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C1-OBD
HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C1-OBD,144,High Output,High Output,3500K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C1-OBD
HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C1-OBD,144,High Output,Standard,4000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C1-OBD
HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C1-OBD,144,High Output,High Output,4000K,277,Dual Circuit,1” T-Bar,Daylight,HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C1-OBD
HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C2-OBD,144,High Output,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C2-OBD
HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C2-OBD,144,High Output,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C2-OBD
HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C2-OBD,144,High Output,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C2-OBD
HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C2-OBD,144,High Output,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C2-OBD
HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C2-OBD,144,High Output,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C2-OBD
HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C2-OBD,144,High Output,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C2-OBD
HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C2-OBD,144,High Output,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C2-OBD
HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C2-OBD,144,High Output,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C2-OBD
HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C2-OBD,144,High Output,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C2-OBD
HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C2-OBD,144,High Output,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C2-OBD
HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C2-OBD,144,High Output,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C2-OBD
HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C2-OBD,144,High Output,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Daylight,HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C2-OBD
HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C3-OBD,144,High Output,Standard,3000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C3-OBD
HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C3-OBD,144,High Output,High Output,3000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C3-OBD
HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C3-OBD,144,High Output,Standard,3500K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C3-OBD
HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C3-OBD,144,High Output,High Output,3500K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C3-OBD
HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C3-OBD,144,High Output,Standard,4000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C3-OBD
HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C3-OBD,144,High Output,High Output,4000K,120,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C3-OBD
HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C3-OBD,144,High Output,Standard,3000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C3-OBD
HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C3-OBD,144,High Output,High Output,3000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C3-OBD
HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C3-OBD,144,High Output,Standard,3500K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C3-OBD
HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C3-OBD,144,High Output,High Output,3500K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C3-OBD
HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C3-OBD,144,High Output,Standard,4000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C3-OBD
HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C3-OBD,144,High Output,High Output,4000K,277,Dual Circuit,Slot Grid,Daylight,HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C3-OBD
HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C4-OBD,144,High Output,Standard,3000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C4-OBD
HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C4-OBD,144,High Output,High Output,3000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C4-OBD
HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C4-OBD,144,High Output,Standard,3500K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C4-OBD
HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C4-OBD,144,High Output,High Output,3500K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C4-OBD
HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C4-OBD,144,High Output,Standard,4000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C4-OBD
HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C4-OBD,144,High Output,High Output,4000K,120,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C4-OBD
HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C4-OBD,144,High Output,Standard,3000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C4-OBD
HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C4-OBD,144,High Output,High Output,3000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C4-OBD
HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C4-OBD,144,High Output,Standard,3500K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C4-OBD
HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C4-OBD,144,High Output,High Output,3500K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C4-OBD
HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C4-OBD,144,High Output,Standard,4000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C4-OBD
HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C4-OBD,144,High Output,High Output,4000K,277,Dual Circuit,Hard Ceiling,Daylight,HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C4-OBD
HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C1-OBB,48,High Output,Standard,3000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C1-OBB
HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C1-OBB,96,High Output,Standard,3000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C1-OBB
HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C1-OBB,48,High Output,High Output,3000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C1-OBB
HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C1-OBB,96,High Output,High Output,3000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C1-OBB
HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C1-OBB,48,High Output,Standard,3500K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C1-OBB
HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C1-OBB,96,High Output,Standard,3500K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C1-OBB
HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C1-OBB,48,High Output,High Output,3500K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C1-OBB
HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C1-OBB,96,High Output,High Output,3500K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C1-OBB
HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C1-OBB,48,High Output,Standard,4000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C1-OBB
HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C1-OBB,96,High Output,Standard,4000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C1-OBB
HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C1-OBB,48,High Output,High Output,4000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C1-OBB
HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C1-OBB,96,High Output,High Output,4000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C1-OBB
HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C1-OBB,48,High Output,Standard,3000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C1-OBB
HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C1-OBB,96,High Output,Standard,3000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C1-OBB
HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C1-OBB,48,High Output,High Output,3000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C1-OBB
HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C1-OBB,96,High Output,High Output,3000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C1-OBB
HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C1-OBB,48,High Output,Standard,3500K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C1-OBB
HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C1-OBB,96,High Output,Standard,3500K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C1-OBB
HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C1-OBB,48,High Output,High Output,3500K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C1-OBB
HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C1-OBB,96,High Output,High Output,3500K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C1-OBB
HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C1-OBB,48,High Output,Standard,4000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C1-OBB
HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C1-OBB,96,High Output,Standard,4000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C1-OBB
HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C1-OBB,48,High Output,High Output,4000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C1-OBB
HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C1-OBB,96,High Output,High Output,4000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C1-OBB
HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C2-OBB,48,High Output,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C2-OBB
HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C2-OBB,96,High Output,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C2-OBB
HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C2-OBB,48,High Output,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C2-OBB
HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C2-OBB,96,High Output,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C2-OBB
HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C2-OBB,48,High Output,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C2-OBB
HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C2-OBB,96,High Output,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C2-OBB
HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C2-OBB,48,High Output,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C2-OBB
HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C2-OBB,96,High Output,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C2-OBB
HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C2-OBB,48,High Output,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C2-OBB
HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C2-OBB,96,High Output,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C2-OBB
HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C2-OBB,48,High Output,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C2-OBB
HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C2-OBB,96,High Output,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C2-OBB
HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C2-OBB,48,High Output,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C2-OBB
HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C2-OBB,96,High Output,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C2-OBB
HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C2-OBB,48,High Output,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C2-OBB
HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C2-OBB,96,High Output,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C2-OBB
HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C2-OBB,48,High Output,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C2-OBB
HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C2-OBB,96,High Output,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C2-OBB
HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C2-OBB,48,High Output,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C2-OBB
HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C2-OBB,96,High Output,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C2-OBB
HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C2-OBB,48,High Output,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C2-OBB
HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C2-OBB,96,High Output,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C2-OBB
HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C2-OBB,48,High Output,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C2-OBB
HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C2-OBB,96,High Output,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C2-OBB
HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C3-OBB,48,High Output,Standard,3000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C3-OBB
HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C3-OBB,96,High Output,Standard,3000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C3-OBB
HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C3-OBB,48,High Output,High Output,3000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C3-OBB
HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C3-OBB,96,High Output,High Output,3000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C3-OBB
HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C3-OBB,48,High Output,Standard,3500K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C3-OBB
HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C3-OBB,96,High Output,Standard,3500K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C3-OBB
HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C3-OBB,48,High Output,High Output,3500K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C3-OBB
HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C3-OBB,96,High Output,High Output,3500K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C3-OBB
HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C3-OBB,48,High Output,Standard,4000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C3-OBB
HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C3-OBB,96,High Output,Standard,4000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C3-OBB
HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C3-OBB,48,High Output,High Output,4000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C3-OBB
HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C3-OBB,96,High Output,High Output,4000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C3-OBB
HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C3-OBB,48,High Output,Standard,3000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C3-OBB
HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C3-OBB,96,High Output,Standard,3000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C3-OBB
HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C3-OBB,48,High Output,High Output,3000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C3-OBB
HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C3-OBB,96,High Output,High Output,3000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C3-OBB
HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C3-OBB,48,High Output,Standard,3500K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C3-OBB
HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C3-OBB,96,High Output,Standard,3500K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C3-OBB
HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C3-OBB,48,High Output,High Output,3500K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C3-OBB
HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C3-OBB,96,High Output,High Output,3500K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C3-OBB
HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C3-OBB,48,High Output,Standard,4000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C3-OBB
HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C3-OBB,96,High Output,Standard,4000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C3-OBB
HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C3-OBB,48,High Output,High Output,4000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C3-OBB
HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C3-OBB,96,High Output,High Output,4000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C3-OBB
HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C4-OBB,48,High Output,Standard,3000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-SO-3000K-120-FA-DC-C4-OBB
HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C4-OBB,96,High Output,Standard,3000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-SO-3000K-120-FA-DC-C4-OBB
HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C4-OBB,48,High Output,High Output,3000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-HO-3000K-120-FA-DC-C4-OBB
HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C4-OBB,96,High Output,High Output,3000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-HO-3000K-120-FA-DC-C4-OBB
HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C4-OBB,48,High Output,Standard,3500K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-SO-3500K-120-FA-DC-C4-OBB
HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C4-OBB,96,High Output,Standard,3500K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-SO-3500K-120-FA-DC-C4-OBB
HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C4-OBB,48,High Output,High Output,3500K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-HO-3500K-120-FA-DC-C4-OBB
HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C4-OBB,96,High Output,High Output,3500K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-HO-3500K-120-FA-DC-C4-OBB
HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C4-OBB,48,High Output,Standard,4000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-SO-4000K-120-FA-DC-C4-OBB
HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C4-OBB,96,High Output,Standard,4000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-SO-4000K-120-FA-DC-C4-OBB
HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C4-OBB,48,High Output,High Output,4000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-HO-4000K-120-FA-DC-C4-OBB
HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C4-OBB,96,High Output,High Output,4000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-HO-4000K-120-FA-DC-C4-OBB
HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C4-OBB,48,High Output,Standard,3000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-SO-3000K-277-FA-DC-C4-OBB
HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C4-OBB,96,High Output,Standard,3000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-SO-3000K-277-FA-DC-C4-OBB
HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C4-OBB,48,High Output,High Output,3000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-HO-3000K-277-FA-DC-C4-OBB
HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C4-OBB,96,High Output,High Output,3000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-HO-3000K-277-FA-DC-C4-OBB
HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C4-OBB,48,High Output,Standard,3500K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-SO-3500K-277-FA-DC-C4-OBB
HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C4-OBB,96,High Output,Standard,3500K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-SO-3500K-277-FA-DC-C4-OBB
HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C4-OBB,48,High Output,High Output,3500K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-HO-3500K-277-FA-DC-C4-OBB
HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C4-OBB,96,High Output,High Output,3500K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-HO-3500K-277-FA-DC-C4-OBB
HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C4-OBB,48,High Output,Standard,4000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-SO-4000K-277-FA-DC-C4-OBB
HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C4-OBB,96,High Output,Standard,4000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-SO-4000K-277-FA-DC-C4-OBB
HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C4-OBB,48,High Output,High Output,4000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-4'-HO-HO-4000K-277-FA-DC-C4-OBB
HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C4-OBB,96,High Output,High Output,4000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-8'-HO-HO-4000K-277-FA-DC-C4-OBB
HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C1-OBB,144,High Output,Standard,3000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C1-OBB
HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C1-OBB,144,High Output,High Output,3000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C1-OBB
HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C1-OBB,144,High Output,Standard,3500K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C1-OBB
HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C1-OBB,144,High Output,High Output,3500K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C1-OBB
HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C1-OBB,144,High Output,Standard,4000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C1-OBB
HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C1-OBB,144,High Output,High Output,4000K,120,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C1-OBB
HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C1-OBB,144,High Output,Standard,3000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C1-OBB
HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C1-OBB,144,High Output,High Output,3000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C1-OBB
HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C1-OBB,144,High Output,Standard,3500K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C1-OBB
HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C1-OBB,144,High Output,High Output,3500K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C1-OBB
HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C1-OBB,144,High Output,Standard,4000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C1-OBB
HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C1-OBB,144,High Output,High Output,4000K,277,Dual Circuit,1” T-Bar,Both,HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C1-OBB
HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C2-OBB,144,High Output,Standard,3000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C2-OBB
HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C2-OBB,144,High Output,High Output,3000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C2-OBB
HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C2-OBB,144,High Output,Standard,3500K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C2-OBB
HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C2-OBB,144,High Output,High Output,3500K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C2-OBB
HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C2-OBB,144,High Output,Standard,4000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C2-OBB
HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C2-OBB,144,High Output,High Output,4000K,120,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C2-OBB
HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C2-OBB,144,High Output,Standard,3000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C2-OBB
HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C2-OBB,144,High Output,High Output,3000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C2-OBB
HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C2-OBB,144,High Output,Standard,3500K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C2-OBB
HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C2-OBB,144,High Output,High Output,3500K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C2-OBB
HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C2-OBB,144,High Output,Standard,4000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C2-OBB
HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C2-OBB,144,High Output,High Output,4000K,277,Dual Circuit,9/16” T-Bar,Both,HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C2-OBB
HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C3-OBB,144,High Output,Standard,3000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C3-OBB
HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C3-OBB,144,High Output,High Output,3000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C3-OBB
HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C3-OBB,144,High Output,Standard,3500K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C3-OBB
HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C3-OBB,144,High Output,High Output,3500K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C3-OBB
HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C3-OBB,144,High Output,Standard,4000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C3-OBB
HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C3-OBB,144,High Output,High Output,4000K,120,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C3-OBB
HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C3-OBB,144,High Output,Standard,3000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C3-OBB
HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C3-OBB,144,High Output,High Output,3000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C3-OBB
HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C3-OBB,144,High Output,Standard,3500K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C3-OBB
HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C3-OBB,144,High Output,High Output,3500K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C3-OBB
HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C3-OBB,144,High Output,Standard,4000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C3-OBB
HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C3-OBB,144,High Output,High Output,4000K,277,Dual Circuit,Slot Grid,Both,HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C3-OBB
HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C4-OBB,144,High Output,Standard,3000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-SO-3000K-120-FA-DC-C4-OBB
HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C4-OBB,144,High Output,High Output,3000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-HO-3000K-120-FA-DC-C4-OBB
HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C4-OBB,144,High Output,Standard,3500K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-SO-3500K-120-FA-DC-C4-OBB
HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C4-OBB,144,High Output,High Output,3500K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-HO-3500K-120-FA-DC-C4-OBB
HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C4-OBB,144,High Output,Standard,4000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-SO-4000K-120-FA-DC-C4-OBB
HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C4-OBB,144,High Output,High Output,4000K,120,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-HO-4000K-120-FA-DC-C4-OBB
HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C4-OBB,144,High Output,Standard,3000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-SO-3000K-277-FA-DC-C4-OBB
HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C4-OBB,144,High Output,High Output,3000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-HO-3000K-277-FA-DC-C4-OBB
HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C4-OBB,144,High Output,Standard,3500K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-SO-3500K-277-FA-DC-C4-OBB
HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C4-OBB,144,High Output,High Output,3500K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-HO-3500K-277-FA-DC-C4-OBB
HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C4-OBB,144,High Output,Standard,4000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-SO-4000K-277-FA-DC-C4-OBB
HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C4-OBB,144,High Output,High Output,4000K,277,Dual Circuit,Hard Ceiling,Both,HP-2 ID-12'-HO-HO-4000K-277-FA-DC-C4-OBB
