,Watts##ELECTRICAL_WATTAGE##WATTS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Luminous Flux##Electrical_Luminous_Flux##Lumens,Housing Type##OTHER##,Width##LENGTH##INCHES,Length##LENGTH##INCHES,Photometric File Name##OTHER##,Model##OTHER##
ASC24-LED-HO-CW,56,5000,6854.00,Housing : ASC24,23.78,48,ASC24-LED-HO-CW.ies,ASC24-LED-HO-CW
ASC24-LED-HO-NW,54,4000,6266.00,Housing : ASC24,23.78,48,ASC24-LED-HO-NW.ies,ASC24-LED-HO-NW
ASC24-LED-HO-WW,54,3500,5671.00,Housing : ASC24,23.78,48,ASC24-LED-HO-WW.ies,ASC24-LED-HO-WW
ASC24-LED-SS-CW,45,5000,5574.00,Housing : ASC24,23.78,48,ASC24-LED-SS-CW.ies,ASC24-LED-SS-CW
ASC24-LED-SS-NW,44,4000,5148.00,Housing : ASC24,23.78,48,ASC24-LED-SS-NW.ies,ASC24-LED-SS-NW
ASC24-LED-SS-WW,45,3500,4623.00,Housing : ASC24,23.78,48,ASC24-LED-SS-WW.ies,ASC24-LED-SS-WW
ASC14-LED-HO-CW,34,5000,4098.00,Housing : ASC14,11.61,48,ASC14-LED-HO-CW.ies,ASC14-LED-HO-CW
ASC14-LED-HO-NW,34,4000,3487.00,Housing : ASC14,11.61,48,ASC14-LED-HO-NW.ies,ASC14-LED-HO-NW
ASC14-LED-HO-WW,34,3500,3440.00,Housing : ASC14,11.61,48,ASC14-LED-HO-WW.ies,ASC14-LED-HO-WW
ASC14-LED-SS-CW,27,5000,3453.00,Housing : ASC14,11.61,48,ASC14-LED-SS-CW.ies,ASC14-LED-SS-CW
ASC14-LED-SS-NW,27,4000,2935.00,Housing : ASC14,11.61,48,ASC14-LED-SS-NW.ies,ASC14-LED-SS-NW
ASC14-LED-SS-WW,27,3500,2889.00,Housing : ASC14,11.61,48,ASC14-LED-SS-WW.ies,ASC14-LED-SS-WW
ASC22-LED-HO-CW,34,5000,4178.00,Housing : ASC22,23.78,24,ASC22-LED-HO-CW.ies,ASC22-LED-HO-CW
ASC22-LED-HO-NW,34,4000,3521.00,Housing : ASC22,23.78,24,ASC22-LED-HO-NW.ies,ASC22-LED-HO-NW
ASC22-LED-HO-WW,34,3500,3401.00,Housing : ASC22,23.78,24,ASC22-LED-HO-WW.ies,ASC22-LED-HO-WW
ASC22-LED-SS-CW,27,5000,3519.00,Housing : ASC22,23.78,24,ASC22-LED-SS-CW.ies,ASC22-LED-SS-CW
ASC22-LED-SS-NW,27,4000,2993.00,Housing : ASC22,23.78,24,ASC22-LED-SS-NW.ies,ASC22-LED-SS-NW
ASC22-LED-SS-WW,27,3500,2872.00,Housing : ASC22,23.78,24,ASC22-LED-SS-WW.ies,ASC22-LED-SS-WW
