,Watts##ELECTRICAL_WATTAGE##WATTS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Luminous Flux##Electrical_Luminous_Flux##Lumens,Housing Type##OTHER##,Width##LENGTH##INCHES,Length##LENGTH##INCHES,Photometric File Name##OTHER##,Model##OTHER##
PEC14-LED-HO-LPW-CW,39,5000,3094.00,Housing : PEC14,11.61,48,PEC14-LED-HO-LPW-CW.ies,PEC14-LED-HO-LPW-CW
PEC14-LED-HO-LPW-NW,39,4000,2688.00,Housing : PEC14,11.61,48,PEC14-LED-HO-LPW-NW.ies,PEC14-LED-HO-LPW-NW
PEC14-LED-HO-LPW-WW,39,3500,2821.00,Housing : PEC14,11.61,48,PEC14-LED-HO-LPW-WW.ies,PEC14-LED-HO-LPW-WW
PEC14-LED-HO-RAD-CW,34,5000,4181.00,Housing : PEC14,11.61,48,PEC14-LED-HO-RAD-CW.ies,PEC14-LED-HO-RAD-CW
PEC14-LED-HO-RAD-NW,34,4000,3764.00,Housing : PEC14,11.61,48,PEC14-LED-HO-RAD-NW.ies,PEC14-LED-HO-RAD-NW
PEC14-LED-HO-RAD-WW,34,3500,3465.00,Housing : PEC14,11.61,48,PEC14-LED-HO-RAD-WW.ies,PEC14-LED-HO-RAD-WW
PEC14-LED-SS-LPW-CW,33,5000,2615.00,Housing : PEC14,11.61,48,PEC14-LED-SS-LPW-CW.ies,PEC14-LED-SS-LPW-CW
PEC14-LED-SS-LPW-NW,33,4000,2282.00,Housing : PEC14,11.61,48,PEC14-LED-SS-LPW-NW.ies,PEC14-LED-SS-LPW-NW
PEC14-LED-SS-LPW-WW,33,3500,2397.00,Housing : PEC14,11.61,48,PEC14-LED-SS-LPW-WW.ies,PEC14-LED-SS-LPW-WW
PEC14-LED-SS-RAD-CW,27,5000,3485.00,Housing : PEC14,11.61,48,PEC14-LED-SS-RAD-CW.ies,PEC14-LED-SS-RAD-CW
PEC14-LED-SS-RAD-NW,27,4000,3148.00,Housing : PEC14,11.61,48,PEC14-LED-SS-RAD-NW.ies,PEC14-LED-SS-RAD-NW
PEC14-LED-SS-RAD-WW,29,3500,2946.00,Housing : PEC14,11.61,48,PEC14-LED-SS-RAD-WW.ies,PEC14-LED-SS-RAD-WW
PEC22-LED-HO-LPW-CW,45,5000,4148.00,Housing : PEC22,23.74,24,PEC22-LED-HO-LPW-CW.ies,PEC22-LED-HO-LPW-CW
PEC22-LED-HO-LPW-NW,45,4000,3638.00,Housing : PEC22,23.74,24,PEC22-LED-HO-LPW-NW.ies,PEC22-LED-HO-LPW-NW
PEC22-LED-HO-LPW-WW,45,3500,3502.00,Housing : PEC22,23.74,24,PEC22-LED-HO-LPW-WW.ies,PEC22-LED-HO-LPW-WW
PEC22-LED-HO-RAD-CW,45,5000,5372.00,Housing : PEC22,23.74,24,PEC22-LED-HO-RAD-CW.ies,PEC22-LED-HO-RAD-CW
PEC22-LED-HO-RAD-NW,44,4000,4654.00,Housing : PEC22,23.74,24,PEC22-LED-HO-RAD-NW.ies,PEC22-LED-HO-RAD-NW
PEC22-LED-HO-RAD-WW,45,3500,4572.00,Housing : PEC22,23.74,24,PEC22-LED-HO-RAD-WW.ies,PEC22-LED-HO-RAD-WW
PEC22-LED-HO-RPW-NW,45,4000,3146.00,Housing : PEC22,23.74,24,PEC22-LED-HO-RPW-NW.ies,PEC22-LED-HO-RPW-NW
PEC22-LED-HO-LW-NW,24,4000,2406.00,Housing : PEC22,23.74,24,PEC22-LED-LW-RAD-NW.ies,PEC22-LED-HO-LW-NW
PEC22-LED-SS-LPW-CW,35,5000,3210.00,Housing : PEC22,23.74,24,PEC22-LED-SS-LPW-CW.ies,PEC22-LED-SS-LPW-CW
PEC22-LED-SS-LPW-NW,35,4000,2821.00,Housing : PEC22,23.74,24,PEC22-LED-SS-LPW-NW.ies,PEC22-LED-SS-LPW-NW
PEC22-LED-SS-LPW-WW,35,3500,2728.00,Housing : PEC22,23.74,24,PEC22-LED-SS-LPW-WW.ies,PEC22-LED-SS-LPW-WW
PEC22-LED-SS-RAD-CW,35,5000,4130.00,Housing : PEC22,23.74,24,PEC22-LED-SS-RAD-CW.ies,PEC22-LED-SS-RAD-CW
PEC22-LED-SS-RAD-NW,34,4000,3534.00,Housing : PEC22,23.74,24,PEC22-LED-SS-RAD-NW.ies,PEC22-LED-SS-RAD-NW
PEC22-LED-SS-RAD-WW,35,3500,3489.00,Housing : PEC22,23.74,24,PEC22-LED-SS-RAD-WW.ies,PEC22-LED-SS-RAD-WW
PEC22-LED-SS-RPW-NW,35,4000,2390.00,Housing : PEC22,23.74,24,PEC22-LED-SS-RPW-NW.ies,PEC22-LED-SS-RPW-NW
PEC24-LED-HO-LPW-CW,55,5000,5527.00,Housing : PEC24,23.74,48,PEC24-LED-HO-LPW-CW.ies,PEC24-LED-HO-LPW-CW
PEC24-LED-HO-LPW-NW,55,4000,4833.00,Housing : PEC24,23.74,48,PEC24-LED-HO-LPW-NW.ies,PEC24-LED-HO-LPW-NW
PEC24-LED-HO-LPW-WW,55,3500,4595.00,Housing : PEC24,23.74,48,PEC24-LED-HO-LPW-WW.ies,PEC24-LED-HO-LPW-WW
PEC24-LED-HO-RAD-CW,55,5000,7128.00,Housing : PEC24,23.74,48,PEC24-LED-HO-RAD-CW.ies,PEC24-LED-HO-RAD-CW
PEC24-LED-HO-RAD-NW,55,4000,6198.00,Housing : PEC24,23.74,48,PEC24-LED-HO-RAD-NW.ies,PEC24-LED-HO-RAD-NW
PEC24-LED-HO-RAD-WW,55,3500,5934.00,Housing : PEC24,23.74,48,PEC24-LED-HO-RAD-WW.ies,PEC24-LED-HO-RAD-WW
PEC24-LED-HO-RPW-NW,58,4000,4472.00,Housing : PEC24,23.74,48,PEC24-LED-HO-RPW-NW.ies,PEC24-LED-HO-RPW-NW
PEC24-LED-HO-RPW-WW,58,3500,4224.00,Housing : PEC24,23.74,48,PEC24-LED-HO-RPW-WW.ies,PEC24-LED-HO-RPW-WW
PEC24-LED-SS-LPW-CW,44,5000,4527.00,Housing : PEC24,23.74,48,PEC24-LED-SS-LPW-CW.ies,PEC24-LED-SS-LPW-CW
PEC24-LED-SS-LPW-NW,44,4000,3951.00,Housing : PEC24,23.74,48,PEC24-LED-SS-LPW-NW.ies,PEC24-LED-SS-LPW-NW
PEC24-LED-SS-LPW-WW,44,3500,3838.00,Housing : PEC24,23.74,48,PEC24-LED-SS-LPW-WW.ies,PEC24-LED-SS-LPW-WW
PEC24-LED-SS-RAD-CW,44,5000,5841.00,Housing : PEC24,23.74,48,PEC24-LED-SS-RAD-CW.ies,PEC24-LED-SS-RAD-CW
PEC24-LED-SS-RAD-NW,44,4000,5065.00,Housing : PEC24,23.74,48,PEC24-LED-SS-RAD-NW.ies,PEC24-LED-SS-RAD-NW
PEC24-LED-SS-RAD-WW,44,3500,4866.00,Housing : PEC24,23.74,48,PEC24-LED-SS-RAD-WW.ies,PEC24-LED-SS-RAD-WW
PEC24-LED-VHO-LPW-CW,86,5000,8213.00,Housing : PEC24,23.74,48,PEC24-LED-VHO-LPW-CW.ies,PEC24-LED-VHO-LPW-CW
PEC24-LED-VHO-LPW-NW,86,4000,7219.00,Housing : PEC24,23.74,48,PEC24-LED-VHO-LPW-NW.ies,PEC24-LED-VHO-LPW-NW
PEC24-LED-VHO-LPW-WW,86,3500,7372.00,Housing : PEC24,23.74,48,PEC24-LED-VHO-LPW-WW.ies,PEC24-LED-VHO-LPW-WW
PEC24-LED-VHO-RAD-CW,86,5000,10923.00,Housing : PEC24,23.74,48,PEC24-LED-VHO-RAD-CW.ies,PEC24-LED-VHO-RAD-CW
PEC24-LED-VHO-RAD-NW,86,4000,9407.00,Housing : PEC24,23.74,48,PEC24-LED-VHO-RAD-NW.ies,PEC24-LED-VHO-RAD-NW
PEC24-LED-VHO-RAD-WW,86,3500,9748.00,Housing : PEC24,23.74,48,PEC24-LED-VHO-RAD-WW.ies,PEC24-LED-VHO-RAD-WW
