,Watts##ELECTRICAL_WATTAGE##WATTS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Luminous Flux##Electrical_Luminous_Flux##Lumens,Length##LENGTH##INCHES,Photometric File Name##OTHER##,Model##OTHER##
888-LED-HO-CW,0,5000,0,96,IES file not currently available,888-LED-HO-CW
888-LED-HO-NW,0,4000,0,96,IES file not currently available,888-LED-HO-NW
888-LED-HO-WW,0,3500,0,96,IES file not currently available,888-LED-HO-WW
888-LED-SS-CW,0,5000,0,96,IES file not currently available,888-LED-SS-CW
888-LED-SS-NW,0,4000,0,96,IES file not currently available,888-LED-SS-NW
888-LED-SS-WW,0,3500,0,96,IES file not currently available,888-LED-SS-WW
884-LED-HO-CW,43,5000,5827,48,884-LED-HO-CW.ies,884-LED-HO-CW
884-LED-HO-NW,43,4000,5079,48,884-LED-HO-NW.ies,884-LED-HO-NW
884-LED-HO-WW,43,3500,5223,48,884-LED-HO-WW.ies,884-LED-HO-WW
884-LED-SS-CW,29,5000,3795,48,884-LED-SS-CW.ies,884-LED-SS-CW
884-LED-SS-NW,29,4000,3185,48,884-LED-SS-NW.ies,884-LED-SS-NW
884-LED-SS-WW,29,3500,3250,48,884-LED-SS-WW.ies,884-LED-SS-WW
882-LED-SS-CW,29,5000,3457,24,882-LED-SS-CW.ies,882-LED-SS-CW
882-LED-SS-NW,29,4000,3056,24,882-LED-SS-NW.ies,882-LED-SS-NW
882-LED-SS-WW,29,3500,3110,24,882-LED-SS-WW.ies,882-LED-SS-WW
