,Watts##ELECTRICAL_WATTAGE##WATTS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Luminous Flux##Electrical_Luminous_Flux##Lumens,Photometric File Name##OTHER##,Length##LENGTH##INCHES,Model##OTHER##
RAIL-4-LED-FL-SS-30,41.5,3000,4672.9,RAIL-4-LED-FL-SS-30.ies,48,RAIL-4-LED-FL-SS-30
RAIL-4-LED-FL-SS-35,41.5,3500,4817.5,RAIL-4-LED-FL-SS-35.ies,48,RAIL-4-LED-FL-SS-35
RAIL-4-LED-FL-SS-40,41.5,4000,4981.9,RAIL-4-LED-FL-SS-40.ies,48,RAIL-4-LED-FL-SS-40
RAIL-4-LED-FL-HO-30,49.1,3000,5365.6,RAIL-4-LED-FL-HO-30.ies,48,RAIL-4-LED-FL-HO-30
RAIL-4-LED-FL-HO-35,49.1,3500,5531.8,RAIL-4-LED-FL-HO-35.ies,48,RAIL-4-LED-FL-HO-35
RAIL-4-LED-FL-HO-40,49.1,4000,5720.6,RAIL-4-LED-FL-HO-40.ies,48,RAIL-4-LED-FL-HO-40
RAIL-4-LED-FL-VHO-30,66.9,3000,6865.9,RAIL-4-LED-FL-VHO-30.ies,48,RAIL-4-LED-FL-VHO-30
RAIL-4-LED-FL-VHO-35,66.9,3500,7078.3,RAIL-4-LED-FL-VHO-35.ies,48,RAIL-4-LED-FL-VHO-35
RAIL-4-LED-FL-VHO-40,66.9,4000,7319.8,RAIL-4-LED-FL-VHO-40.ies,48,RAIL-4-LED-FL-VHO-40
RAIL-8-LED-FL-SS-30-S,0,3000,0,IES file not currently available,96,RAIL-8-LED-FL-SS-30-S
RAIL-8-LED-FL-SS-35-S,0,3500,0,IES file not currently available,96,RAIL-8-LED-FL-SS-35-S
RAIL-8-LED-FL-SS-40-S,0,4000,0,IES file not currently available,96,RAIL-8-LED-FL-SS-40-S
RAIL-8-LED-FL-HO-30-S,0,3000,0,IES file not currently available,96,RAIL-8-LED-FL-HO-30-S
RAIL-8-LED-FL-HO-35-S,0,3500,0,IES file not currently available,96,RAIL-8-LED-FL-HO-35-S
RAIL-8-LED-FL-HO-40-S,0,4000,0,IES file not currently available,96,RAIL-8-LED-FL-HO-40-S
RAIL-8-LED-FL-VHO-30-S,0,3000,0,IES file not currently available,96,RAIL-8-LED-FL-VHO-30-S
RAIL-8-LED-FL-VHO-35-S,0,3500,0,IES file not currently available,96,RAIL-8-LED-FL-VHO-35-S
RAIL-8-LED-FL-VHO-40-S,0,4000,0,IES file not currently available,96,RAIL-8-LED-FL-VHO-40-S
