,URL##OTHER##,Type Comments##OTHER##,Threshold Material##OTHER##,Thickness##LENGTH##FEET,Overall Length##LENGTH##FEET,OmniClass Number##OTHER##,Model##OTHER##,Manufacturer##OTHER##,Joint Width##LENGTH##FEET,Description##OTHER##,Default Elevation##LENGTH##FEET,Cover Material##OTHER##,Copyright ©##OTHER##,Bracket Material##OTHER##
8"" Joint Width,https://www.inprocorp.com/jointmaster-expansion-joint-systems/architectural-building-applications/exterior-expansion-joints,616 Series Exterior Seal 50% Movement Capable,Rubber-Inpro-EPDM_Membrane,1.213727999646,6.000000000000,23.20.30.24.21.14,616-A07/A09-200,Inpro®,0.666666666667,616 Series Exterior Expansion Joint Seal,0.000000000000,Thermoplastic-Inpro-Santoprene_Seals-Beige,Inpro Corporation,Aluminum-Inpro
10"" Joint Width,https://www.inprocorp.com/jointmaster-expansion-joint-systems/architectural-building-applications/exterior-expansion-joints,616 Series Exterior Seal 50% Movement Capable,Rubber-Inpro-EPDM_Membrane,1.213727999646,6.000000000000,23.20.30.24.21.14,616-A07/A09-250,Inpro®,0.833333333333,616 Series Exterior Expansion Joint Seal,0.000000000000,Thermoplastic-Inpro-Santoprene_Seals-Beige,Inpro Corporation,Aluminum-Inpro
12"" Joint Width,https://www.inprocorp.com/jointmaster-expansion-joint-systems/architectural-building-applications/exterior-expansion-joints,616 Series Exterior Seal 50% Movement Capable,Rubber-Inpro-EPDM_Membrane,1.213727999646,6.000000000000,23.20.30.24.21.14,616-A07/A09-300,Inpro®,1.000000000000,616 Series Exterior Expansion Joint Seal,0.000000000000,Thermoplastic-Inpro-Santoprene_Seals-Beige,Inpro Corporation,Aluminum-Inpro
18"" Joint Width,https://www.inprocorp.com/jointmaster-expansion-joint-systems/architectural-building-applications/exterior-expansion-joints,616 Series Exterior Seal 50% Movement Capable,Rubber-Inpro-EPDM_Membrane,1.213727999646,6.000000000000,23.20.30.24.21.14,616-A07/A09-450,Inpro®,1.500000000000,616 Series Exterior Expansion Joint Seal,0.000000000000,Thermoplastic-Inpro-Santoprene_Seals-Beige,Inpro Corporation,Aluminum-Inpro
24"" Joint Width,https://www.inprocorp.com/jointmaster-expansion-joint-systems/architectural-building-applications/exterior-expansion-joints,616 Series Exterior Seal 50% Movement Capable,Rubber-Inpro-EPDM_Membrane,1.213727999646,6.000000000000,23.20.30.24.21.14,616-A07/A09-600,Inpro®,2.000000000000,616 Series Exterior Expansion Joint Seal,0.000000000000,Thermoplastic-Inpro-Santoprene_Seals-Beige,Inpro Corporation,Aluminum-Inpro
