,Model##OTHER##,Joint Width##LENGTH##INCHES,Fire Rating##OTHER##,Type Comments##OTHER##,Sightline##LENGTH##INCHES,Overall Length##LENGTH##INCHES,OmniClass Title##OTHER##,OmniClass Number##OTHER##,Manufacturer##OTHER##,Length Error##OTHER##,Joint Depth##LENGTH##INCHES,Joint Control##LENGTH##INCHES,Flange Material##OTHER##,Fire Blanket Material##OTHER##,Fire Blanket Face Material##OTHER##,FB Width##LENGTH##INCHES,MasterFormat Number##OTHER##,Description##OTHER##,Default Elevation##LENGTH##INCHES,Copyright ©##OTHER##,CSI MasterFormat Title##OTHER##,Assembly Code##OTHER##,URL##OTHER##
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-1HR-18"""" Joint",F520-1BM-18FL,18,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,20.625,19.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-1HR-16"""" Joint",F520-1BM-16FL,16,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,18.625,17.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-1HR-14"""" Joint",F520-1BM-14FL,14,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,16.625,15.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-1HR-12"""" Joint",F520-1BM-12FL,12,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,14.625,13.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-1HR-10"""" Joint",F520-1BM-10FL,10,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,12.625,11.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-1HR-8"""" Joint",F520-1BM-8FL,8,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,10.625,9.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-1HR-6"""" Joint",F520-1BM-6FL,6,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,8.625,7.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-1HR-2"""" Joint",F520-1BM-2FL,2,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,4.625,3.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-1HR-4"""" Joint",F520-1BM-4FL,4,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,6.625,5.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-2HR-2"""" Joint",F520-2BM-2FL,2,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,4.625,3.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-2HR-4"""" Joint",F520-2BM-4FL,4,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,6.625,5.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-2HR-6"""" Joint",F520-2BM-6FL,6,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,8.625,7.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-2HR-8"""" Joint",F520-2BM-8FL,8,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,10.625,9.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-2HR-10"""" Joint",F520-2BM-10FL,10,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,12.625,11.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-2HR-12"""" Joint",F520-2BM-12FL,12,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,14.625,13.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-2HR-14"""" Joint",F520-2BM-14FL,14,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,16.625,15.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-2HR-16"""" Joint",F520-2BM-16FL,16,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,18.625,17.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-2HR-18"""" Joint",F520-2BM-18FL,18,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,20.625,19.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-3HR-2"""" Joint",F520-3BM-2FL,2,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,4.625,3.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-3HR-4"""" Joint",F520-3BM-4FL,4,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,6.625,5.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-3HR-6"""" Joint",F520-3BM-6FL,6,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,8.625,7.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-3HR-8"""" Joint",F520-3BM-8FL,8,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,10.625,9.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-3HR-10"""" Joint",F520-3BM-10FL,10,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,12.625,11.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-3HR-12"""" Joint",F520-3BM-12FL,12,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,14.625,13.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-3HR-14"""" Joint",F520-3BM-14FL,14,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,16.625,15.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-3HR-16"""" Joint",F520-3BM-16FL,16,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,18.625,17.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorFloor-3HR-18"""" Joint",F520-3BM-18FL,18,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,20.625,19.125,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
