,Model##OTHER##,Joint Width##LENGTH##INCHES,Fire Rating##OTHER##,Type Comments##OTHER##,Sightline##LENGTH##INCHES,Overall Length##LENGTH##INCHES,OmniClass Title##OTHER##,OmniClass Number##OTHER##,Manufacturer##OTHER##,Length Error##OTHER##,Flange Material##OTHER##,Fire Blanket Material##OTHER##,Fire Blanket Face Material##OTHER##,FB Width##LENGTH##INCHES,MasterFormat Number##OTHER##,Description##OTHER##,Default Elevation##LENGTH##INCHES,Copyright ©##OTHER##,CSI MasterFormat Title##OTHER##,Assembly Code##OTHER##,URL##OTHER##
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-1HR-18"""" Joint",F520-1BM-18FW,18,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-1HR-16"""" Joint",F520-1BM-16FW,16,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-1HR-14"""" Joint",F520-1BM-14FW,14,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-1HR-12"""" Joint",F520-1BM-12FW,12,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-1HR-10"""" Joint",F520-1BM-10FW,10,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-1HR-8"""" Joint",F520-1BM-8FW,8,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-1HR-6"""" Joint",F520-1BM-6FW,6,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-1HR-4"""" Joint",F520-1BM-4FW,4,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-1HR-2"""" Joint",F520-1BM-2FW,2,1HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-2HR-2"""" Joint",F520-2BM-2FW,2,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-2HR-4"""" Joint",F520-2BM-4FW,4,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-2HR-6"""" Joint",F520-2BM-6FW,6,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-2HR-8"""" Joint",F520-2BM-8FW,8,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-2HR-10"""" Joint",F520-2BM-10FW,10,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-2HR-12"""" Joint",F520-2BM-12FW,12,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-2HR-14"""" Joint",F520-2BM-14FW,14,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-2HR-16"""" Joint",F520-2BM-16FW,16,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-2HR-18"""" Joint",F520-2BM-18FW,18,2HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-3HR-2"""" Joint",F520-3BM-2FW,2,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-3HR-4"""" Joint",F520-3BM-4FW,4,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-3HR-6"""" Joint",F520-3BM-6FW,6,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-3HR-8"""" Joint",F520-3BM-8FW,8,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-3HR-10"""" Joint",F520-3BM-10FW,10,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-3HR-12"""" Joint",F520-3BM-12FW,12,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-3HR-14"""" Joint",F520-3BM-14FW,14,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-3HR-16"""" Joint",F520-3BM-16FW,16,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
"Fire_Blanket_F520_Series-Inpro-Bottom_Mount-FloorWall-3HR-18"""" Joint",F520-3BM-18FW,18,3HR,50% movement capable - Max 10' length - Available in 1:2:3 HR ratings,24,36,Expansion Joint,23.20.30.24.21.14,Inpro,0,Metal-Steel-Inpro,Fire Blanket-Insulation-Inpro,Fire Blanket-Fabric-Inpro,1.5,07 95 00,520 Fireblanket,0,Inpro Corporation,Expansion Joint Cover Assemblies,F1030,https://inprocorp.com/jointmaster-expansion-joint-systems/parking-open-air-structures/fire-barrier-systems/fire-blanket-systems/fireline-520-series
