,Placement##OTHER##,Fire Rating##OTHER##,Joint Width##LENGTH##INCHES,Length##LENGTH##INCHES,Description##OTHER##,Type Comments##OTHER##,OmniClass Number##OTHER##,Manufacturer##OTHER##,Assembly Code##OTHER##
Fire_Blanket-F520_Series-Inpro-2_Hour-4in-TM-FloorFloor,Horizontal,2HR,4,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-2_Hour-6in-TM-FloorFloor,Horizontal,2HR,6,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3 and 4hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-2_Hour-8in-TM-FloorFloor,Horizontal,2HR,8,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-2_Hour-10in-TM-FloorFloor,Horizontal,2HR,10,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-2_Hour-12in-TM-FloorFloor,Horizontal,2HR,12,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-2_Hour-14in-TM-FloorFloor,Horizontal,2HR,14,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-2_Hour-16in-TM-FloorFloor,Horizontal,2HR,16,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-2_Hour-18in-TM-FloorFloor,Horizontal,2HR,18,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-3_Hour-4in-TM-FloorFloor,Horizontal,3HR,4,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-3_Hour-6in-TM-FloorFloor,Horizontal,3HR,6,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-3_Hour-8in-TM-FloorFloor,Horizontal,3HR,8,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-3_Hour-10in-TM-FloorFloor,Horizontal,3HR,10,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-3_Hour-12in-TM-FloorFloor,Horizontal,3HR,12,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-3_Hour-14in-TM-FloorFloor,Horizontal,3HR,14,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-3_Hour-16in-TM-FloorFloor,Horizontal,3HR,16,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-3_Hour-18in-TM-FloorFloor,Horizontal,3HR,18,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-2_Hour-4in-TM-WallWall,Vertical,2HR,4,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-2_Hour-6in-TM-WallWall,Vertical,2HR,6,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3 and 4hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-2_Hour-8in-TM-WallWall,Vertical,2HR,8,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-2_Hour-10in-TM-WallWall,Vertical,2HR,10,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-2_Hour-12in-TM-WallWall,Vertical,2HR,12,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-2_Hour-14in-TM-WallWall,Vertical,2HR,14,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-2_Hour-16in-TM-WallWall,Vertical,2HR,16,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-2_Hour-18in-TM-WallWall,Vertical,2HR,18,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-3_Hour-4in-TM-WallWall,Vertical,3HR,4,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-3_Hour-6in-TM-WallWall,Vertical,3HR,6,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-3_Hour-8in-TM-WallWall,Vertical,3HR,8,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-3_Hour-10in-TM-WallWall,Vertical,3HR,10,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-3_Hour-12in-TM-WallWall,Vertical,3HR,12,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-3_Hour-14in-TM-WallWall,Vertical,3HR,14,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-3_Hour-16in-TM-WallWall,Vertical,3HR,16,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
Fire_Blanket-F520_Series-Inpro-3_Hour-18in-TM-WallWall,Vertical,3HR,18,120,FireBlanket,"50 percent movement capable, Max 10' Length, Available in 1,2,3hr ratings and 2"" joints",23.20.50.11.14,Inpro,F1030
