,Model##OTHER##,Joint Width##LENGTH##INCHES,Fire Rating##OTHER##,Void Depth##LENGTH##INCHES,URL##OTHER##,Type Comments##OTHER##,OmniClass Title##OTHER##,OmniClass Number##OTHER##,MasterFormat Number##OTHER##,Flange Material##OTHER##,Flange Length Right##LENGTH##INCHES,Flange Length Left##LENGTH##INCHES,Flange Inset##LENGTH##INCHES,Fire Blanket Material##OTHER##,Fire Blanket Face Material##OTHER##,CSI MasterFormat Title##OTHER##,Blockout Depth##LENGTH##INCHES,Manufacturer##OTHER##,Length##LENGTH##INCHES,Joint Depth##LENGTH##INCHES,Length Error##OTHER##,FB Width##LENGTH##INCHES,Description##OTHER##,Default Elevation##LENGTH##INCHES,Copyright Š##OTHER##,Assembly Code##OTHER##
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-1HR-2"""" Joint",F520-1TM-2FW,2,1HR,5,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1,2,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,2,0,0.9375,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-1HR-4"""" Joint",F520-1TM-4FW,4,1HR,7,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,4,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-1HR-6"""" Joint",F520-1TM-6FW,6,1HR,9,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,6,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-1HR-8"""" Joint",F520-1TM-8FW,8,1HR,11,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,8,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-1HR-10"""" Joint",F520-1TM-10FW,10,1HR,13,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,10,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-1HR-12"""" Joint",F520-1TM-12FW,12,1HR,15,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,12,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-1HR-14"""" Joint",F520-1TM-14FW,14,1HR,17,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,14,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-1HR-16"""" Joint",F520-1TM-16FW,16,1HR,19,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,16,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-1HR-18"""" Joint",F520-1TM-18FW,18,1HR,21,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,18,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-2HR-2"""" Joint",F520-2TM-2FW,2,2HR,5,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1,2,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,2,0,0.9375,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-2HR-4"""" Joint",F520-2TM-4FW,4,2HR,7,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,4,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-2HR-6"""" Joint",F520-2TM-6FW,6,2HR,9,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,6,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-2HR-8"""" Joint",F520-2TM-8FW,8,2HR,11,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,8,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-2HR-10"""" Joint",F520-2TM-10FW,10,2HR,13,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,10,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-2HR-12"""" Joint",F520-2TM-12FW,12,2HR,15,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,12,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-2HR-14"""" Joint",F520-2TM-14FW,14,2HR,17,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,14,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-2HR-16"""" Joint",F520-2TM-16FW,16,2HR,19,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,16,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-2HR-18"""" Joint",F520-2TM-18FW,18,2HR,21,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,18,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-3HR-2"""" Joint",F520-3TM-2FW,2,3HR,5,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1,2,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,2,0,0.9375,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-3HR-4"""" Joint",F520-3TM-4FW,4,3HR,7,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,4,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-3HR-6"""" Joint",F520-3TM-6FW,6,3HR,9,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,6,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-3HR-8"""" Joint",F520-3TM-8FW,8,3HR,11,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,8,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-3HR-10"""" Joint",F520-3TM-10FW,10,3HR,13,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,10,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-3HR-12"""" Joint",F520-3TM-12FW,12,3HR,15,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,12,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-3HR-14"""" Joint",F520-3TM-14FW,14,3HR,17,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,14,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-3HR-16"""" Joint",F520-3TM-16FW,16,3HR,19,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,16,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-FloorWall-3HR-18"""" Joint",F520-3TM-18FW,18,3HR,21,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,18,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-1HR-2"""" Joint",F520-1TM-2WC,2,1HR,5,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1,2,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,2,0,0.9375,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-1HR-4"""" Joint",F520-1TM-4WC,4,1HR,7,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,4,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-1HR-6"""" Joint",F520-1TM-6WC,6,1HR,9,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,6,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WalllCorner-1HR-8"""" Joint",F520-1TM-8WC,8,1HR,11,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,8,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-1HR-10"""" Joint",F520-1TM-10WC,10,1HR,13,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,10,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-1HR-12"""" Joint",F520-1TM-12WC,12,1HR,15,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,12,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-1HR-14"""" Joint",F520-1TM-14WC,14,1HR,17,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,14,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-1HR-16"""" Joint",F520-1TM-16WC,16,1HR,19,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,16,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-1HR-18"""" Joint",F520-1TM-18WC,18,1HR,21,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,18,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-2HR-2"""" Joint",F520-2TM-2WC,2,2HR,5,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1,2,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,2,0,0.9375,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-2HR-4"""" Joint",F520-2TM-4WC,4,2HR,7,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,4,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-2HR-6"""" Joint",F520-2TM-6WC,6,2HR,9,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,6,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-2HR-8"""" Joint",F520-2TM-8WC,8,2HR,11,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,8,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-2HR-10"""" Joint",F520-2TM-10WC,10,2HR,13,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,10,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-2HR-12"""" Joint",F520-2TM-12WC,12,2HR,15,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,12,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WalllCorner-2HR-14"""" Joint",F520-2TM-14WC,14,2HR,17,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,14,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-2HR-16"""" Joint",F520-2TM-16WC,16,2HR,19,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,16,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-2HR-18"""" Joint",F520-2TM-18WC,18,2HR,21,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,18,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-3HR-2"""" Joint",F520-3TM-2WC,2,3HR,5,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1,2,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,2,0,0.9375,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-3HR-4"""" Joint",F520-3TM-4WC,4,3HR,7,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,4,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-3HR-6"""" Joint",F520-3TM-6WC,6,3HR,9,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,6,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-3HR-8"""" Joint",F520-3TM-8WC,8,3HR,11,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,8,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-3HR-10"""" Joint",F520-3TM-10WC,10,3HR,13,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,10,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-3HR-12"""" Joint",F520-3TM-12WC,12,3HR,15,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,12,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-3HR-14"""" Joint",F520-3TM-14WC,14,3HR,17,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,14,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-3HR-16"""" Joint",F520-3TM-16WC,16,3HR,19,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,16,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
"Fire_Blanket-F520_Series-Inpro-TM-WallCorner-3HR-18"""" Joint",F520-3TM-18WC,18,3HR,21,https://www.inprocorp.com/jointmaster-expansion-joint-systems,50 percent movement capable - Max 10' Length - Available in 1:2:3hr ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,1.96875,2.96875,2,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,18,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030
