,Model##OTHER##,Joint Width##LENGTH##INCHES,Fire Rating##OTHER##,Void Depth##LENGTH##INCHES,Type Comments##OTHER##,OmniClass Title##OTHER##,OmniClass Number##OTHER##,MasterFormat Number##OTHER##,Flange Material##OTHER##,Flange Inset##LENGTH##INCHES,Flange Height##LENGTH##INCHES,Fire Blanket Material##OTHER##,Fire Blanket Face Material##OTHER##,CSI MasterFormat Title##OTHER##,Blockout Depth##LENGTH##INCHES,Manufacturer##OTHER##,Length##LENGTH##INCHES,Joint Depth##LENGTH##INCHES,Length Error##OTHER##,FB Width##LENGTH##INCHES,Description##OTHER##,Default Elevation##LENGTH##INCHES,Copyright Š##OTHER##,Assembly Code##OTHER##,URL##OTHER##
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-1HR-4"""" Joint",F520-1IM-4FL,4,1HR,7,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,4,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-1HR-2"""" Joint",F520-1IM-2FL,2,1HR,5,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,2,0,0.9375,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-1HR-6"""" Joint",F520-1IM-6FL,6,1HR,9,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,6,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-1HR-8"""" Joint",F520-1IM-8FL,8,1HR,11,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,8,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-1HR-10"""" Joint",F520-1IM-10FL,10,1HR,13,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,10,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-1HR-12"""" Joint",F520-1IM-12FL,12,1HR,15,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,12,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-1HR-14"""" Joint",F520-1IM-14FL,14,1HR,17,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,14,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-1HR-16"""" Joint",F520-1IM-16FL,16,1HR,19,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,16,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-1HR-18"""" Joint",F520-1IM-18FL,18,1HR,21,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,18,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-2HR-2"""" Joint",F520-2IM-2FL,2,2HR,5,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,2,0,0.9375,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-2HR-4"""" Joint",F520-2IM-4FL,4,2HR,7,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,4,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-2HR-6"""" Joint",F520-2IM-6FL,6,2HR,9,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,6,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-2HR-8"""" Joint",F520-2IM-8FL,8,2HR,11,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,8,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-2HR-10"""" Joint",F520-2IM-10FL,10,2HR,13,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,10,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-2HR-12"""" Joint",F520-2IM-12FL,12,2HR,15,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,12,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-2HR-14"""" Joint",F520-2IM-14FL,14,2HR,17,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,14,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-2HR-16"""" Joint",F520-2IM-16FL,16,2HR,19,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,16,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-2HR-18"""" Joint",F520-2IM-18FL,18,2HR,21,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,18,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-3HR-2"""" Joint",F520-3IM-2FL,2,3HR,5,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,2,0,0.9375,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-3HR-4"""" Joint",F520-3IM-4FL,4,3HR,7,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,4,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-3HR-6"""" Joint",F520-3IM-6FL,6,3HR,9,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,6,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-3HR-8"""" Joint",F520-3IM-8FL,8,3HR,11,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,8,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-3HR-10"""" Joint",F520-3IM-10FL,10,3HR,13,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,10,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-3HR-12"""" Joint",F520-3IM-12FL,12,3HR,15,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,12,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-3HR-14"""" Joint",F520-3IM-14FL,14,3HR,17,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,14,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-3HR-16"""" Joint",F520-3IM-16FL,16,3HR,19,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,16,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-FloorFloor-3HR-18"""" Joint",F520-3IM-18FL,18,3HR,21,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,18,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-1HR-2"""" Joint",F520-1IM-2WL,2,1HR,5,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,2,0,0.9375,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-1HR-4"""" Joint",F520-1IM-4WL,4,1HR,7,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,4,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-1HR-6"""" Joint",F520-1IM-6WL,6,1HR,9,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,6,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-1HR-8"""" Joint",F520-1IM-8WL,8,1HR,11,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,8,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-1HR-10"""" Joint",F520-1IM-10WL,10,1HR,13,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,10,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-1HR-12"""" Joint",F520-1IM-12WL,12,1HR,15,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,12,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-1HR-14"""" Joint",F520-1IM-14WL,14,1HR,17,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,14,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-1HR-16"""" Joint",F520-1IM-16WL,16,1HR,19,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,16,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-1HR-18"""" Joint",F520-1IM-18WL,18,1HR,21,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,18,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-2HR-2"""" Joint",F520-2IM-2WL,2,2HR,5,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,2,0,0.9375,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-2HR-4"""" Joint",F520-2IM-4WL,4,2HR,7,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,4,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-2HR-6"""" Joint",F520-2IM-6WL,6,2HR,9,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,6,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-2HR-8"""" Joint",F520-2IM-8WL,8,2HR,11,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,8,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-2HR-10"""" Joint",F520-2IM-10WL,10,2HR,13,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,10,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-2HR-12"""" Joint",F520-2IM-12WL,12,2HR,15,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,12,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-2HR-14"""" Joint",F520-2IM-14WL,14,2HR,17,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,14,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-2HR-16"""" Joint",F520-2IM-16WL,16,2HR,19,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,16,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-2HR-18"""" Joint",F520-2IM-18WL,18,2HR,21,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,18,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-3HR-2"""" Joint",F520-3IM-2WL,2,3HR,5,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,2,0,0.9375,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-3HR-4"""" Joint",F520-3IM-4WL,4,3HR,7,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,4,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-3HR-6"""" Joint",F520-3IM-6WL,6,3HR,9,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,6,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-3HR-8"""" Joint",F520-3IM-8WL,8,3HR,11,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,8,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-3HR-10"""" Joint",F520-3IM-10WL,10,3HR,13,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,10,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-3HR-12"""" Joint",F520-3IM-12WL,12,3HR,15,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,12,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-3HR-14"""" Joint",F520-3IM-14WL,14,3HR,17,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,14,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-3HR-16"""" Joint",F520-3IM-16WL,16,3HR,19,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,16,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
"Fire_Blanket-F520_Series-Inpro-IM-WallWall-3HR-18"""" Joint",F520-3IM-18WL,18,3HR,21,50 percent movement capable - Max 10' Length - Available in 1:2:3 HR ratings,Expansion Joint,23.20.50.11.14,07 95 00,Metal-Steel-Bare-Inpro,2,1.96875,Insulation-FireBlanket-Inpro,Fabric-Fire Blanket-Inpro,Expansion Joint Cover Assemblies,1,InproŽ,36,18,0,1.5,520 FireBlanket,0,Inpro Corporation,F1030,https://www.inprocorp.com/jointmaster-expansion-joint-systems
