
Luxboxx Vapor Echo Large (Downward and Upward Shining) - LX-VE-L-DU


Use the IES file, in conjunction with the 3DS file of the luminaire shade, to perform
light modelling using a program such as DIALux.

Place the LED panel from the IES file at the following position within the 3DS shade file:

X and Y axis: Centred within shade.

Z axis: Recess the downward shining LED panel 400mm from the bottom edge of the shade.
	Recess the upward shining LED panel 500mm from the bottom edge of the shade.