900.34.01SXA
Ceiling hanger, System 900
- straight rail with fixing trim
- for mounting curtain rods
- made of high-quality stainless steel matt sanded
- length made to measure from 11 7/8 inch (301 mm) to 59 1/16 inch (1500 mm)
- rail diameter 1 inch (25 mm), rose diameter 2 3/4 inch (70 mm)
- can be shortened at the rose to 7 7/8 inch (200 mm) on site
- mounted to ceiling with rose
- including non-corrosive fixing material and sealing tape for sealing the drilling points

Article no.: HEWI 900.34.01SXA

