900.51.214XA
Fold-away seat, System 900
- construction consisting of wall bracket and continuous seat
- slip-resistant, textured seat made of synthetic material in HEWI colors 98 (signal white) and 92 (anthracite gray)
- reinforcement of the seat made of aluminum, powder coated in the colour of the seat
- wall bracket made of stainless steel, satin
- seat with hygiene cutout can be folded up to save space
- seat depth when folded up 3 inch (77 mm)
- load capacity up to 330 lbs (150 kg)
- with floor support for seat height 17 11/16 - 19 11/16 inch (450-500 mm), powder coated in the colour of the seat)
- 17 3/4 inch (450 mm) wide, 20 11/16 inch (525 mm) deep and 4 7/16 inch (112 mm) high
- seat area 17 3/4 inch (450 mm) wide and 17 3/4 inch (450 mm) deep
- for mounting with non-corrosive and tested HEWI fixing materials for different wall systems (to be ordered separately)
- sealing tape for sealing the fixing points is included in the scope of supply
- fulfils the DIN 18040, ÖNORM B1600/1601 and SIA 500 requirements

Article no.: HEWI 900.51.214XA

