950.50.62040
Hinged support rail Duo
- with two gripping levels arranged above each other
- upper rail is merged with the top rail at an angle of 135°
- upper rail made of rectangular profile, 40 mm wide and 30 mm, provides a wide support surface and large radii for pleasant gripping, used to hold on tight and for support
- bottom rail (diameter 25 mm) starts at a distance of 250 mm from the front edge of the upper rail and is used for holding on to and for turning in from the side
- 700 mm projection, wall mounting plate 181 mm high and 130 mm wide
- can be folded upwards and, folded downwards with braking mechanism
- made of metal, high-quality chrome-plated
- wall-mounting plate cover made of high-quality chrome-plated synthetic material
- stable three-point fixing
- for wall mounting with concealed, non-corrosive and tested fixing materials for different wall systems
- with toilet roll holder 950.50.01150, toilet roll holder with WC flushing mechanism and function button (radio-controlled) 950.50.06490 (right), 950.50.06590 (left), floor supports 950.50.020XA, 950.50.025XA, 950.50.026XA and arm pad 950.50.03192 for retrofitting
- CE marking according to Directive 93/42 / EEC
- fulfils the ÖNORM B1600/1601 and SIA 500 requirements
- weight capacity 100 kg

Article no.: HEWI 950.50.62040

