801.35B340
Range 801 Rail with vertical support bar and sliding shower head holder
- vertical and horizontal rails joined to form an L shape and fitted with rose fixings and a shower head holder
- with vertical rail with shower head holder that can be moved to the side (for installation)
- vertical length of 1250 mm, horizontal lengths 762 mm
- 90 mm deep, rail diameter 33 mm, rose diameter 70 mm
- suitable for shower heads of various manufacturers
- shower head holder can be continuously tilted and, after pulling or pushing a large lever, its height can be adjusted
- functional area of the shower head holder in high-quality, glossy polyamide
- conical adapter on shower head holder makes it easier to hook in the handheld shower head
- with continuous, corrosion resistant steel core
- for wall mounting with special HEWI fixing materials and roses
- can be mounted in left hand or right hand position
- made of high-quality matt polyamide in HEWI colours 99 (pure white), 98 (signal white), 97 (light grey), 95 (stone grey) and 92 (anthracite grey)
- with continuous, corrosion resistant steel core
- suitable for HEWI hanging seats 950.51...10..., 950.51...11..., 802.51...11..., 802.51...12... and 801.51...100 (only on W2)

Article no.: HEWI 801.35B340

