900.35.40040
Shower handrail with sliding shower head rail, System 900
- vertical and horizontally arranged rails connected at right angles with mounting roses and shower head holder 
- with shower head rail that can be pushed to the side (for installation)
- vertical length 1250 mm, horizontal lengths 765 mm, 88 mm deep
- rail diameter 32 mm, tube thickness 2 mm, rose diameter 70 mm
- made of high-quality stainless steel, chrome
- shower head holder made of high-quality matt polyamide in the HEWI colours 98 (signal white) and 92 (anthracite grey)
- suitable for shower heads of various manufacturers
- shower head holder can be tilted continuously and, after pressing a large pushbutton, its height can be adjusted
- conical adapter on shower head holder makes it easier to hook in the shower head
- including non-corrosive and tested HEWI fixing material for wall mounting and sealing tape for sealing the drilling points
- suitable for HEWI System 900 hook-on seats

Article no.: HEWI 900.35.40040

