,Basic Model##Other##,Model##Other##,Width##Length##inches,Height##Length##inches,Finish 1##Other##,Power & Comm##Other##,Top Cap Style##Other##,Description##Other##,Option##Other##,Cover Value##Other##,Has Top Cap##Other##,Screen Core##Other##
"48Wx48H,Magnetic,Non-Powered,Flat Top Cap",TSSNE4848,TSSNE4848,48,48,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Non-Powered,No Top Cap",TSSNE4848,TSSNE4848:NC:N,48,48,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE4848,TSSNE4848:DN:F,48,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE4848,TSSNE4848:DN:N,48,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE4848,TSSNE4848:DC:F,48,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE4848,TSSNE4848:DC:N,48,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Non-Powered,Flat Top Cap",TSSNE5448,TSSNE5448,54,48,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Non-Powered,No Top Cap",TSSNE5448,TSSNE5448:NC:N,54,48,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE5448,TSSNE5448:DN:F,54,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE5448,TSSNE5448:DN:N,54,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE5448,TSSNE5448:DC:F,54,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE5448,TSSNE5448:DC:N,54,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Non-Powered,Flat Top Cap",TSSNE6048,TSSNE6048,60,48,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Non-Powered,No Top Cap",TSSNE6048,TSSNE6048:NC:N,60,48,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE6048,TSSNE6048:DN:F,60,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE6048,TSSNE6048:DN:N,60,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE6048,TSSNE6048:DC:F,60,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE6048,TSSNE6048:DC:N,60,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Non-Powered,Flat Top Cap",TSSNE6648,TSSNE6648,66,48,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Non-Powered,No Top Cap",TSSNE6648,TSSNE6648:NC:N,66,48,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE6648,TSSNE6648:DN:F,66,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE6648,TSSNE6648:DN:N,66,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE6648,TSSNE6648:DC:F,66,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE6648,TSSNE6648:DC:N,66,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Non-Powered,Flat Top Cap",TSSNE7248,TSSNE7248,72,48,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Non-Powered,No Top Cap",TSSNE7248,TSSNE7248:NC:N,72,48,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE7248,TSSNE7248:DN:F,72,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE7248,TSSNE7248:DN:N,72,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE7248,TSSNE7248:DC:F,72,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE7248,TSSNE7248:DC:N,72,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Non-Powered,Flat Top Cap",TSSNE7848,TSSNE7848,78,48,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Non-Powered,No Top Cap",TSSNE7848,TSSNE7848:NC:N,78,48,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE7848,TSSNE7848:DN:F,78,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE7848,TSSNE7848:DN:N,78,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE7848,TSSNE7848:DC:F,78,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE7848,TSSNE7848:DC:N,78,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Non-Powered,Flat Top Cap",TSSNE8448,TSSNE8448,84,48,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Non-Powered,No Top Cap",TSSNE8448,TSSNE8448:NC:N,84,48,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE8448,TSSNE8448:DN:F,84,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE8448,TSSNE8448:DN:N,84,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE8448,TSSNE8448:DC:F,84,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE8448,TSSNE8448:DC:N,84,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Non-Powered,Flat Top Cap",TSSNE9048,TSSNE9048,90,48,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Non-Powered,No Top Cap",TSSNE9048,TSSNE9048:NC:N,90,48,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE9048,TSSNE9048:DN:F,90,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE9048,TSSNE9048:DN:N,90,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE9048,TSSNE9048:DC:F,90,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE9048,TSSNE9048:DC:N,90,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Non-Powered,Flat Top Cap",TSSNE9648,TSSNE9648,96,48,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Non-Powered,No Top Cap",TSSNE9648,TSSNE9648:NC:N,96,48,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE9648,TSSNE9648:DN:F,96,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE9648,TSSNE9648:DN:N,96,48,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE9648,TSSNE9648:DC:F,96,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE9648,TSSNE9648:DC:N,96,48,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Non-Powered,Flat Top Cap",TSSNE4854,TSSNE4854,48,54,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Non-Powered,No Top Cap",TSSNE4854,TSSNE4854:NC:N,48,54,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE4854,TSSNE4854:DN:F,48,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE4854,TSSNE4854:DN:N,48,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE4854,TSSNE4854:DC:F,48,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE4854,TSSNE4854:DC:N,48,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Non-Powered,Flat Top Cap",TSSNE5454,TSSNE5454,54,54,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Non-Powered,No Top Cap",TSSNE5454,TSSNE5454:NC:N,54,54,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE5454,TSSNE5454:DN:F,54,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE5454,TSSNE5454:DN:N,54,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE5454,TSSNE5454:DC:F,54,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE5454,TSSNE5454:DC:N,54,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Non-Powered,Flat Top Cap",TSSNE6054,TSSNE6054,60,54,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Non-Powered,No Top Cap",TSSNE6054,TSSNE6054:NC:N,60,54,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE6054,TSSNE6054:DN:F,60,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE6054,TSSNE6054:DN:N,60,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE6054,TSSNE6054:DC:F,60,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE6054,TSSNE6054:DC:N,60,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Non-Powered,Flat Top Cap",TSSNE6654,TSSNE6654,66,54,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Non-Powered,No Top Cap",TSSNE6654,TSSNE6654:NC:N,66,54,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE6654,TSSNE6654:DN:F,66,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE6654,TSSNE6654:DN:N,66,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE6654,TSSNE6654:DC:F,66,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE6654,TSSNE6654:DC:N,66,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Non-Powered,Flat Top Cap",TSSNE7254,TSSNE7254,72,54,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Non-Powered,No Top Cap",TSSNE7254,TSSNE7254:NC:N,72,54,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE7254,TSSNE7254:DN:F,72,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE7254,TSSNE7254:DN:N,72,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE7254,TSSNE7254:DC:F,72,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE7254,TSSNE7254:DC:N,72,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Non-Powered,Flat Top Cap",TSSNE7854,TSSNE7854,78,54,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Non-Powered,No Top Cap",TSSNE7854,TSSNE7854:NC:N,78,54,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE7854,TSSNE7854:DN:F,78,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE7854,TSSNE7854:DN:N,78,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE7854,TSSNE7854:DC:F,78,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE7854,TSSNE7854:DC:N,78,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Non-Powered,Flat Top Cap",TSSNE8454,TSSNE8454,84,54,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Non-Powered,No Top Cap",TSSNE8454,TSSNE8454:NC:N,84,54,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE8454,TSSNE8454:DN:F,84,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE8454,TSSNE8454:DN:N,84,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE8454,TSSNE8454:DC:F,84,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE8454,TSSNE8454:DC:N,84,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Non-Powered,Flat Top Cap",TSSNE9054,TSSNE9054,90,54,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Non-Powered,No Top Cap",TSSNE9054,TSSNE9054:NC:N,90,54,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE9054,TSSNE9054:DN:F,90,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE9054,TSSNE9054:DN:N,90,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE9054,TSSNE9054:DC:F,90,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE9054,TSSNE9054:DC:N,90,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Non-Powered,Flat Top Cap",TSSNE9654,TSSNE9654,96,54,Magnetic Dry-Erasable Steel,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Non-Powered,No Top Cap",TSSNE9654,TSSNE9654:NC:N,96,54,Magnetic Dry-Erasable Steel,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Data Cutout Side 1,Flat Top Cap",TSSNE9654,TSSNE9654:DN:F,96,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Data Cutout Side 1,No Top Cap",TSSNE9654,TSSNE9654:DN:N,96,54,Magnetic Dry-Erasable Steel,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Data Cutout Both Sides,Flat Top Cap",TSSNE9654,TSSNE9654:DC:F,96,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Data Cutout Both Sides,No Top Cap",TSSNE9654,TSSNE9654:DC:N,96,54,Magnetic Dry-Erasable Steel,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Markerboard
"48Wx48H,Laminate,Non-Powered,Flat Top Cap",TSSNM4848,TSSNM4848,48,48,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Non-Powered,No Top Cap",TSSNM4848,TSSNM4848:NC:N,48,48,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM4848,TSSNM4848:DN:F,48,48,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM4848,TSSNM4848:DN:N,48,48,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM4848,TSSNM4848:DC:F,48,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM4848,TSSNM4848:DC:N,48,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Non-Powered,Flat Top Cap",TSSNM5448,TSSNM5448,54,48,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Non-Powered,No Top Cap",TSSNM5448,TSSNM5448:NC:N,54,48,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM5448,TSSNM5448:DN:F,54,48,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM5448,TSSNM5448:DN:N,54,48,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM5448,TSSNM5448:DC:F,54,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM5448,TSSNM5448:DC:N,54,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Non-Powered,Flat Top Cap",TSSNM6048,TSSNM6048,60,48,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Non-Powered,No Top Cap",TSSNM6048,TSSNM6048:NC:N,60,48,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM6048,TSSNM6048:DN:F,60,48,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM6048,TSSNM6048:DN:N,60,48,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM6048,TSSNM6048:DC:F,60,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM6048,TSSNM6048:DC:N,60,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Non-Powered,Flat Top Cap",TSSNM6648,TSSNM6648,66,48,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Non-Powered,No Top Cap",TSSNM6648,TSSNM6648:NC:N,66,48,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM6648,TSSNM6648:DN:F,66,48,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM6648,TSSNM6648:DN:N,66,48,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM6648,TSSNM6648:DC:F,66,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM6648,TSSNM6648:DC:N,66,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Non-Powered,Flat Top Cap",TSSNM7248,TSSNM7248,72,48,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Non-Powered,No Top Cap",TSSNM7248,TSSNM7248:NC:N,72,48,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM7248,TSSNM7248:DN:F,72,48,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM7248,TSSNM7248:DN:N,72,48,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM7248,TSSNM7248:DC:F,72,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM7248,TSSNM7248:DC:N,72,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Non-Powered,Flat Top Cap",TSSNM7848,TSSNM7848,78,48,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Non-Powered,No Top Cap",TSSNM7848,TSSNM7848:NC:N,78,48,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM7848,TSSNM7848:DN:F,78,48,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM7848,TSSNM7848:DN:N,78,48,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM7848,TSSNM7848:DC:F,78,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM7848,TSSNM7848:DC:N,78,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Non-Powered,Flat Top Cap",TSSNM8448,TSSNM8448,84,48,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Non-Powered,No Top Cap",TSSNM8448,TSSNM8448:NC:N,84,48,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM8448,TSSNM8448:DN:F,84,48,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM8448,TSSNM8448:DN:N,84,48,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM8448,TSSNM8448:DC:F,84,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM8448,TSSNM8448:DC:N,84,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Non-Powered,Flat Top Cap",TSSNM9048,TSSNM9048,90,48,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Non-Powered,No Top Cap",TSSNM9048,TSSNM9048:NC:N,90,48,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM9048,TSSNM9048:DN:F,90,48,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM9048,TSSNM9048:DN:N,90,48,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM9048,TSSNM9048:DC:F,90,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM9048,TSSNM9048:DC:N,90,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Non-Powered,Flat Top Cap",TSSNM9648,TSSNM9648,96,48,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Non-Powered,No Top Cap",TSSNM9648,TSSNM9648:NC:N,96,48,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM9648,TSSNM9648:DN:F,96,48,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM9648,TSSNM9648:DN:N,96,48,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM9648,TSSNM9648:DC:F,96,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM9648,TSSNM9648:DC:N,96,48,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Non-Powered,Flat Top Cap",TSSNM4854,TSSNM4854,48,54,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Non-Powered,No Top Cap",TSSNM4854,TSSNM4854:NC:N,48,54,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM4854,TSSNM4854:DN:F,48,54,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM4854,TSSNM4854:DN:N,48,54,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM4854,TSSNM4854:DC:F,48,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM4854,TSSNM4854:DC:N,48,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Non-Powered,Flat Top Cap",TSSNM5454,TSSNM5454,54,54,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Non-Powered,No Top Cap",TSSNM5454,TSSNM5454:NC:N,54,54,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM5454,TSSNM5454:DN:F,54,54,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM5454,TSSNM5454:DN:N,54,54,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM5454,TSSNM5454:DC:F,54,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM5454,TSSNM5454:DC:N,54,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Non-Powered,Flat Top Cap",TSSNM6054,TSSNM6054,60,54,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Non-Powered,No Top Cap",TSSNM6054,TSSNM6054:NC:N,60,54,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM6054,TSSNM6054:DN:F,60,54,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM6054,TSSNM6054:DN:N,60,54,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM6054,TSSNM6054:DC:F,60,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM6054,TSSNM6054:DC:N,60,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Non-Powered,Flat Top Cap",TSSNM6654,TSSNM6654,66,54,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Non-Powered,No Top Cap",TSSNM6654,TSSNM6654:NC:N,66,54,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM6654,TSSNM6654:DN:F,66,54,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM6654,TSSNM6654:DN:N,66,54,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM6654,TSSNM6654:DC:F,66,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM6654,TSSNM6654:DC:N,66,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Non-Powered,Flat Top Cap",TSSNM7254,TSSNM7254,72,54,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Non-Powered,No Top Cap",TSSNM7254,TSSNM7254:NC:N,72,54,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM7254,TSSNM7254:DN:F,72,54,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM7254,TSSNM7254:DN:N,72,54,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM7254,TSSNM7254:DC:F,72,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM7254,TSSNM7254:DC:N,72,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Non-Powered,Flat Top Cap",TSSNM7854,TSSNM7854,78,54,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Non-Powered,No Top Cap",TSSNM7854,TSSNM7854:NC:N,78,54,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM7854,TSSNM7854:DN:F,78,54,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM7854,TSSNM7854:DN:N,78,54,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM7854,TSSNM7854:DC:F,78,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM7854,TSSNM7854:DC:N,78,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Non-Powered,Flat Top Cap",TSSNM8454,TSSNM8454,84,54,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Non-Powered,No Top Cap",TSSNM8454,TSSNM8454:NC:N,84,54,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM8454,TSSNM8454:DN:F,84,54,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM8454,TSSNM8454:DN:N,84,54,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM8454,TSSNM8454:DC:F,84,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM8454,TSSNM8454:DC:N,84,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Non-Powered,Flat Top Cap",TSSNM9054,TSSNM9054,90,54,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Non-Powered,No Top Cap",TSSNM9054,TSSNM9054:NC:N,90,54,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM9054,TSSNM9054:DN:F,90,54,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM9054,TSSNM9054:DN:N,90,54,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM9054,TSSNM9054:DC:F,90,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM9054,TSSNM9054:DC:N,90,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Non-Powered,Flat Top Cap",TSSNM9654,TSSNM9654,96,54,Thermally-Fused Laminate,Non-Powered,Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, Non-Powered, Flat Aluminum Top Cap",NC:F,0,1,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Non-Powered,No Top Cap",TSSNM9654,TSSNM9654:NC:N,96,54,Thermally-Fused Laminate,Non-Powered,No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, Non-Powered, No Top Cap",NC:N,0,0,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Data Cutout Side 1,Flat Top Cap",TSSNM9654,TSSNM9654:DN:F,96,54,Thermally-Fused Laminate,"Data Cutout, Side 1",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, Data Cutout, Side 1, Flat Aluminum Top Cap",DN:F,1,1,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Data Cutout Side 1,No Top Cap",TSSNM9654,TSSNM9654:DN:N,96,54,Thermally-Fused Laminate,"Data Cutout, Side 1",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, Data Cutout, Side 1, No Top Cap",DN:N,1,0,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Data Cutout Both Sides,Flat Top Cap",TSSNM9654,TSSNM9654:DC:F,96,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",Flat,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, Data Cutout, Both Sides, Flat Aluminum Top Cap",DC:F,2,1,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Data Cutout Both Sides,No Top Cap",TSSNM9654,TSSNM9654:DC:N,96,54,Thermally-Fused Laminate,"Data Cutout, Both Sides",No Top Cap,"Tattoo Non-Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, Data Cutout, Both Sides, No Top Cap",DC:N,2,0,Furniture - KI - Systems Laminate
"48Wx48H,Magnetic,Power Side 1,Flat Top Cap",TSSPE4848,TSSPE4848:1P:F,48,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Power Side 1,No Top Cap",TSSPE4848,TSSPE4848:1P:N,48,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE4848,TSSPE4848:1D:F,48,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE4848,TSSPE4848:1D:N,48,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Power,Flat Top Cap",TSSPE4848,TSSPE4848,48,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Power,No Top Cap",TSSPE4848,TSSPE4848:DP:N,48,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE4848,TSSPE4848:2D:F,48,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE4848,TSSPE4848:2D:N,48,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE4848,TSSPE4848:DD:F,48,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Power w/ DC,No Top Cap",TSSPE4848,TSSPE4848:DD:N,48,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Hardwired,Flat Top Cap",TSSPE4848,TSSPE4848:CP:F,48,48,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Hardwired,No Top Cap",TSSPE4848,TSSPE4848:CP:N,48,48,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE4848,TSSPE4848:CD:F,48,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"48Wx48H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE4848,TSSPE4848:CD:N,48,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Power Side 1,Flat Top Cap",TSSPE5448,TSSPE5448:1P:F,54,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Power Side 1,No Top Cap",TSSPE5448,TSSPE5448:1P:N,54,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE5448,TSSPE5448:1D:F,54,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE5448,TSSPE5448:1D:N,54,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Power,Flat Top Cap",TSSPE5448,TSSPE5448,54,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Power,No Top Cap",TSSPE5448,TSSPE5448:DP:N,54,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE5448,TSSPE5448:2D:F,54,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE5448,TSSPE5448:2D:N,54,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE5448,TSSPE5448:DD:F,54,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Power w/ DC,No Top Cap",TSSPE5448,TSSPE5448:DD:N,54,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Hardwired,Flat Top Cap",TSSPE5448,TSSPE5448:CP:F,54,48,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Hardwired,No Top Cap",TSSPE5448,TSSPE5448:CP:N,54,48,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE5448,TSSPE5448:CD:F,54,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"54Wx48H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE5448,TSSPE5448:CD:N,54,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Power Side 1,Flat Top Cap",TSSPE6048,TSSPE6048:1P:F,60,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Power Side 1,No Top Cap",TSSPE6048,TSSPE6048:1P:N,60,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE6048,TSSPE6048:1D:F,60,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE6048,TSSPE6048:1D:N,60,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Power,Flat Top Cap",TSSPE6048,TSSPE6048,60,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Power,No Top Cap",TSSPE6048,TSSPE6048:DP:N,60,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE6048,TSSPE6048:2D:F,60,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE6048,TSSPE6048:2D:N,60,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE6048,TSSPE6048:DD:F,60,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Power w/ DC,No Top Cap",TSSPE6048,TSSPE6048:DD:N,60,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Hardwired,Flat Top Cap",TSSPE6048,TSSPE6048:CP:F,60,48,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Hardwired,No Top Cap",TSSPE6048,TSSPE6048:CP:N,60,48,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE6048,TSSPE6048:CD:F,60,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"60Wx48H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE6048,TSSPE6048:CD:N,60,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Power Side 1,Flat Top Cap",TSSPE6648,TSSPE6648:1P:F,66,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Power Side 1,No Top Cap",TSSPE6648,TSSPE6648:1P:N,66,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE6648,TSSPE6648:1D:F,66,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE6648,TSSPE6648:1D:N,66,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Power,Flat Top Cap",TSSPE6648,TSSPE6648,66,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Power,No Top Cap",TSSPE6648,TSSPE6648:DP:N,66,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE6648,TSSPE6648:2D:F,66,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE6648,TSSPE6648:2D:N,66,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE6648,TSSPE6648:DD:F,66,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Power w/ DC,No Top Cap",TSSPE6648,TSSPE6648:DD:N,66,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Hardwired,Flat Top Cap",TSSPE6648,TSSPE6648:CP:F,66,48,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Hardwired,No Top Cap",TSSPE6648,TSSPE6648:CP:N,66,48,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE6648,TSSPE6648:CD:F,66,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"66Wx48H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE6648,TSSPE6648:CD:N,66,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Power Side 1,Flat Top Cap",TSSPE7248,TSSPE7248:1P:F,72,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Power Side 1,No Top Cap",TSSPE7248,TSSPE7248:1P:N,72,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE7248,TSSPE7248:1D:F,72,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE7248,TSSPE7248:1D:N,72,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Power,Flat Top Cap",TSSPE7248,TSSPE7248,72,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Power,No Top Cap",TSSPE7248,TSSPE7248:DP:N,72,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE7248,TSSPE7248:2D:F,72,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE7248,TSSPE7248:2D:N,72,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE7248,TSSPE7248:DD:F,72,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Power w/ DC,No Top Cap",TSSPE7248,TSSPE7248:DD:N,72,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Hardwired,Flat Top Cap",TSSPE7248,TSSPE7248:CP:F,72,48,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Hardwired,No Top Cap",TSSPE7248,TSSPE7248:CP:N,72,48,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE7248,TSSPE7248:CD:F,72,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"72Wx48H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE7248,TSSPE7248:CD:N,72,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Power Side 1,Flat Top Cap",TSSPE7848,TSSPE7848:1P:F,78,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Power Side 1,No Top Cap",TSSPE7848,TSSPE7848:1P:N,78,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE7848,TSSPE7848:1D:F,78,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE7848,TSSPE7848:1D:N,78,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Power,Flat Top Cap",TSSPE7848,TSSPE7848,78,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Power,No Top Cap",TSSPE7848,TSSPE7848:DP:N,78,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE7848,TSSPE7848:2D:F,78,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE7848,TSSPE7848:2D:N,78,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE7848,TSSPE7848:DD:F,78,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Power w/ DC,No Top Cap",TSSPE7848,TSSPE7848:DD:N,78,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Hardwired,Flat Top Cap",TSSPE7848,TSSPE7848:CP:F,78,48,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Hardwired,No Top Cap",TSSPE7848,TSSPE7848:CP:N,78,48,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE7848,TSSPE7848:CD:F,78,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"78Wx48H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE7848,TSSPE7848:CD:N,78,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Power Side 1,Flat Top Cap",TSSPE8448,TSSPE8448:1P:F,84,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Power Side 1,No Top Cap",TSSPE8448,TSSPE8448:1P:N,84,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE8448,TSSPE8448:1D:F,84,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE8448,TSSPE8448:1D:N,84,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Power,Flat Top Cap",TSSPE8448,TSSPE8448,84,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Power,No Top Cap",TSSPE8448,TSSPE8448:DP:N,84,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE8448,TSSPE8448:2D:F,84,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE8448,TSSPE8448:2D:N,84,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE8448,TSSPE8448:DD:F,84,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Power w/ DC,No Top Cap",TSSPE8448,TSSPE8448:DD:N,84,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Hardwired,Flat Top Cap",TSSPE8448,TSSPE8448:CP:F,84,48,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Hardwired,No Top Cap",TSSPE8448,TSSPE8448:CP:N,84,48,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE8448,TSSPE8448:CD:F,84,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"84Wx48H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE8448,TSSPE8448:CD:N,84,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Power Side 1,Flat Top Cap",TSSPE9048,TSSPE9048:1P:F,90,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Power Side 1,No Top Cap",TSSPE9048,TSSPE9048:1P:N,90,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE9048,TSSPE9048:1D:F,90,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE9048,TSSPE9048:1D:N,90,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Power,Flat Top Cap",TSSPE9048,TSSPE9048,90,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Power,No Top Cap",TSSPE9048,TSSPE9048:DP:N,90,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE9048,TSSPE9048:2D:F,90,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE9048,TSSPE9048:2D:N,90,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE9048,TSSPE9048:DD:F,90,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Power w/ DC,No Top Cap",TSSPE9048,TSSPE9048:DD:N,90,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Hardwired,Flat Top Cap",TSSPE9048,TSSPE9048:CP:F,90,48,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Hardwired,No Top Cap",TSSPE9048,TSSPE9048:CP:N,90,48,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE9048,TSSPE9048:CD:F,90,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"90Wx48H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE9048,TSSPE9048:CD:N,90,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Power Side 1,Flat Top Cap",TSSPE9648,TSSPE9648:1P:F,96,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Power Side 1,No Top Cap",TSSPE9648,TSSPE9648:1P:N,96,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE9648,TSSPE9648:1D:F,96,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE9648,TSSPE9648:1D:N,96,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Power,Flat Top Cap",TSSPE9648,TSSPE9648,96,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Power,No Top Cap",TSSPE9648,TSSPE9648:DP:N,96,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE9648,TSSPE9648:2D:F,96,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE9648,TSSPE9648:2D:N,96,48,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE9648,TSSPE9648:DD:F,96,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Power w/ DC,No Top Cap",TSSPE9648,TSSPE9648:DD:N,96,48,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Hardwired,Flat Top Cap",TSSPE9648,TSSPE9648:CP:F,96,48,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Hardwired,No Top Cap",TSSPE9648,TSSPE9648:CP:N,96,48,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE9648,TSSPE9648:CD:F,96,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"96Wx48H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE9648,TSSPE9648:CD:N,96,48,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Power Side 1,Flat Top Cap",TSSPE4854,TSSPE4854:1P:F,48,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Power Side 1,No Top Cap",TSSPE4854,TSSPE4854:1P:N,48,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE4854,TSSPE4854:1D:F,48,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE4854,TSSPE4854:1D:N,48,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Power,Flat Top Cap",TSSPE4854,TSSPE4854,48,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Power,No Top Cap",TSSPE4854,TSSPE4854:DP:N,48,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE4854,TSSPE4854:2D:F,48,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE4854,TSSPE4854:2D:N,48,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE4854,TSSPE4854:DD:F,48,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Power w/ DC,No Top Cap",TSSPE4854,TSSPE4854:DD:N,48,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Hardwired,Flat Top Cap",TSSPE4854,TSSPE4854:CP:F,48,54,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Hardwired,No Top Cap",TSSPE4854,TSSPE4854:CP:N,48,54,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE4854,TSSPE4854:CD:F,48,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"48Wx54H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE4854,TSSPE4854:CD:N,48,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 48""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Power Side 1,Flat Top Cap",TSSPE5454,TSSPE5454:1P:F,54,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Power Side 1,No Top Cap",TSSPE5454,TSSPE5454:1P:N,54,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE5454,TSSPE5454:1D:F,54,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE5454,TSSPE5454:1D:N,54,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Power,Flat Top Cap",TSSPE5454,TSSPE5454,54,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Power,No Top Cap",TSSPE5454,TSSPE5454:DP:N,54,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE5454,TSSPE5454:2D:F,54,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE5454,TSSPE5454:2D:N,54,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE5454,TSSPE5454:DD:F,54,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Power w/ DC,No Top Cap",TSSPE5454,TSSPE5454:DD:N,54,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Hardwired,Flat Top Cap",TSSPE5454,TSSPE5454:CP:F,54,54,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Hardwired,No Top Cap",TSSPE5454,TSSPE5454:CP:N,54,54,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE5454,TSSPE5454:CD:F,54,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"54Wx54H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE5454,TSSPE5454:CD:N,54,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 54""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Power Side 1,Flat Top Cap",TSSPE6054,TSSPE6054:1P:F,60,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Power Side 1,No Top Cap",TSSPE6054,TSSPE6054:1P:N,60,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE6054,TSSPE6054:1D:F,60,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE6054,TSSPE6054:1D:N,60,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Power,Flat Top Cap",TSSPE6054,TSSPE6054,60,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Power,No Top Cap",TSSPE6054,TSSPE6054:DP:N,60,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE6054,TSSPE6054:2D:F,60,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE6054,TSSPE6054:2D:N,60,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE6054,TSSPE6054:DD:F,60,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Power w/ DC,No Top Cap",TSSPE6054,TSSPE6054:DD:N,60,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Hardwired,Flat Top Cap",TSSPE6054,TSSPE6054:CP:F,60,54,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Hardwired,No Top Cap",TSSPE6054,TSSPE6054:CP:N,60,54,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE6054,TSSPE6054:CD:F,60,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"60Wx54H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE6054,TSSPE6054:CD:N,60,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 60""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Power Side 1,Flat Top Cap",TSSPE6654,TSSPE6654:1P:F,66,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Power Side 1,No Top Cap",TSSPE6654,TSSPE6654:1P:N,66,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE6654,TSSPE6654:1D:F,66,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE6654,TSSPE6654:1D:N,66,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Power,Flat Top Cap",TSSPE6654,TSSPE6654,66,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Power,No Top Cap",TSSPE6654,TSSPE6654:DP:N,66,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE6654,TSSPE6654:2D:F,66,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE6654,TSSPE6654:2D:N,66,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE6654,TSSPE6654:DD:F,66,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Power w/ DC,No Top Cap",TSSPE6654,TSSPE6654:DD:N,66,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Hardwired,Flat Top Cap",TSSPE6654,TSSPE6654:CP:F,66,54,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Hardwired,No Top Cap",TSSPE6654,TSSPE6654:CP:N,66,54,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE6654,TSSPE6654:CD:F,66,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"66Wx54H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE6654,TSSPE6654:CD:N,66,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 66""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Power Side 1,Flat Top Cap",TSSPE7254,TSSPE7254:1P:F,72,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Power Side 1,No Top Cap",TSSPE7254,TSSPE7254:1P:N,72,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE7254,TSSPE7254:1D:F,72,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE7254,TSSPE7254:1D:N,72,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Power,Flat Top Cap",TSSPE7254,TSSPE7254,72,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Power,No Top Cap",TSSPE7254,TSSPE7254:DP:N,72,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE7254,TSSPE7254:2D:F,72,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE7254,TSSPE7254:2D:N,72,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE7254,TSSPE7254:DD:F,72,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Power w/ DC,No Top Cap",TSSPE7254,TSSPE7254:DD:N,72,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Hardwired,Flat Top Cap",TSSPE7254,TSSPE7254:CP:F,72,54,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Hardwired,No Top Cap",TSSPE7254,TSSPE7254:CP:N,72,54,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE7254,TSSPE7254:CD:F,72,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"72Wx54H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE7254,TSSPE7254:CD:N,72,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 72""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Power Side 1,Flat Top Cap",TSSPE7854,TSSPE7854:1P:F,78,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Power Side 1,No Top Cap",TSSPE7854,TSSPE7854:1P:N,78,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE7854,TSSPE7854:1D:F,78,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE7854,TSSPE7854:1D:N,78,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Power,Flat Top Cap",TSSPE7854,TSSPE7854,78,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Power,No Top Cap",TSSPE7854,TSSPE7854:DP:N,78,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE7854,TSSPE7854:2D:F,78,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE7854,TSSPE7854:2D:N,78,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE7854,TSSPE7854:DD:F,78,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Power w/ DC,No Top Cap",TSSPE7854,TSSPE7854:DD:N,78,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Hardwired,Flat Top Cap",TSSPE7854,TSSPE7854:CP:F,78,54,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Hardwired,No Top Cap",TSSPE7854,TSSPE7854:CP:N,78,54,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE7854,TSSPE7854:CD:F,78,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"78Wx54H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE7854,TSSPE7854:CD:N,78,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 78""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Power Side 1,Flat Top Cap",TSSPE8454,TSSPE8454:1P:F,84,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Power Side 1,No Top Cap",TSSPE8454,TSSPE8454:1P:N,84,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE8454,TSSPE8454:1D:F,84,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE8454,TSSPE8454:1D:N,84,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Power,Flat Top Cap",TSSPE8454,TSSPE8454,84,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Power,No Top Cap",TSSPE8454,TSSPE8454:DP:N,84,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE8454,TSSPE8454:2D:F,84,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE8454,TSSPE8454:2D:N,84,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE8454,TSSPE8454:DD:F,84,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Power w/ DC,No Top Cap",TSSPE8454,TSSPE8454:DD:N,84,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Hardwired,Flat Top Cap",TSSPE8454,TSSPE8454:CP:F,84,54,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Hardwired,No Top Cap",TSSPE8454,TSSPE8454:CP:N,84,54,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE8454,TSSPE8454:CD:F,84,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"84Wx54H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE8454,TSSPE8454:CD:N,84,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 84""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Power Side 1,Flat Top Cap",TSSPE9054,TSSPE9054:1P:F,90,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Power Side 1,No Top Cap",TSSPE9054,TSSPE9054:1P:N,90,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE9054,TSSPE9054:1D:F,90,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE9054,TSSPE9054:1D:N,90,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Power,Flat Top Cap",TSSPE9054,TSSPE9054,90,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Power,No Top Cap",TSSPE9054,TSSPE9054:DP:N,90,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE9054,TSSPE9054:2D:F,90,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE9054,TSSPE9054:2D:N,90,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE9054,TSSPE9054:DD:F,90,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Power w/ DC,No Top Cap",TSSPE9054,TSSPE9054:DD:N,90,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Hardwired,Flat Top Cap",TSSPE9054,TSSPE9054:CP:F,90,54,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Hardwired,No Top Cap",TSSPE9054,TSSPE9054:CP:N,90,54,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE9054,TSSPE9054:CD:F,90,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"90Wx54H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE9054,TSSPE9054:CD:N,90,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 90""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Power Side 1,Flat Top Cap",TSSPE9654,TSSPE9654:1P:F,96,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Power Side 1,No Top Cap",TSSPE9654,TSSPE9654:1P:N,96,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Power & DC Side 1,Flat Top Cap",TSSPE9654,TSSPE9654:1D:F,96,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Power & DC Side 1,No Top Cap",TSSPE9654,TSSPE9654:1D:N,96,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Power,Flat Top Cap",TSSPE9654,TSSPE9654,96,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Power,No Top Cap",TSSPE9654,TSSPE9654:DP:N,96,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Power w/ DC Side 1,Flat Top Cap",TSSPE9654,TSSPE9654:2D:F,96,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Power w/ DC Side 1,No Top Cap",TSSPE9654,TSSPE9654:2D:N,96,54,Magnetic Dry-Erasable Steel,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Power w/ DC,Flat Top Cap",TSSPE9654,TSSPE9654:DD:F,96,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Power w/ DC,No Top Cap",TSSPE9654,TSSPE9654:DD:N,96,54,Magnetic Dry-Erasable Steel,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Hardwired,Flat Top Cap",TSSPE9654,TSSPE9654:CP:F,96,54,Magnetic Dry-Erasable Steel,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Hardwired,No Top Cap",TSSPE9654,TSSPE9654:CP:N,96,54,Magnetic Dry-Erasable Steel,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Hardwired w/ DC,Flat Top Cap",TSSPE9654,TSSPE9654:CD:F,96,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Markerboard
"96Wx54H,Magnetic,Hardwired w/ DC,No Top Cap",TSSPE9654,TSSPE9654:CD:N,96,54,Magnetic Dry-Erasable Steel,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Magnetic Dry-Erasable Steel Core, 96""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Markerboard
"48Wx48H,Laminate,Power Side 1,Flat Top Cap",TSSPM4848,TSSPM4848:1P:F,48,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Power Side 1,No Top Cap",TSSPM4848,TSSPM4848:1P:N,48,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM4848,TSSPM4848:1D:F,48,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Power & DC Side 1,No Top Cap",TSSPM4848,TSSPM4848:1D:N,48,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Power,Flat Top Cap",TSSPM4848,TSSPM4848,48,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Power,No Top Cap",TSSPM4848,TSSPM4848:DP:N,48,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM4848,TSSPM4848:2D:F,48,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM4848,TSSPM4848:2D:N,48,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Power w/ DC,Flat Top Cap",TSSPM4848,TSSPM4848:DD:F,48,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Power w/ DC,No Top Cap",TSSPM4848,TSSPM4848:DD:N,48,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Hardwired,Flat Top Cap",TSSPM4848,TSSPM4848:CP:F,48,48,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Hardwired,No Top Cap",TSSPM4848,TSSPM4848:CP:N,48,48,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM4848,TSSPM4848:CD:F,48,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"48Wx48H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM4848,TSSPM4848:CD:N,48,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Power Side 1,Flat Top Cap",TSSPM5448,TSSPM5448:1P:F,54,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Power Side 1,No Top Cap",TSSPM5448,TSSPM5448:1P:N,54,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM5448,TSSPM5448:1D:F,54,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Power & DC Side 1,No Top Cap",TSSPM5448,TSSPM5448:1D:N,54,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Power,Flat Top Cap",TSSPM5448,TSSPM5448,54,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Power,No Top Cap",TSSPM5448,TSSPM5448:DP:N,54,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM5448,TSSPM5448:2D:F,54,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM5448,TSSPM5448:2D:N,54,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Power w/ DC,Flat Top Cap",TSSPM5448,TSSPM5448:DD:F,54,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Power w/ DC,No Top Cap",TSSPM5448,TSSPM5448:DD:N,54,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Hardwired,Flat Top Cap",TSSPM5448,TSSPM5448:CP:F,54,48,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Hardwired,No Top Cap",TSSPM5448,TSSPM5448:CP:N,54,48,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM5448,TSSPM5448:CD:F,54,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"54Wx48H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM5448,TSSPM5448:CD:N,54,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Power Side 1,Flat Top Cap",TSSPM6048,TSSPM6048:1P:F,60,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Power Side 1,No Top Cap",TSSPM6048,TSSPM6048:1P:N,60,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM6048,TSSPM6048:1D:F,60,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Power & DC Side 1,No Top Cap",TSSPM6048,TSSPM6048:1D:N,60,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Power,Flat Top Cap",TSSPM6048,TSSPM6048,60,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Power,No Top Cap",TSSPM6048,TSSPM6048:DP:N,60,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM6048,TSSPM6048:2D:F,60,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM6048,TSSPM6048:2D:N,60,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Power w/ DC,Flat Top Cap",TSSPM6048,TSSPM6048:DD:F,60,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Power w/ DC,No Top Cap",TSSPM6048,TSSPM6048:DD:N,60,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Hardwired,Flat Top Cap",TSSPM6048,TSSPM6048:CP:F,60,48,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Hardwired,No Top Cap",TSSPM6048,TSSPM6048:CP:N,60,48,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM6048,TSSPM6048:CD:F,60,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"60Wx48H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM6048,TSSPM6048:CD:N,60,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Power Side 1,Flat Top Cap",TSSPM6648,TSSPM6648:1P:F,66,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Power Side 1,No Top Cap",TSSPM6648,TSSPM6648:1P:N,66,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM6648,TSSPM6648:1D:F,66,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Power & DC Side 1,No Top Cap",TSSPM6648,TSSPM6648:1D:N,66,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Power,Flat Top Cap",TSSPM6648,TSSPM6648,66,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Power,No Top Cap",TSSPM6648,TSSPM6648:DP:N,66,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM6648,TSSPM6648:2D:F,66,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM6648,TSSPM6648:2D:N,66,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Power w/ DC,Flat Top Cap",TSSPM6648,TSSPM6648:DD:F,66,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Power w/ DC,No Top Cap",TSSPM6648,TSSPM6648:DD:N,66,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Hardwired,Flat Top Cap",TSSPM6648,TSSPM6648:CP:F,66,48,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Hardwired,No Top Cap",TSSPM6648,TSSPM6648:CP:N,66,48,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM6648,TSSPM6648:CD:F,66,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"66Wx48H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM6648,TSSPM6648:CD:N,66,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Power Side 1,Flat Top Cap",TSSPM7248,TSSPM7248:1P:F,72,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Power Side 1,No Top Cap",TSSPM7248,TSSPM7248:1P:N,72,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM7248,TSSPM7248:1D:F,72,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Power & DC Side 1,No Top Cap",TSSPM7248,TSSPM7248:1D:N,72,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Power,Flat Top Cap",TSSPM7248,TSSPM7248,72,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Power,No Top Cap",TSSPM7248,TSSPM7248:DP:N,72,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM7248,TSSPM7248:2D:F,72,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM7248,TSSPM7248:2D:N,72,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Power w/ DC,Flat Top Cap",TSSPM7248,TSSPM7248:DD:F,72,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Power w/ DC,No Top Cap",TSSPM7248,TSSPM7248:DD:N,72,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Hardwired,Flat Top Cap",TSSPM7248,TSSPM7248:CP:F,72,48,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Hardwired,No Top Cap",TSSPM7248,TSSPM7248:CP:N,72,48,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM7248,TSSPM7248:CD:F,72,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"72Wx48H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM7248,TSSPM7248:CD:N,72,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Power Side 1,Flat Top Cap",TSSPM7848,TSSPM7848:1P:F,78,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Power Side 1,No Top Cap",TSSPM7848,TSSPM7848:1P:N,78,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM7848,TSSPM7848:1D:F,78,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Power & DC Side 1,No Top Cap",TSSPM7848,TSSPM7848:1D:N,78,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Power,Flat Top Cap",TSSPM7848,TSSPM7848,78,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Power,No Top Cap",TSSPM7848,TSSPM7848:DP:N,78,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM7848,TSSPM7848:2D:F,78,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM7848,TSSPM7848:2D:N,78,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Power w/ DC,Flat Top Cap",TSSPM7848,TSSPM7848:DD:F,78,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Power w/ DC,No Top Cap",TSSPM7848,TSSPM7848:DD:N,78,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Hardwired,Flat Top Cap",TSSPM7848,TSSPM7848:CP:F,78,48,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Hardwired,No Top Cap",TSSPM7848,TSSPM7848:CP:N,78,48,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM7848,TSSPM7848:CD:F,78,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"78Wx48H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM7848,TSSPM7848:CD:N,78,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Power Side 1,Flat Top Cap",TSSPM8448,TSSPM8448:1P:F,84,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Power Side 1,No Top Cap",TSSPM8448,TSSPM8448:1P:N,84,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM8448,TSSPM8448:1D:F,84,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Power & DC Side 1,No Top Cap",TSSPM8448,TSSPM8448:1D:N,84,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Power,Flat Top Cap",TSSPM8448,TSSPM8448,84,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Power,No Top Cap",TSSPM8448,TSSPM8448:DP:N,84,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM8448,TSSPM8448:2D:F,84,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM8448,TSSPM8448:2D:N,84,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Power w/ DC,Flat Top Cap",TSSPM8448,TSSPM8448:DD:F,84,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Power w/ DC,No Top Cap",TSSPM8448,TSSPM8448:DD:N,84,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Hardwired,Flat Top Cap",TSSPM8448,TSSPM8448:CP:F,84,48,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Hardwired,No Top Cap",TSSPM8448,TSSPM8448:CP:N,84,48,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM8448,TSSPM8448:CD:F,84,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"84Wx48H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM8448,TSSPM8448:CD:N,84,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Power Side 1,Flat Top Cap",TSSPM9048,TSSPM9048:1P:F,90,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Power Side 1,No Top Cap",TSSPM9048,TSSPM9048:1P:N,90,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM9048,TSSPM9048:1D:F,90,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Power & DC Side 1,No Top Cap",TSSPM9048,TSSPM9048:1D:N,90,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Power,Flat Top Cap",TSSPM9048,TSSPM9048,90,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Power,No Top Cap",TSSPM9048,TSSPM9048:DP:N,90,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM9048,TSSPM9048:2D:F,90,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM9048,TSSPM9048:2D:N,90,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Power w/ DC,Flat Top Cap",TSSPM9048,TSSPM9048:DD:F,90,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Power w/ DC,No Top Cap",TSSPM9048,TSSPM9048:DD:N,90,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Hardwired,Flat Top Cap",TSSPM9048,TSSPM9048:CP:F,90,48,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Hardwired,No Top Cap",TSSPM9048,TSSPM9048:CP:N,90,48,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM9048,TSSPM9048:CD:F,90,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"90Wx48H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM9048,TSSPM9048:CD:N,90,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Power Side 1,Flat Top Cap",TSSPM9648,TSSPM9648:1P:F,96,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Power Side 1,No Top Cap",TSSPM9648,TSSPM9648:1P:N,96,48,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM9648,TSSPM9648:1D:F,96,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Power & DC Side 1,No Top Cap",TSSPM9648,TSSPM9648:1D:N,96,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Power,Flat Top Cap",TSSPM9648,TSSPM9648,96,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Power,No Top Cap",TSSPM9648,TSSPM9648:DP:N,96,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM9648,TSSPM9648:2D:F,96,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM9648,TSSPM9648:2D:N,96,48,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Power w/ DC,Flat Top Cap",TSSPM9648,TSSPM9648:DD:F,96,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Power w/ DC,No Top Cap",TSSPM9648,TSSPM9648:DD:N,96,48,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Hardwired,Flat Top Cap",TSSPM9648,TSSPM9648:CP:F,96,48,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Hardwired,No Top Cap",TSSPM9648,TSSPM9648:CP:N,96,48,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM9648,TSSPM9648:CD:F,96,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"96Wx48H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM9648,TSSPM9648:CD:N,96,48,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 48""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Power Side 1,Flat Top Cap",TSSPM4854,TSSPM4854:1P:F,48,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Power Side 1,No Top Cap",TSSPM4854,TSSPM4854:1P:N,48,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM4854,TSSPM4854:1D:F,48,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Power & DC Side 1,No Top Cap",TSSPM4854,TSSPM4854:1D:N,48,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Power,Flat Top Cap",TSSPM4854,TSSPM4854,48,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Power,No Top Cap",TSSPM4854,TSSPM4854:DP:N,48,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM4854,TSSPM4854:2D:F,48,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM4854,TSSPM4854:2D:N,48,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Power w/ DC,Flat Top Cap",TSSPM4854,TSSPM4854:DD:F,48,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Power w/ DC,No Top Cap",TSSPM4854,TSSPM4854:DD:N,48,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Hardwired,Flat Top Cap",TSSPM4854,TSSPM4854:CP:F,48,54,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Hardwired,No Top Cap",TSSPM4854,TSSPM4854:CP:N,48,54,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM4854,TSSPM4854:CD:F,48,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"48Wx54H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM4854,TSSPM4854:CD:N,48,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 48""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Power Side 1,Flat Top Cap",TSSPM5454,TSSPM5454:1P:F,54,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Power Side 1,No Top Cap",TSSPM5454,TSSPM5454:1P:N,54,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM5454,TSSPM5454:1D:F,54,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Power & DC Side 1,No Top Cap",TSSPM5454,TSSPM5454:1D:N,54,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Power,Flat Top Cap",TSSPM5454,TSSPM5454,54,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Power,No Top Cap",TSSPM5454,TSSPM5454:DP:N,54,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM5454,TSSPM5454:2D:F,54,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM5454,TSSPM5454:2D:N,54,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Power w/ DC,Flat Top Cap",TSSPM5454,TSSPM5454:DD:F,54,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Power w/ DC,No Top Cap",TSSPM5454,TSSPM5454:DD:N,54,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Hardwired,Flat Top Cap",TSSPM5454,TSSPM5454:CP:F,54,54,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Hardwired,No Top Cap",TSSPM5454,TSSPM5454:CP:N,54,54,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM5454,TSSPM5454:CD:F,54,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"54Wx54H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM5454,TSSPM5454:CD:N,54,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 54""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Power Side 1,Flat Top Cap",TSSPM6054,TSSPM6054:1P:F,60,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Power Side 1,No Top Cap",TSSPM6054,TSSPM6054:1P:N,60,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM6054,TSSPM6054:1D:F,60,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Power & DC Side 1,No Top Cap",TSSPM6054,TSSPM6054:1D:N,60,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Power,Flat Top Cap",TSSPM6054,TSSPM6054,60,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Power,No Top Cap",TSSPM6054,TSSPM6054:DP:N,60,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM6054,TSSPM6054:2D:F,60,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM6054,TSSPM6054:2D:N,60,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Power w/ DC,Flat Top Cap",TSSPM6054,TSSPM6054:DD:F,60,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Power w/ DC,No Top Cap",TSSPM6054,TSSPM6054:DD:N,60,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Hardwired,Flat Top Cap",TSSPM6054,TSSPM6054:CP:F,60,54,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Hardwired,No Top Cap",TSSPM6054,TSSPM6054:CP:N,60,54,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM6054,TSSPM6054:CD:F,60,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"60Wx54H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM6054,TSSPM6054:CD:N,60,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 60""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Power Side 1,Flat Top Cap",TSSPM6654,TSSPM6654:1P:F,66,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Power Side 1,No Top Cap",TSSPM6654,TSSPM6654:1P:N,66,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM6654,TSSPM6654:1D:F,66,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Power & DC Side 1,No Top Cap",TSSPM6654,TSSPM6654:1D:N,66,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Power,Flat Top Cap",TSSPM6654,TSSPM6654,66,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Power,No Top Cap",TSSPM6654,TSSPM6654:DP:N,66,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM6654,TSSPM6654:2D:F,66,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM6654,TSSPM6654:2D:N,66,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Power w/ DC,Flat Top Cap",TSSPM6654,TSSPM6654:DD:F,66,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Power w/ DC,No Top Cap",TSSPM6654,TSSPM6654:DD:N,66,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Hardwired,Flat Top Cap",TSSPM6654,TSSPM6654:CP:F,66,54,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Hardwired,No Top Cap",TSSPM6654,TSSPM6654:CP:N,66,54,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM6654,TSSPM6654:CD:F,66,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"66Wx54H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM6654,TSSPM6654:CD:N,66,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 66""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Power Side 1,Flat Top Cap",TSSPM7254,TSSPM7254:1P:F,72,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Power Side 1,No Top Cap",TSSPM7254,TSSPM7254:1P:N,72,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM7254,TSSPM7254:1D:F,72,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Power & DC Side 1,No Top Cap",TSSPM7254,TSSPM7254:1D:N,72,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Power,Flat Top Cap",TSSPM7254,TSSPM7254,72,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Power,No Top Cap",TSSPM7254,TSSPM7254:DP:N,72,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM7254,TSSPM7254:2D:F,72,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM7254,TSSPM7254:2D:N,72,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Power w/ DC,Flat Top Cap",TSSPM7254,TSSPM7254:DD:F,72,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Power w/ DC,No Top Cap",TSSPM7254,TSSPM7254:DD:N,72,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Hardwired,Flat Top Cap",TSSPM7254,TSSPM7254:CP:F,72,54,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Hardwired,No Top Cap",TSSPM7254,TSSPM7254:CP:N,72,54,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM7254,TSSPM7254:CD:F,72,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"72Wx54H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM7254,TSSPM7254:CD:N,72,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 72""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Power Side 1,Flat Top Cap",TSSPM7854,TSSPM7854:1P:F,78,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Power Side 1,No Top Cap",TSSPM7854,TSSPM7854:1P:N,78,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM7854,TSSPM7854:1D:F,78,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Power & DC Side 1,No Top Cap",TSSPM7854,TSSPM7854:1D:N,78,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Power,Flat Top Cap",TSSPM7854,TSSPM7854,78,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Power,No Top Cap",TSSPM7854,TSSPM7854:DP:N,78,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM7854,TSSPM7854:2D:F,78,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM7854,TSSPM7854:2D:N,78,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Power w/ DC,Flat Top Cap",TSSPM7854,TSSPM7854:DD:F,78,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Power w/ DC,No Top Cap",TSSPM7854,TSSPM7854:DD:N,78,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Hardwired,Flat Top Cap",TSSPM7854,TSSPM7854:CP:F,78,54,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Hardwired,No Top Cap",TSSPM7854,TSSPM7854:CP:N,78,54,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM7854,TSSPM7854:CD:F,78,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"78Wx54H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM7854,TSSPM7854:CD:N,78,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 78""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Power Side 1,Flat Top Cap",TSSPM8454,TSSPM8454:1P:F,84,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Power Side 1,No Top Cap",TSSPM8454,TSSPM8454:1P:N,84,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM8454,TSSPM8454:1D:F,84,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Power & DC Side 1,No Top Cap",TSSPM8454,TSSPM8454:1D:N,84,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Power,Flat Top Cap",TSSPM8454,TSSPM8454,84,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Power,No Top Cap",TSSPM8454,TSSPM8454:DP:N,84,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM8454,TSSPM8454:2D:F,84,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM8454,TSSPM8454:2D:N,84,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Power w/ DC,Flat Top Cap",TSSPM8454,TSSPM8454:DD:F,84,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Power w/ DC,No Top Cap",TSSPM8454,TSSPM8454:DD:N,84,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Hardwired,Flat Top Cap",TSSPM8454,TSSPM8454:CP:F,84,54,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Hardwired,No Top Cap",TSSPM8454,TSSPM8454:CP:N,84,54,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM8454,TSSPM8454:CD:F,84,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"84Wx54H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM8454,TSSPM8454:CD:N,84,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 84""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Power Side 1,Flat Top Cap",TSSPM9054,TSSPM9054:1P:F,90,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Power Side 1,No Top Cap",TSSPM9054,TSSPM9054:1P:N,90,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM9054,TSSPM9054:1D:F,90,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Power & DC Side 1,No Top Cap",TSSPM9054,TSSPM9054:1D:N,90,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Power,Flat Top Cap",TSSPM9054,TSSPM9054,90,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Power,No Top Cap",TSSPM9054,TSSPM9054:DP:N,90,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM9054,TSSPM9054:2D:F,90,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM9054,TSSPM9054:2D:N,90,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Power w/ DC,Flat Top Cap",TSSPM9054,TSSPM9054:DD:F,90,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Power w/ DC,No Top Cap",TSSPM9054,TSSPM9054:DD:N,90,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Hardwired,Flat Top Cap",TSSPM9054,TSSPM9054:CP:F,90,54,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Hardwired,No Top Cap",TSSPM9054,TSSPM9054:CP:N,90,54,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM9054,TSSPM9054:CD:F,90,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"90Wx54H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM9054,TSSPM9054:CD:N,90,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 90""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Power Side 1,Flat Top Cap",TSSPM9654,TSSPM9654:1P:F,96,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, 10-Wire Power, Side 1, Flat Aluminum Top Cap",1P:F,3,1,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Power Side 1,No Top Cap",TSSPM9654,TSSPM9654:1P:N,96,54,Thermally-Fused Laminate,"10-Wire Power, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, 10-Wire Power, Side 1, No Top Cap",1P:N,3,0,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Power & DC Side 1,Flat Top Cap",TSSPM9654,TSSPM9654:1D:F,96,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, Flat Aluminum Top Cap",1D:F,4,1,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Power & DC Side 1,No Top Cap",TSSPM9654,TSSPM9654:1D:N,96,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, 10-Wire Power w/ Data Cutout, Side 1, No Top Cap",1D:N,4,0,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Power,Flat Top Cap",TSSPM9654,TSSPM9654,96,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, 10-Wire Power, Both Sides, Flat Aluminum Top Cap",DP:F,5,1,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Power,No Top Cap",TSSPM9654,TSSPM9654:DP:N,96,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, 10-Wire Power, Both Sides, No Top Cap",DP:N,5,0,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Power w/ DC Side 1,Flat Top Cap",TSSPM9654,TSSPM9654:2D:F,96,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, Flat Aluminum Top Cap",2D:F,6,1,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Power w/ DC Side 1,No Top Cap",TSSPM9654,TSSPM9654:2D:N,96,54,Thermally-Fused Laminate,"10-Wire Power, Both Sides w/ Data, Side 1",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, 10-Wire Power, Both Sides w/ Data, Side 1, No Top Cap",2D:N,6,0,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Power w/ DC,Flat Top Cap",TSSPM9654,TSSPM9654:DD:F,96,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, Flat Aluminum Top Cap",DD:F,7,1,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Power w/ DC,No Top Cap",TSSPM9654,TSSPM9654:DD:N,96,54,Thermally-Fused Laminate,"10-Wire Power w/ Data Cutout, Both Sides",No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, 10-Wire Power w/ Data Cutout, Both Sides, No Top Cap",DD:N,7,0,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Hardwired,Flat Top Cap",TSSPM9654,TSSPM9654:CP:F,96,54,Thermally-Fused Laminate,Hardwired,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, Hardwired, Flat Aluminum Top Cap",CP:F,8,1,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Hardwired,No Top Cap",TSSPM9654,TSSPM9654:CP:N,96,54,Thermally-Fused Laminate,Hardwired,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, Hardwired, No Top Cap",CP:N,8,0,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Hardwired w/ DC,Flat Top Cap",TSSPM9654,TSSPM9654:CD:F,96,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,Flat,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, Hardwired w/ Data Cutout, Flat Aluminum Top Cap",CD:F,9,1,Furniture - KI - Systems Laminate
"96Wx54H,Laminate,Hardwired w/ DC,No Top Cap",TSSPM9654,TSSPM9654:CD:N,96,54,Thermally-Fused Laminate,Hardwired w/ Data Cutout,No Top Cap,"Tattoo Powered Monolithic Spine Screen - Thermally-Fused Laminate Core, 96""W x 54""H, Hardwired w/ Data Cutout, No Top Cap",CD:N,9,0,Furniture - KI - Systems Laminate
