,Basic Model##Other##,Model##Other##,Depth##Length##inches,Depth Center##Length##inches,Width##Length##inches,Edge Style##Other##,Power Option##Other##,Power Option Description##Other##,Base Style##Other##,Description##Other##,Option##Other##,Has Glide##Other##,Power Style##Other##
"29Hx30-36Dx60W,No Power,Casters",PIFDC3060T,PIFDC3060T-74P:NNN:NMP:4EC,30,36,60,74P,NNN,None,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, No Power, Casters",NNN:NMP:4EC,0,0
"29Hx30-36Dx60W,Wire Management Only,Casters",PIFDC3060T,PIFDC3060T-74P:WMO:NMP:4EC,30,36,60,74P,WMO,Wire Management Only,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, Wire Management Only, Casters",WMO:NMP:4EC,0,1
"29Hx30-36Dx60W,(1) Nacre In-Surface Module,Casters",PIFDC3060T,PIFDC3060T-74P:MA1:NMP:4EC,30,36,60,74P,MA1,(1) Nacre In-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, (1) Nacre In-Surface Module, Casters",MA1:NMP:4EC,0,2
"29Hx30-36Dx60W,(1) Dubble Under-Surface Module,Casters",PIFDC3060T,PIFDC3060T-74P:MB1:NMP:4EC,30,36,60,74P,MB1,(1) Dubble Under-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, (1) Dubble Under-Surface Module, Casters",MB1:NMP:4EC,0,3
"29Hx30-36Dx60W,(1) Dean In-Surface Module,Casters",PIFDC3060T,PIFDC3060T-74P:MD1:NMP:4EC,30,36,60,74P,MD1,(1) Dean In-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, (1) Dean In-Surface Module, Casters",MD1:NMP:4EC,0,4
"29Hx30-36Dx60W,(1) Node In Surface Module,Casters",PIFDC3060T,PIFDC3060T-74P:MO1:NMP:4EC,30,36,60,74P,MO1,(1) Node In Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, (1) Node In Surface Module, Casters",MO1:NMP:4EC,0,5
"29Hx30-36Dx60W,(1) Grommet - Nacre,Casters",PIFDC3060T,PIFDC3060T-74P:GA1:NMP:4EC,30,36,60,74P,GA1,(1) Grommet - Nacre,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, (1) Grommet - Nacre, Casters",GA1:NMP:4EC,0,6
"29Hx30-36Dx60W,(1) Grommet - Dean,Casters",PIFDC3060T,PIFDC3060T-74P:GD1:NMP:4EC,30,36,60,74P,GD1,(1) Grommet - Dean,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, (1) Grommet - Dean, Casters",GD1:NMP:4EC,0,7
"29Hx30-36Dx60W,(1) Grommet - Node,Casters",PIFDC3060T,PIFDC3060T-74P:GO1:NMP:4EC,30,36,60,74P,GO1,(1) Grommet - Node,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, (1) Grommet - Node, Casters",GO1:NMP:4EC,0,8
"29Hx30-36Dx60W,No Power,Glides",PIFDC3060T,PIFDC3060T-74P,30,36,60,74P,NNN,None,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, No Power, Glides",NNN:NMP:4GB,1,0
"29Hx30-36Dx60W,Wire Management Only,Glides",PIFDC3060T,PIFDC3060T-74P:WMO:NMP:4GB,30,36,60,74P,WMO,Wire Management Only,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, Wire Management Only, Glides",WMO:NMP:4GB,1,1
"29Hx30-36Dx60W,(1) Nacre In-Surface Module,Glides",PIFDC3060T,PIFDC3060T-74P:MA1:NMP:4GB,30,36,60,74P,MA1,(1) Nacre In-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, (1) Nacre In-Surface Module, Glides",MA1:NMP:4GB,1,2
"29Hx30-36Dx60W,(1) Dubble Under-Surface Module,Glides",PIFDC3060T,PIFDC3060T-74P:MB1:NMP:4GB,30,36,60,74P,MB1,(1) Dubble Under-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, (1) Dubble Under-Surface Module, Glides",MB1:NMP:4GB,1,3
"29Hx30-36Dx60W,(1) Dean In-Surface Module,Glides",PIFDC3060T,PIFDC3060T-74P:MD1:NMP:4GB,30,36,60,74P,MD1,(1) Dean In-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, (1) Dean In-Surface Module, Glides",MD1:NMP:4GB,1,4
"29Hx30-36Dx60W,(1) Node In Surface Module,Glides",PIFDC3060T,PIFDC3060T-74P:MO1:NMP:4GB,30,36,60,74P,MO1,(1) Node In Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, (1) Node In Surface Module, Glides",MO1:NMP:4GB,1,5
"29Hx30-36Dx60W,(1) Grommet - Nacre,Glides",PIFDC3060T,PIFDC3060T-74P:GA1:NMP:4GB,30,36,60,74P,GA1,(1) Grommet - Nacre,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, (1) Grommet - Nacre, Glides",GA1:NMP:4GB,1,6
"29Hx30-36Dx60W,(1) Grommet - Dean,Glides",PIFDC3060T,PIFDC3060T-74P:GD1:NMP:4GB,30,36,60,74P,GD1,(1) Grommet - Dean,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, (1) Grommet - Dean, Glides",GD1:NMP:4GB,1,7
"29Hx30-36Dx60W,(1) Grommet - Node,Glides",PIFDC3060T,PIFDC3060T-74P:GO1:NMP:4GB,30,36,60,74P,GO1,(1) Grommet - Node,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 60""W, 29""H, 74P Edge, (1) Grommet - Node, Glides",GO1:NMP:4GB,1,8
"29Hx30-36Dx72W,No Power,Casters",PIFDC3072T,PIFDC3072T-74P:NNN:NMP:4EC,30,36,72,74P,NNN,None,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, No Power, Casters",NNN:NMP:4EC,0,0
"29Hx30-36Dx72W,Wire Management Only,Casters",PIFDC3072T,PIFDC3072T-74P:WMO:NMP:4EC,30,36,72,74P,WMO,Wire Management Only,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, Wire Management Only, Casters",WMO:NMP:4EC,0,1
"29Hx30-36Dx72W,(1) Nacre In-Surface Module,Casters",PIFDC3072T,PIFDC3072T-74P:MA1:NMP:4EC,30,36,72,74P,MA1,(1) Nacre In-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, (1) Nacre In-Surface Module, Casters",MA1:NMP:4EC,0,2
"29Hx30-36Dx72W,(1) Dubble Under-Surface Module,Casters",PIFDC3072T,PIFDC3072T-74P:MB1:NMP:4EC,30,36,72,74P,MB1,(1) Dubble Under-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, (1) Dubble Under-Surface Module, Casters",MB1:NMP:4EC,0,3
"29Hx30-36Dx72W,(1) Dean In-Surface Module,Casters",PIFDC3072T,PIFDC3072T-74P:MD1:NMP:4EC,30,36,72,74P,MD1,(1) Dean In-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, (1) Dean In-Surface Module, Casters",MD1:NMP:4EC,0,4
"29Hx30-36Dx72W,(1) Node In Surface Module,Casters",PIFDC3072T,PIFDC3072T-74P:MO1:NMP:4EC,30,36,72,74P,MO1,(1) Node In Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, (1) Node In Surface Module, Casters",MO1:NMP:4EC,0,5
"29Hx30-36Dx72W,(1) Grommet - Nacre,Casters",PIFDC3072T,PIFDC3072T-74P:GA1:NMP:4EC,30,36,72,74P,GA1,(1) Grommet - Nacre,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, (1) Grommet - Nacre, Casters",GA1:NMP:4EC,0,6
"29Hx30-36Dx72W,(1) Grommet - Dean,Casters",PIFDC3072T,PIFDC3072T-74P:GD1:NMP:4EC,30,36,72,74P,GD1,(1) Grommet - Dean,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, (1) Grommet - Dean, Casters",GD1:NMP:4EC,0,7
"29Hx30-36Dx72W,(1) Grommet - Node,Casters",PIFDC3072T,PIFDC3072T-74P:GO1:NMP:4EC,30,36,72,74P,GO1,(1) Grommet - Node,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, (1) Grommet - Node, Casters",GO1:NMP:4EC,0,8
"29Hx30-36Dx72W,No Power,Glides",PIFDC3072T,PIFDC3072T-74P,30,36,72,74P,NNN,None,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, No Power, Glides",NNN:NMP:4GB,1,0
"29Hx30-36Dx72W,Wire Management Only,Glides",PIFDC3072T,PIFDC3072T-74P:WMO:NMP:4GB,30,36,72,74P,WMO,Wire Management Only,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, Wire Management Only, Glides",WMO:NMP:4GB,1,1
"29Hx30-36Dx72W,(1) Nacre In-Surface Module,Glides",PIFDC3072T,PIFDC3072T-74P:MA1:NMP:4GB,30,36,72,74P,MA1,(1) Nacre In-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, (1) Nacre In-Surface Module, Glides",MA1:NMP:4GB,1,2
"29Hx30-36Dx72W,(1) Dubble Under-Surface Module,Glides",PIFDC3072T,PIFDC3072T-74P:MB1:NMP:4GB,30,36,72,74P,MB1,(1) Dubble Under-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, (1) Dubble Under-Surface Module, Glides",MB1:NMP:4GB,1,3
"29Hx30-36Dx72W,(1) Dean In-Surface Module,Glides",PIFDC3072T,PIFDC3072T-74P:MD1:NMP:4GB,30,36,72,74P,MD1,(1) Dean In-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, (1) Dean In-Surface Module, Glides",MD1:NMP:4GB,1,4
"29Hx30-36Dx72W,(1) Node In Surface Module,Glides",PIFDC3072T,PIFDC3072T-74P:MO1:NMP:4GB,30,36,72,74P,MO1,(1) Node In Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, (1) Node In Surface Module, Glides",MO1:NMP:4GB,1,5
"29Hx30-36Dx72W,(1) Grommet - Nacre,Glides",PIFDC3072T,PIFDC3072T-74P:GA1:NMP:4GB,30,36,72,74P,GA1,(1) Grommet - Nacre,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, (1) Grommet - Nacre, Glides",GA1:NMP:4GB,1,6
"29Hx30-36Dx72W,(1) Grommet - Dean,Glides",PIFDC3072T,PIFDC3072T-74P:GD1:NMP:4GB,30,36,72,74P,GD1,(1) Grommet - Dean,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, (1) Grommet - Dean, Glides",GD1:NMP:4GB,1,7
"29Hx30-36Dx72W,(1) Grommet - Node,Glides",PIFDC3072T,PIFDC3072T-74P:GO1:NMP:4GB,30,36,72,74P,GO1,(1) Grommet - Node,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 30""-36""D x 72""W, 29""H, 74P Edge, (1) Grommet - Node, Glides",GO1:NMP:4GB,1,8
"29Hx36-42Dx60W,No Power,Casters",PIFDC3660T,PIFDC3660T-74P:NNN:NMP:4EC,36,42,60,74P,NNN,None,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, No Power, Casters",NNN:NMP:4EC,0,0
"29Hx36-42Dx60W,Wire Management Only,Casters",PIFDC3660T,PIFDC3660T-74P:WMO:NMP:4EC,36,42,60,74P,WMO,Wire Management Only,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, Wire Management Only, Casters",WMO:NMP:4EC,0,1
"29Hx36-42Dx60W,(1) Nacre In-Surface Module,Casters",PIFDC3660T,PIFDC3660T-74P:MA1:NMP:4EC,36,42,60,74P,MA1,(1) Nacre In-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, (1) Nacre In-Surface Module, Casters",MA1:NMP:4EC,0,2
"29Hx36-42Dx60W,(1) Dubble Under-Surface Module,Casters",PIFDC3660T,PIFDC3660T-74P:MB1:NMP:4EC,36,42,60,74P,MB1,(1) Dubble Under-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, (1) Dubble Under-Surface Module, Casters",MB1:NMP:4EC,0,3
"29Hx36-42Dx60W,(1) Dean In-Surface Module,Casters",PIFDC3660T,PIFDC3660T-74P:MD1:NMP:4EC,36,42,60,74P,MD1,(1) Dean In-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, (1) Dean In-Surface Module, Casters",MD1:NMP:4EC,0,4
"29Hx36-42Dx60W,(1) Node In Surface Module,Casters",PIFDC3660T,PIFDC3660T-74P:MO1:NMP:4EC,36,42,60,74P,MO1,(1) Node In Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, (1) Node In Surface Module, Casters",MO1:NMP:4EC,0,5
"29Hx36-42Dx60W,(1) Grommet - Nacre,Casters",PIFDC3660T,PIFDC3660T-74P:GA1:NMP:4EC,36,42,60,74P,GA1,(1) Grommet - Nacre,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, (1) Grommet - Nacre, Casters",GA1:NMP:4EC,0,6
"29Hx36-42Dx60W,(1) Grommet - Dean,Casters",PIFDC3660T,PIFDC3660T-74P:GD1:NMP:4EC,36,42,60,74P,GD1,(1) Grommet - Dean,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, (1) Grommet - Dean, Casters",GD1:NMP:4EC,0,7
"29Hx36-42Dx60W,(1) Grommet - Node,Casters",PIFDC3660T,PIFDC3660T-74P:GO1:NMP:4EC,36,42,60,74P,GO1,(1) Grommet - Node,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, (1) Grommet - Node, Casters",GO1:NMP:4EC,0,8
"29Hx36-42Dx60W,No Power,Glides",PIFDC3660T,PIFDC3660T-74P,36,42,60,74P,NNN,None,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, No Power, Glides",NNN:NMP:4GB,1,0
"29Hx36-42Dx60W,Wire Management Only,Glides",PIFDC3660T,PIFDC3660T-74P:WMO:NMP:4GB,36,42,60,74P,WMO,Wire Management Only,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, Wire Management Only, Glides",WMO:NMP:4GB,1,1
"29Hx36-42Dx60W,(1) Nacre In-Surface Module,Glides",PIFDC3660T,PIFDC3660T-74P:MA1:NMP:4GB,36,42,60,74P,MA1,(1) Nacre In-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, (1) Nacre In-Surface Module, Glides",MA1:NMP:4GB,1,2
"29Hx36-42Dx60W,(1) Dubble Under-Surface Module,Glides",PIFDC3660T,PIFDC3660T-74P:MB1:NMP:4GB,36,42,60,74P,MB1,(1) Dubble Under-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, (1) Dubble Under-Surface Module, Glides",MB1:NMP:4GB,1,3
"29Hx36-42Dx60W,(1) Dean In-Surface Module,Glides",PIFDC3660T,PIFDC3660T-74P:MD1:NMP:4GB,36,42,60,74P,MD1,(1) Dean In-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, (1) Dean In-Surface Module, Glides",MD1:NMP:4GB,1,4
"29Hx36-42Dx60W,(1) Node In Surface Module,Glides",PIFDC3660T,PIFDC3660T-74P:MO1:NMP:4GB,36,42,60,74P,MO1,(1) Node In Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, (1) Node In Surface Module, Glides",MO1:NMP:4GB,1,5
"29Hx36-42Dx60W,(1) Grommet - Nacre,Glides",PIFDC3660T,PIFDC3660T-74P:GA1:NMP:4GB,36,42,60,74P,GA1,(1) Grommet - Nacre,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, (1) Grommet - Nacre, Glides",GA1:NMP:4GB,1,6
"29Hx36-42Dx60W,(1) Grommet - Dean,Glides",PIFDC3660T,PIFDC3660T-74P:GD1:NMP:4GB,36,42,60,74P,GD1,(1) Grommet - Dean,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, (1) Grommet - Dean, Glides",GD1:NMP:4GB,1,7
"29Hx36-42Dx60W,(1) Grommet - Node,Glides",PIFDC3660T,PIFDC3660T-74P:GO1:NMP:4GB,36,42,60,74P,GO1,(1) Grommet - Node,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 60""W, 29""H, 74P Edge, (1) Grommet - Node, Glides",GO1:NMP:4GB,1,8
"29Hx36-42Dx72W,No Power,Casters",PIFDC3672T,PIFDC3672T-74P:NNN:NMP:4EC,36,42,72,74P,NNN,None,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, No Power, Casters",NNN:NMP:4EC,0,0
"29Hx36-42Dx72W,Wire Management Only,Casters",PIFDC3672T,PIFDC3672T-74P:WMO:NMP:4EC,36,42,72,74P,WMO,Wire Management Only,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, Wire Management Only, Casters",WMO:NMP:4EC,0,1
"29Hx36-42Dx72W,(1) Nacre In-Surface Module,Casters",PIFDC3672T,PIFDC3672T-74P:MA1:NMP:4EC,36,42,72,74P,MA1,(1) Nacre In-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, (1) Nacre In-Surface Module, Casters",MA1:NMP:4EC,0,2
"29Hx36-42Dx72W,(1) Dubble Under-Surface Module,Casters",PIFDC3672T,PIFDC3672T-74P:MB1:NMP:4EC,36,42,72,74P,MB1,(1) Dubble Under-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, (1) Dubble Under-Surface Module, Casters",MB1:NMP:4EC,0,3
"29Hx36-42Dx72W,(1) Dean In-Surface Module,Casters",PIFDC3672T,PIFDC3672T-74P:MD1:NMP:4EC,36,42,72,74P,MD1,(1) Dean In-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, (1) Dean In-Surface Module, Casters",MD1:NMP:4EC,0,4
"29Hx36-42Dx72W,(1) Node In Surface Module,Casters",PIFDC3672T,PIFDC3672T-74P:MO1:NMP:4EC,36,42,72,74P,MO1,(1) Node In Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, (1) Node In Surface Module, Casters",MO1:NMP:4EC,0,5
"29Hx36-42Dx72W,(1) Grommet - Nacre,Casters",PIFDC3672T,PIFDC3672T-74P:GA1:NMP:4EC,36,42,72,74P,GA1,(1) Grommet - Nacre,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, (1) Grommet - Nacre, Casters",GA1:NMP:4EC,0,6
"29Hx36-42Dx72W,(1) Grommet - Dean,Casters",PIFDC3672T,PIFDC3672T-74P:GD1:NMP:4EC,36,42,72,74P,GD1,(1) Grommet - Dean,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, (1) Grommet - Dean, Casters",GD1:NMP:4EC,0,7
"29Hx36-42Dx72W,(1) Grommet - Node,Casters",PIFDC3672T,PIFDC3672T-74P:GO1:NMP:4EC,36,42,72,74P,GO1,(1) Grommet - Node,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, (1) Grommet - Node, Casters",GO1:NMP:4EC,0,8
"29Hx36-42Dx72W,No Power,Glides",PIFDC3672T,PIFDC3672T-74P,36,42,72,74P,NNN,None,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, No Power, Glides",NNN:NMP:4GB,1,0
"29Hx36-42Dx72W,Wire Management Only,Glides",PIFDC3672T,PIFDC3672T-74P:WMO:NMP:4GB,36,42,72,74P,WMO,Wire Management Only,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, Wire Management Only, Glides",WMO:NMP:4GB,1,1
"29Hx36-42Dx72W,(1) Nacre In-Surface Module,Glides",PIFDC3672T,PIFDC3672T-74P:MA1:NMP:4GB,36,42,72,74P,MA1,(1) Nacre In-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, (1) Nacre In-Surface Module, Glides",MA1:NMP:4GB,1,2
"29Hx36-42Dx72W,(1) Dubble Under-Surface Module,Glides",PIFDC3672T,PIFDC3672T-74P:MB1:NMP:4GB,36,42,72,74P,MB1,(1) Dubble Under-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, (1) Dubble Under-Surface Module, Glides",MB1:NMP:4GB,1,3
"29Hx36-42Dx72W,(1) Dean In-Surface Module,Glides",PIFDC3672T,PIFDC3672T-74P:MD1:NMP:4GB,36,42,72,74P,MD1,(1) Dean In-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, (1) Dean In-Surface Module, Glides",MD1:NMP:4GB,1,4
"29Hx36-42Dx72W,(1) Node In Surface Module,Glides",PIFDC3672T,PIFDC3672T-74P:MO1:NMP:4GB,36,42,72,74P,MO1,(1) Node In Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, (1) Node In Surface Module, Glides",MO1:NMP:4GB,1,5
"29Hx36-42Dx72W,(1) Grommet - Nacre,Glides",PIFDC3672T,PIFDC3672T-74P:GA1:NMP:4GB,36,42,72,74P,GA1,(1) Grommet - Nacre,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, (1) Grommet - Nacre, Glides",GA1:NMP:4GB,1,6
"29Hx36-42Dx72W,(1) Grommet - Dean,Glides",PIFDC3672T,PIFDC3672T-74P:GD1:NMP:4GB,36,42,72,74P,GD1,(1) Grommet - Dean,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, (1) Grommet - Dean, Glides",GD1:NMP:4GB,1,7
"29Hx36-42Dx72W,(1) Grommet - Node,Glides",PIFDC3672T,PIFDC3672T-74P:GO1:NMP:4GB,36,42,72,74P,GO1,(1) Grommet - Node,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 72""W, 29""H, 74P Edge, (1) Grommet - Node, Glides",GO1:NMP:4GB,1,8
"29Hx36-42Dx84W,No Power,Casters",PIFDC3684T,PIFDC3684T-74P:NNN:NMP:4EC,36,42,84,74P,NNN,None,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, No Power, Casters",NNN:NMP:4EC,0,0
"29Hx36-42Dx84W,Wire Management Only,Casters",PIFDC3684T,PIFDC3684T-74P:WMO:NMP:4EC,36,42,84,74P,WMO,Wire Management Only,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, Wire Management Only, Casters",WMO:NMP:4EC,0,1
"29Hx36-42Dx84W,(2) Nacre In-Surface Module,Casters",PIFDC3684T,PIFDC3684T-74P:MA2:NMP:4EC,36,42,84,74P,MA2,(2) Nacre In-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, (2) Nacre In-Surface Module, Casters",MA2:NMP:4EC,0,9
"29Hx36-42Dx84W,(2) Dubble Under-Surface Module,Casters",PIFDC3684T,PIFDC3684T-74P:MB2:NMP:4EC,36,42,84,74P,MB2,(2) Dubble Under-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, (2) Dubble Under-Surface Module, Casters",MB2:NMP:4EC,0,10
"29Hx36-42Dx84W,(2) Dean In-Surface Module,Casters",PIFDC3684T,PIFDC3684T-74P:MD2:NMP:4EC,36,42,84,74P,MD2,(2) Dean In-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, (2) Dean In-Surface Module, Casters",MD2:NMP:4EC,0,11
"29Hx36-42Dx84W,(2) Node In Surface Module,Casters",PIFDC3684T,PIFDC3684T-74P:MO2:NMP:4EC,36,42,84,74P,MO2,(2) Node In Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, (2) Node In Surface Module, Casters",MO2:NMP:4EC,0,12
"29Hx36-42Dx84W,(2) Grommet - Nacre,Casters",PIFDC3684T,PIFDC3684T-74P:GA2:NMP:4EC,36,42,84,74P,GA2,(2) Grommet - Nacre,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, (2) Grommet - Nacre, Casters",GA2:NMP:4EC,0,13
"29Hx36-42Dx84W,(2) Grommet - Dean,Casters",PIFDC3684T,PIFDC3684T-74P:GD2:NMP:4EC,36,42,84,74P,GD2,(2) Grommet - Dean,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, (2) Grommet - Dean, Casters",GD2:NMP:4EC,0,14
"29Hx36-42Dx84W,(2) Grommet - Node,Casters",PIFDC3684T,PIFDC3684T-74P:GO2:NMP:4EC,36,42,84,74P,GO2,(2) Grommet - Node,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, (2) Grommet - Node, Casters",GO2:NMP:4EC,0,15
"29Hx36-42Dx84W,No Power,Glides",PIFDC3684T,PIFDC3684T-74P,36,42,84,74P,NNN,None,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, No Power, Glides",NNN:NMP:4GB,1,0
"29Hx36-42Dx84W,Wire Management Only,Glides",PIFDC3684T,PIFDC3684T-74P:WMO:NMP:4GB,36,42,84,74P,WMO,Wire Management Only,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, Wire Management Only, Glides",WMO:NMP:4GB,1,1
"29Hx36-42Dx84W,(2) Nacre In-Surface Module,Glides",PIFDC3684T,PIFDC3684T-74P:MA2:NMP:4GB,36,42,84,74P,MA2,(2) Nacre In-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, (2) Nacre In-Surface Module, Glides",MA2:NMP:4GB,1,9
"29Hx36-42Dx84W,(2) Dubble Under-Surface Module,Glides",PIFDC3684T,PIFDC3684T-74P:MB2:NMP:4GB,36,42,84,74P,MB2,(2) Dubble Under-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, (2) Dubble Under-Surface Module, Glides",MB2:NMP:4GB,1,10
"29Hx36-42Dx84W,(2) Dean In-Surface Module,Glides",PIFDC3684T,PIFDC3684T-74P:MD2:NMP:4GB,36,42,84,74P,MD2,(2) Dean In-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, (2) Dean In-Surface Module, Glides",MD2:NMP:4GB,1,11
"29Hx36-42Dx84W,(2) Node In Surface Module,Glides",PIFDC3684T,PIFDC3684T-74P:MO2:NMP:4GB,36,42,84,74P,MO2,(2) Node In Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, (2) Node In Surface Module, Glides",MO2:NMP:4GB,1,12
"29Hx36-42Dx84W,(2) Grommet - Nacre,Glides",PIFDC3684T,PIFDC3684T-74P:GA2:NMP:4GB,36,42,84,74P,GA2,(2) Grommet - Nacre,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, (2) Grommet - Nacre, Glides",GA2:NMP:4GB,1,13
"29Hx36-42Dx84W,(2) Grommet - Dean,Glides",PIFDC3684T,PIFDC3684T-74P:GD2:NMP:4GB,36,42,84,74P,GD2,(2) Grommet - Dean,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, (2) Grommet - Dean, Glides",GD2:NMP:4GB,1,14
"29Hx36-42Dx84W,(2) Grommet - Node,Glides",PIFDC3684T,PIFDC3684T-74P:GO2:NMP:4GB,36,42,84,74P,GO2,(2) Grommet - Node,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 84""W, 29""H, 74P Edge, (2) Grommet - Node, Glides",GO2:NMP:4GB,1,15
"29Hx36-42Dx96W,No Power,Casters",PIFDC3696T,PIFDC3696T-74P:NNN:NMP:4EC,36,42,96,74P,NNN,None,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, No Power, Casters",NNN:NMP:4EC,0,0
"29Hx36-42Dx96W,Wire Management Only,Casters",PIFDC3696T,PIFDC3696T-74P:WMO:NMP:4EC,36,42,96,74P,WMO,Wire Management Only,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, Wire Management Only, Casters",WMO:NMP:4EC,0,1
"29Hx36-42Dx96W,(2) Nacre In-Surface Module,Casters",PIFDC3696T,PIFDC3696T-74P:MA2:NMP:4EC,36,42,96,74P,MA2,(2) Nacre In-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, (2) Nacre In-Surface Module, Casters",MA2:NMP:4EC,0,9
"29Hx36-42Dx96W,(2) Dubble Under-Surface Module,Casters",PIFDC3696T,PIFDC3696T-74P:MB2:NMP:4EC,36,42,96,74P,MB2,(2) Dubble Under-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, (2) Dubble Under-Surface Module, Casters",MB2:NMP:4EC,0,10
"29Hx36-42Dx96W,(2) Dean In-Surface Module,Casters",PIFDC3696T,PIFDC3696T-74P:MD2:NMP:4EC,36,42,96,74P,MD2,(2) Dean In-Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, (2) Dean In-Surface Module, Casters",MD2:NMP:4EC,0,11
"29Hx36-42Dx96W,(2) Node In Surface Module,Casters",PIFDC3696T,PIFDC3696T-74P:MO2:NMP:4EC,36,42,96,74P,MO2,(2) Node In Surface Module,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, (2) Node In Surface Module, Casters",MO2:NMP:4EC,0,12
"29Hx36-42Dx96W,(2) Grommet - Nacre,Casters",PIFDC3696T,PIFDC3696T-74P:GA2:NMP:4EC,36,42,96,74P,GA2,(2) Grommet - Nacre,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, (2) Grommet - Nacre, Casters",GA2:NMP:4EC,0,13
"29Hx36-42Dx96W,(2) Grommet - Dean,Casters",PIFDC3696T,PIFDC3696T-74P:GD2:NMP:4EC,36,42,96,74P,GD2,(2) Grommet - Dean,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, (2) Grommet - Dean, Casters",GD2:NMP:4EC,0,14
"29Hx36-42Dx96W,(2) Grommet - Node,Casters",PIFDC3696T,PIFDC3696T-74P:GO2:NMP:4EC,36,42,96,74P,GO2,(2) Grommet - Node,Casters,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, (2) Grommet - Node, Casters",GO2:NMP:4EC,0,15
"29Hx36-42Dx96W,No Power,Glides",PIFDC3696T,PIFDC3696T-74P,36,42,96,74P,NNN,None,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, No Power, Glides",NNN:NMP:4GB,1,0
"29Hx36-42Dx96W,Wire Management Only,Glides",PIFDC3696T,PIFDC3696T-74P:WMO:NMP:4GB,36,42,96,74P,WMO,Wire Management Only,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, Wire Management Only, Glides",WMO:NMP:4GB,1,1
"29Hx36-42Dx96W,(2) Nacre In-Surface Module,Glides",PIFDC3696T,PIFDC3696T-74P:MA2:NMP:4GB,36,42,96,74P,MA2,(2) Nacre In-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, (2) Nacre In-Surface Module, Glides",MA2:NMP:4GB,1,9
"29Hx36-42Dx96W,(2) Dubble Under-Surface Module,Glides",PIFDC3696T,PIFDC3696T-74P:MB2:NMP:4GB,36,42,96,74P,MB2,(2) Dubble Under-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, (2) Dubble Under-Surface Module, Glides",MB2:NMP:4GB,1,10
"29Hx36-42Dx96W,(2) Dean In-Surface Module,Glides",PIFDC3696T,PIFDC3696T-74P:MD2:NMP:4GB,36,42,96,74P,MD2,(2) Dean In-Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, (2) Dean In-Surface Module, Glides",MD2:NMP:4GB,1,11
"29Hx36-42Dx96W,(2) Node In Surface Module,Glides",PIFDC3696T,PIFDC3696T-74P:MO2:NMP:4GB,36,42,96,74P,MO2,(2) Node In Surface Module,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, (2) Node In Surface Module, Glides",MO2:NMP:4GB,1,12
"29Hx36-42Dx96W,(2) Grommet - Nacre,Glides",PIFDC3696T,PIFDC3696T-74P:GA2:NMP:4GB,36,42,96,74P,GA2,(2) Grommet - Nacre,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, (2) Grommet - Nacre, Glides",GA2:NMP:4GB,1,13
"29Hx36-42Dx96W,(2) Grommet - Dean,Glides",PIFDC3696T,PIFDC3696T-74P:GD2:NMP:4GB,36,42,96,74P,GD2,(2) Grommet - Dean,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, (2) Grommet - Dean, Glides",GD2:NMP:4GB,1,14
"29Hx36-42Dx96W,(2) Grommet - Node,Glides",PIFDC3696T,PIFDC3696T-74P:GO2:NMP:4GB,36,42,96,74P,GO2,(2) Grommet - Node,Glides,"Pirouette Fixed Double Chevon Standard Height Table - 36""-42""D x 96""W, 29""H, 74P Edge, (2) Grommet - Node, Glides",GO2:NMP:4GB,1,15
