,Base Model##Other##,Model##Other##,Table Height##Length##inches,Depth##Length##inches,Width##Length##inches,Edge Style##Other##,Power Option##Other##,Power Option Description##Other##,Modesty##Other##,Base Style##Other##,Description##Other##,Option##Other##,Has Fabric Modesty##Other##,Has Polyester Modesty##Other##,Has Glide##Other##,Power Style##Other##
"29Hx24Dx60W,Nacre In-Surface Pattern Module,No Modesty Panel,Casters",PAFCV2460,PAFCV2460-74P:PMA1:NMP:4EC,29,24,60,74P,PMA1,Nacre In-Surface Pattern Module,No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Nacre In-Surface Pattern Module, No Modesty Panel, Casters",PMA1:NMP:4EC,0,0,0,0
"29Hx24Dx60W,Dubble Under-Surface Pattern Module,No Modesty Panel,Casters",PAFCV2460,PAFCV2460-74P:PMB1:NMP:4EC,29,24,60,74P,PMB1,Dubble Under-Surface Pattern Module,No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Dubble Under-Surface Pattern Module, No Modesty Panel, Casters",PMB1:NMP:4EC,0,0,0,1
"29Hx24Dx60W,Dean In-Surface Pattern Module,No Modesty Panel,Casters",PAFCV2460,PAFCV2460-74P:PMD1:NMP:4EC,29,24,60,74P,PMD1,Dean In-Surface Pattern Module,No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Dean In-Surface Pattern Module, No Modesty Panel, Casters",PMD1:NMP:4EC,0,0,0,2
"29Hx24Dx60W,Node In Surface Pattern Module,No Modesty Panel,Casters",PAFCV2460,PAFCV2460-74P:PMO1:NMP:4EC,29,24,60,74P,PMO1,Node In Surface Pattern Module,No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Node In Surface Pattern Module, No Modesty Panel, Casters",PMO1:NMP:4EC,0,0,0,3
"29Hx24Dx60W,Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1),No Modesty Panel,Casters",PAFCV2460,PAFCV2460-74P:PS2GA1:NMP:4EC,29,24,60,74P,PS2GA1,"Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1)",No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1), No Modesty Panel, Casters",PS2GA1:NMP:4EC,0,0,0,10
"29Hx24Dx60W,Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1),No Modesty Panel,Casters",PAFCV2460,PAFCV2460-74P:PS2MB1GA1:NMP:4EC,29,24,60,74P,PS2MB1GA1,"Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1)",No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1), No Modesty Panel, Casters",PS2MB1GA1:NMP:4EC,0,0,0,11
"29Hx24Dx60W,Nacre In-Surface Pattern Module,No Modesty Panel,Glides",PAFCV2460,PAFCV2460-74P,29,24,60,74P,PMA1,Nacre In-Surface Pattern Module,No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Nacre In-Surface Pattern Module, No Modesty Panel, Glides",PMA1:NMP:4GB,0,0,1,0
"29Hx24Dx60W,Dubble Under-Surface Pattern Module,No Modesty Panel,Glides",PAFCV2460,PAFCV2460-74P:PMB1:NMP:4GB,29,24,60,74P,PMB1,Dubble Under-Surface Pattern Module,No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Dubble Under-Surface Pattern Module, No Modesty Panel, Glides",PMB1:NMP:4GB,0,0,1,1
"29Hx24Dx60W,Dean In-Surface Pattern Module,No Modesty Panel,Glides",PAFCV2460,PAFCV2460-74P:PMD1:NMP:4GB,29,24,60,74P,PMD1,Dean In-Surface Pattern Module,No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Dean In-Surface Pattern Module, No Modesty Panel, Glides",PMD1:NMP:4GB,0,0,1,2
"29Hx24Dx60W,Node In Surface Pattern Module,No Modesty Panel,Glides",PAFCV2460,PAFCV2460-74P:PMO1:NMP:4GB,29,24,60,74P,PMO1,Node In Surface Pattern Module,No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Node In Surface Pattern Module, No Modesty Panel, Glides",PMO1:NMP:4GB,0,0,1,3
"29Hx24Dx60W,Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1),No Modesty Panel,Glides",PAFCV2460,PAFCV2460-74P:PS2GA1:NMP:4GB,29,24,60,74P,PS2GA1,"Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1)",No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1), No Modesty Panel, Glides",PS2GA1:NMP:4GB,0,0,1,10
"29Hx24Dx60W,Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1),No Modesty Panel,Glides",PAFCV2460,PAFCV2460-74P:PS2MB1GA1:NMP:4GB,29,24,60,74P,PS2MB1GA1,"Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1)",No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1), No Modesty Panel, Glides",PS2MB1GA1:NMP:4GB,0,0,1,11
"29Hx24Dx60W,Nacre In-Surface Pattern Module,Polyester Modesty Panel,Casters",PAFCV2460,PAFCV2460-74P:PMA1:PMP:4EC,29,24,60,74P,PMA1,Nacre In-Surface Pattern Module,Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Nacre In-Surface Pattern Module, Polyester Modesty Panel, Casters",PMA1:PMP:4EC,0,1,0,0
"29Hx24Dx60W,Dubble Under-Surface Pattern Module,Polyester Modesty Panel,Casters",PAFCV2460,PAFCV2460-74P:PMB1:PMP:4EC,29,24,60,74P,PMB1,Dubble Under-Surface Pattern Module,Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Dubble Under-Surface Pattern Module, Polyester Modesty Panel, Casters",PMB1:PMP:4EC,0,1,0,1
"29Hx24Dx60W,Dean In-Surface Pattern Module,Polyester Modesty Panel,Casters",PAFCV2460,PAFCV2460-74P:PMD1:PMP:4EC,29,24,60,74P,PMD1,Dean In-Surface Pattern Module,Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Dean In-Surface Pattern Module, Polyester Modesty Panel, Casters",PMD1:PMP:4EC,0,1,0,2
"29Hx24Dx60W,Node In Surface Pattern Module,Polyester Modesty Panel,Casters",PAFCV2460,PAFCV2460-74P:PMO1:PMP:4EC,29,24,60,74P,PMO1,Node In Surface Pattern Module,Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Node In Surface Pattern Module, Polyester Modesty Panel, Casters",PMO1:PMP:4EC,0,1,0,3
"29Hx24Dx60W,Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1),Polyester Modesty Panel,Casters",PAFCV2460,PAFCV2460-74P:PS2GA1:PMP:4EC,29,24,60,74P,PS2GA1,"Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1)",Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1), Polyester Modesty Panel, Casters",PS2GA1:PMP:4EC,0,1,0,10
"29Hx24Dx60W,Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1),Polyester Modesty Panel,Casters",PAFCV2460,PAFCV2460-74P:PS2MB1GA1:PMP:4EC,29,24,60,74P,PS2MB1GA1,"Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1)",Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1), Polyester Modesty Panel, Casters",PS2MB1GA1:PMP:4EC,0,1,0,11
"29Hx24Dx60W,Nacre In-Surface Pattern Module,Polyester Modesty Panel,Glides",PAFCV2460,PAFCV2460-74P:PMA1:PMP:4GB,29,24,60,74P,PMA1,Nacre In-Surface Pattern Module,Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Nacre In-Surface Pattern Module, Polyester Modesty Panel, Glides",PMA1:PMP:4GB,0,1,1,0
"29Hx24Dx60W,Dubble Under-Surface Pattern Module,Polyester Modesty Panel,Glides",PAFCV2460,PAFCV2460-74P:PMB1:PMP:4GB,29,24,60,74P,PMB1,Dubble Under-Surface Pattern Module,Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Dubble Under-Surface Pattern Module, Polyester Modesty Panel, Glides",PMB1:PMP:4GB,0,1,1,1
"29Hx24Dx60W,Dean In-Surface Pattern Module,Polyester Modesty Panel,Glides",PAFCV2460,PAFCV2460-74P:PMD1:PMP:4GB,29,24,60,74P,PMD1,Dean In-Surface Pattern Module,Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Dean In-Surface Pattern Module, Polyester Modesty Panel, Glides",PMD1:PMP:4GB,0,1,1,2
"29Hx24Dx60W,Node In Surface Pattern Module,Polyester Modesty Panel,Glides",PAFCV2460,PAFCV2460-74P:PMO1:PMP:4GB,29,24,60,74P,PMO1,Node In Surface Pattern Module,Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Node In Surface Pattern Module, Polyester Modesty Panel, Glides",PMO1:PMP:4GB,0,1,1,3
"29Hx24Dx60W,Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1),Polyester Modesty Panel,Glides",PAFCV2460,PAFCV2460-74P:PS2GA1:PMP:4GB,29,24,60,74P,PS2GA1,"Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1)",Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1), Polyester Modesty Panel, Glides",PS2GA1:PMP:4GB,0,1,1,10
"29Hx24Dx60W,Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1),Polyester Modesty Panel,Glides",PAFCV2460,PAFCV2460-74P:PS2MB1GA1:PMP:4GB,29,24,60,74P,PS2MB1GA1,"Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1)",Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 60""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1), Polyester Modesty Panel, Glides",PS2MB1GA1:PMP:4GB,0,1,1,11
"29Hx24Dx72W,Nacre In-Surface Pattern Module,No Modesty Panel,Casters",PAFCV2472,PAFCV2472-74P:PMA1:NMP:4EC,29,24,72,74P,PMA1,Nacre In-Surface Pattern Module,No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Nacre In-Surface Pattern Module, No Modesty Panel, Casters",PMA1:NMP:4EC,0,0,0,0
"29Hx24Dx72W,Dubble Under-Surface Pattern Module,No Modesty Panel,Casters",PAFCV2472,PAFCV2472-74P:PMB1:NMP:4EC,29,24,72,74P,PMB1,Dubble Under-Surface Pattern Module,No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Dubble Under-Surface Pattern Module, No Modesty Panel, Casters",PMB1:NMP:4EC,0,0,0,1
"29Hx24Dx72W,Dean In-Surface Pattern Module,No Modesty Panel,Casters",PAFCV2472,PAFCV2472-74P:PMD1:NMP:4EC,29,24,72,74P,PMD1,Dean In-Surface Pattern Module,No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Dean In-Surface Pattern Module, No Modesty Panel, Casters",PMD1:NMP:4EC,0,0,0,2
"29Hx24Dx72W,Node In Surface Pattern Module,No Modesty Panel,Casters",PAFCV2472,PAFCV2472-74P:PMO1:NMP:4EC,29,24,72,74P,PMO1,Node In Surface Pattern Module,No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Node In Surface Pattern Module, No Modesty Panel, Casters",PMO1:NMP:4EC,0,0,0,3
"29Hx24Dx72W,Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1),No Modesty Panel,Casters",PAFCV2472,PAFCV2472-74P:PS2GA1:NMP:4EC,29,24,72,74P,PS2GA1,"Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1)",No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1), No Modesty Panel, Casters",PS2GA1:NMP:4EC,0,0,0,10
"29Hx24Dx72W,Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1),No Modesty Panel,Casters",PAFCV2472,PAFCV2472-74P:PS2MB1GA1:NMP:4EC,29,24,72,74P,PS2MB1GA1,"Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1)",No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1), No Modesty Panel, Casters",PS2MB1GA1:NMP:4EC,0,0,0,11
"29Hx24Dx72W,Nacre In-Surface Pattern Module,No Modesty Panel,Glides",PAFCV2472,PAFCV2472-74P,29,24,72,74P,PMA1,Nacre In-Surface Pattern Module,No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Nacre In-Surface Pattern Module, No Modesty Panel, Glides",PMA1:NMP:4GB,0,0,1,0
"29Hx24Dx72W,Dubble Under-Surface Pattern Module,No Modesty Panel,Glides",PAFCV2472,PAFCV2472-74P:PMB1:NMP:4GB,29,24,72,74P,PMB1,Dubble Under-Surface Pattern Module,No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Dubble Under-Surface Pattern Module, No Modesty Panel, Glides",PMB1:NMP:4GB,0,0,1,1
"29Hx24Dx72W,Dean In-Surface Pattern Module,No Modesty Panel,Glides",PAFCV2472,PAFCV2472-74P:PMD1:NMP:4GB,29,24,72,74P,PMD1,Dean In-Surface Pattern Module,No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Dean In-Surface Pattern Module, No Modesty Panel, Glides",PMD1:NMP:4GB,0,0,1,2
"29Hx24Dx72W,Node In Surface Pattern Module,No Modesty Panel,Glides",PAFCV2472,PAFCV2472-74P:PMO1:NMP:4GB,29,24,72,74P,PMO1,Node In Surface Pattern Module,No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Node In Surface Pattern Module, No Modesty Panel, Glides",PMO1:NMP:4GB,0,0,1,3
"29Hx24Dx72W,Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1),No Modesty Panel,Glides",PAFCV2472,PAFCV2472-74P:PS2GA1:NMP:4GB,29,24,72,74P,PS2GA1,"Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1)",No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1), No Modesty Panel, Glides",PS2GA1:NMP:4GB,0,0,1,10
"29Hx24Dx72W,Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1),No Modesty Panel,Glides",PAFCV2472,PAFCV2472-74P:PS2MB1GA1:NMP:4GB,29,24,72,74P,PS2MB1GA1,"Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1)",No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1), No Modesty Panel, Glides",PS2MB1GA1:NMP:4GB,0,0,1,11
"29Hx24Dx72W,Nacre In-Surface Pattern Module,Polyester Modesty Panel,Casters",PAFCV2472,PAFCV2472-74P:PMA1:PMP:4EC,29,24,72,74P,PMA1,Nacre In-Surface Pattern Module,Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Nacre In-Surface Pattern Module, Polyester Modesty Panel, Casters",PMA1:PMP:4EC,0,1,0,0
"29Hx24Dx72W,Dubble Under-Surface Pattern Module,Polyester Modesty Panel,Casters",PAFCV2472,PAFCV2472-74P:PMB1:PMP:4EC,29,24,72,74P,PMB1,Dubble Under-Surface Pattern Module,Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Dubble Under-Surface Pattern Module, Polyester Modesty Panel, Casters",PMB1:PMP:4EC,0,1,0,1
"29Hx24Dx72W,Dean In-Surface Pattern Module,Polyester Modesty Panel,Casters",PAFCV2472,PAFCV2472-74P:PMD1:PMP:4EC,29,24,72,74P,PMD1,Dean In-Surface Pattern Module,Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Dean In-Surface Pattern Module, Polyester Modesty Panel, Casters",PMD1:PMP:4EC,0,1,0,2
"29Hx24Dx72W,Node In Surface Pattern Module,Polyester Modesty Panel,Casters",PAFCV2472,PAFCV2472-74P:PMO1:PMP:4EC,29,24,72,74P,PMO1,Node In Surface Pattern Module,Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Node In Surface Pattern Module, Polyester Modesty Panel, Casters",PMO1:PMP:4EC,0,1,0,3
"29Hx24Dx72W,Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1),Polyester Modesty Panel,Casters",PAFCV2472,PAFCV2472-74P:PS2GA1:PMP:4EC,29,24,72,74P,PS2GA1,"Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1)",Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1), Polyester Modesty Panel, Casters",PS2GA1:PMP:4EC,0,1,0,10
"29Hx24Dx72W,Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1),Polyester Modesty Panel,Casters",PAFCV2472,PAFCV2472-74P:PS2MB1GA1:PMP:4EC,29,24,72,74P,PS2MB1GA1,"Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1)",Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1), Polyester Modesty Panel, Casters",PS2MB1GA1:PMP:4EC,0,1,0,11
"29Hx24Dx72W,Nacre In-Surface Pattern Module,Polyester Modesty Panel,Glides",PAFCV2472,PAFCV2472-74P:PMA1:PMP:4GB,29,24,72,74P,PMA1,Nacre In-Surface Pattern Module,Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Nacre In-Surface Pattern Module, Polyester Modesty Panel, Glides",PMA1:PMP:4GB,0,1,1,0
"29Hx24Dx72W,Dubble Under-Surface Pattern Module,Polyester Modesty Panel,Glides",PAFCV2472,PAFCV2472-74P:PMB1:PMP:4GB,29,24,72,74P,PMB1,Dubble Under-Surface Pattern Module,Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Dubble Under-Surface Pattern Module, Polyester Modesty Panel, Glides",PMB1:PMP:4GB,0,1,1,1
"29Hx24Dx72W,Dean In-Surface Pattern Module,Polyester Modesty Panel,Glides",PAFCV2472,PAFCV2472-74P:PMD1:PMP:4GB,29,24,72,74P,PMD1,Dean In-Surface Pattern Module,Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Dean In-Surface Pattern Module, Polyester Modesty Panel, Glides",PMD1:PMP:4GB,0,1,1,2
"29Hx24Dx72W,Node In Surface Pattern Module,Polyester Modesty Panel,Glides",PAFCV2472,PAFCV2472-74P:PMO1:PMP:4GB,29,24,72,74P,PMO1,Node In Surface Pattern Module,Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Node In Surface Pattern Module, Polyester Modesty Panel, Glides",PMO1:PMP:4GB,0,1,1,3
"29Hx24Dx72W,Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1),Polyester Modesty Panel,Glides",PAFCV2472,PAFCV2472-74P:PS2GA1:PMP:4GB,29,24,72,74P,PS2GA1,"Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1)",Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1), Polyester Modesty Panel, Glides",PS2GA1:PMP:4GB,0,1,1,10
"29Hx24Dx72W,Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1),Polyester Modesty Panel,Glides",PAFCV2472,PAFCV2472-74P:PS2MB1GA1:PMP:4GB,29,24,72,74P,PS2MB1GA1,"Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1)",Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 24""D x 72""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1), Polyester Modesty Panel, Glides",PS2MB1GA1:PMP:4GB,0,1,1,11
"29Hx30Dx60W,Nacre In-Surface Pattern Module,No Modesty Panel,Casters",PAFCV3060,PAFCV3060-74P:PMA1:NMP:4EC,29,30,60,74P,PMA1,Nacre In-Surface Pattern Module,No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Nacre In-Surface Pattern Module, No Modesty Panel, Casters",PMA1:NMP:4EC,0,0,0,0
"29Hx30Dx60W,Dubble Under-Surface Pattern Module,No Modesty Panel,Casters",PAFCV3060,PAFCV3060-74P:PMB1:NMP:4EC,29,30,60,74P,PMB1,Dubble Under-Surface Pattern Module,No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Dubble Under-Surface Pattern Module, No Modesty Panel, Casters",PMB1:NMP:4EC,0,0,0,1
"29Hx30Dx60W,Dean In-Surface Pattern Module,No Modesty Panel,Casters",PAFCV3060,PAFCV3060-74P:PMD1:NMP:4EC,29,30,60,74P,PMD1,Dean In-Surface Pattern Module,No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Dean In-Surface Pattern Module, No Modesty Panel, Casters",PMD1:NMP:4EC,0,0,0,2
"29Hx30Dx60W,Node In Surface Pattern Module,No Modesty Panel,Casters",PAFCV3060,PAFCV3060-74P:PMO1:NMP:4EC,29,30,60,74P,PMO1,Node In Surface Pattern Module,No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Node In Surface Pattern Module, No Modesty Panel, Casters",PMO1:NMP:4EC,0,0,0,3
"29Hx30Dx60W,Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1),No Modesty Panel,Casters",PAFCV3060,PAFCV3060-74P:PS2GA1:NMP:4EC,29,30,60,74P,PS2GA1,"Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1)",No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1), No Modesty Panel, Casters",PS2GA1:NMP:4EC,0,0,0,10
"29Hx30Dx60W,Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1),No Modesty Panel,Casters",PAFCV3060,PAFCV3060-74P:PS2MB1GA1:NMP:4EC,29,30,60,74P,PS2MB1GA1,"Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1)",No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1), No Modesty Panel, Casters",PS2MB1GA1:NMP:4EC,0,0,0,11
"29Hx30Dx60W,Nacre In-Surface Pattern Module,No Modesty Panel,Glides",PAFCV3060,PAFCV3060-74P,29,30,60,74P,PMA1,Nacre In-Surface Pattern Module,No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Nacre In-Surface Pattern Module, No Modesty Panel, Glides",PMA1:NMP:4GB,0,0,1,0
"29Hx30Dx60W,Dubble Under-Surface Pattern Module,No Modesty Panel,Glides",PAFCV3060,PAFCV3060-74P:PMB1:NMP:4GB,29,30,60,74P,PMB1,Dubble Under-Surface Pattern Module,No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Dubble Under-Surface Pattern Module, No Modesty Panel, Glides",PMB1:NMP:4GB,0,0,1,1
"29Hx30Dx60W,Dean In-Surface Pattern Module,No Modesty Panel,Glides",PAFCV3060,PAFCV3060-74P:PMD1:NMP:4GB,29,30,60,74P,PMD1,Dean In-Surface Pattern Module,No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Dean In-Surface Pattern Module, No Modesty Panel, Glides",PMD1:NMP:4GB,0,0,1,2
"29Hx30Dx60W,Node In Surface Pattern Module,No Modesty Panel,Glides",PAFCV3060,PAFCV3060-74P:PMO1:NMP:4GB,29,30,60,74P,PMO1,Node In Surface Pattern Module,No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Node In Surface Pattern Module, No Modesty Panel, Glides",PMO1:NMP:4GB,0,0,1,3
"29Hx30Dx60W,Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1),No Modesty Panel,Glides",PAFCV3060,PAFCV3060-74P:PS2GA1:NMP:4GB,29,30,60,74P,PS2GA1,"Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1)",No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1), No Modesty Panel, Glides",PS2GA1:NMP:4GB,0,0,1,10
"29Hx30Dx60W,Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1),No Modesty Panel,Glides",PAFCV3060,PAFCV3060-74P:PS2MB1GA1:NMP:4GB,29,30,60,74P,PS2MB1GA1,"Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1)",No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1), No Modesty Panel, Glides",PS2MB1GA1:NMP:4GB,0,0,1,11
"29Hx30Dx60W,Nacre In-Surface Pattern Module,Polyester Modesty Panel,Casters",PAFCV3060,PAFCV3060-74P:PMA1:PMP:4EC,29,30,60,74P,PMA1,Nacre In-Surface Pattern Module,Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Nacre In-Surface Pattern Module, Polyester Modesty Panel, Casters",PMA1:PMP:4EC,0,1,0,0
"29Hx30Dx60W,Dubble Under-Surface Pattern Module,Polyester Modesty Panel,Casters",PAFCV3060,PAFCV3060-74P:PMB1:PMP:4EC,29,30,60,74P,PMB1,Dubble Under-Surface Pattern Module,Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Dubble Under-Surface Pattern Module, Polyester Modesty Panel, Casters",PMB1:PMP:4EC,0,1,0,1
"29Hx30Dx60W,Dean In-Surface Pattern Module,Polyester Modesty Panel,Casters",PAFCV3060,PAFCV3060-74P:PMD1:PMP:4EC,29,30,60,74P,PMD1,Dean In-Surface Pattern Module,Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Dean In-Surface Pattern Module, Polyester Modesty Panel, Casters",PMD1:PMP:4EC,0,1,0,2
"29Hx30Dx60W,Node In Surface Pattern Module,Polyester Modesty Panel,Casters",PAFCV3060,PAFCV3060-74P:PMO1:PMP:4EC,29,30,60,74P,PMO1,Node In Surface Pattern Module,Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Node In Surface Pattern Module, Polyester Modesty Panel, Casters",PMO1:PMP:4EC,0,1,0,3
"29Hx30Dx60W,Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1),Polyester Modesty Panel,Casters",PAFCV3060,PAFCV3060-74P:PS2GA1:PMP:4EC,29,30,60,74P,PS2GA1,"Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1)",Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1), Polyester Modesty Panel, Casters",PS2GA1:PMP:4EC,0,1,0,10
"29Hx30Dx60W,Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1),Polyester Modesty Panel,Casters",PAFCV3060,PAFCV3060-74P:PS2MB1GA1:PMP:4EC,29,30,60,74P,PS2MB1GA1,"Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1)",Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1), Polyester Modesty Panel, Casters",PS2MB1GA1:PMP:4EC,0,1,0,11
"29Hx30Dx60W,Nacre In-Surface Pattern Module,Polyester Modesty Panel,Glides",PAFCV3060,PAFCV3060-74P:PMA1:PMP:4GB,29,30,60,74P,PMA1,Nacre In-Surface Pattern Module,Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Nacre In-Surface Pattern Module, Polyester Modesty Panel, Glides",PMA1:PMP:4GB,0,1,1,0
"29Hx30Dx60W,Dubble Under-Surface Pattern Module,Polyester Modesty Panel,Glides",PAFCV3060,PAFCV3060-74P:PMB1:PMP:4GB,29,30,60,74P,PMB1,Dubble Under-Surface Pattern Module,Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Dubble Under-Surface Pattern Module, Polyester Modesty Panel, Glides",PMB1:PMP:4GB,0,1,1,1
"29Hx30Dx60W,Dean In-Surface Pattern Module,Polyester Modesty Panel,Glides",PAFCV3060,PAFCV3060-74P:PMD1:PMP:4GB,29,30,60,74P,PMD1,Dean In-Surface Pattern Module,Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Dean In-Surface Pattern Module, Polyester Modesty Panel, Glides",PMD1:PMP:4GB,0,1,1,2
"29Hx30Dx60W,Node In Surface Pattern Module,Polyester Modesty Panel,Glides",PAFCV3060,PAFCV3060-74P:PMO1:PMP:4GB,29,30,60,74P,PMO1,Node In Surface Pattern Module,Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Node In Surface Pattern Module, Polyester Modesty Panel, Glides",PMO1:PMP:4GB,0,1,1,3
"29Hx30Dx60W,Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1),Polyester Modesty Panel,Glides",PAFCV3060,PAFCV3060-74P:PS2GA1:PMP:4GB,29,30,60,74P,PS2GA1,"Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1)",Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1), Polyester Modesty Panel, Glides",PS2GA1:PMP:4GB,0,1,1,10
"29Hx30Dx60W,Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1),Polyester Modesty Panel,Glides",PAFCV3060,PAFCV3060-74P:PS2MB1GA1:PMP:4GB,29,30,60,74P,PS2MB1GA1,"Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1)",Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 60""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1), Polyester Modesty Panel, Glides",PS2MB1GA1:PMP:4GB,0,1,1,11
"29Hx30Dx72W,Nacre In-Surface Pattern Module,No Modesty Panel,Casters",PAFCV3072,PAFCV3072-74P:PMA1:NMP:4EC,29,30,72,74P,PMA1,Nacre In-Surface Pattern Module,No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Nacre In-Surface Pattern Module, No Modesty Panel, Casters",PMA1:NMP:4EC,0,0,0,0
"29Hx30Dx72W,Dubble Under-Surface Pattern Module,No Modesty Panel,Casters",PAFCV3072,PAFCV3072-74P:PMB1:NMP:4EC,29,30,72,74P,PMB1,Dubble Under-Surface Pattern Module,No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Dubble Under-Surface Pattern Module, No Modesty Panel, Casters",PMB1:NMP:4EC,0,0,0,1
"29Hx30Dx72W,Dean In-Surface Pattern Module,No Modesty Panel,Casters",PAFCV3072,PAFCV3072-74P:PMD1:NMP:4EC,29,30,72,74P,PMD1,Dean In-Surface Pattern Module,No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Dean In-Surface Pattern Module, No Modesty Panel, Casters",PMD1:NMP:4EC,0,0,0,2
"29Hx30Dx72W,Node In Surface Pattern Module,No Modesty Panel,Casters",PAFCV3072,PAFCV3072-74P:PMO1:NMP:4EC,29,30,72,74P,PMO1,Node In Surface Pattern Module,No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Node In Surface Pattern Module, No Modesty Panel, Casters",PMO1:NMP:4EC,0,0,0,3
"29Hx30Dx72W,Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1),No Modesty Panel,Casters",PAFCV3072,PAFCV3072-74P:PS2GA1:NMP:4EC,29,30,72,74P,PS2GA1,"Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1)",No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1), No Modesty Panel, Casters",PS2GA1:NMP:4EC,0,0,0,10
"29Hx30Dx72W,Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1),No Modesty Panel,Casters",PAFCV3072,PAFCV3072-74P:PS2MB1GA1:NMP:4EC,29,30,72,74P,PS2MB1GA1,"Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1)",No Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1), No Modesty Panel, Casters",PS2MB1GA1:NMP:4EC,0,0,0,11
"29Hx30Dx72W,Nacre In-Surface Pattern Module,No Modesty Panel,Glides",PAFCV3072,PAFCV3072-74P,29,30,72,74P,PMA1,Nacre In-Surface Pattern Module,No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Nacre In-Surface Pattern Module, No Modesty Panel, Glides",PMA1:NMP:4GB,0,0,1,0
"29Hx30Dx72W,Dubble Under-Surface Pattern Module,No Modesty Panel,Glides",PAFCV3072,PAFCV3072-74P:PMB1:NMP:4GB,29,30,72,74P,PMB1,Dubble Under-Surface Pattern Module,No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Dubble Under-Surface Pattern Module, No Modesty Panel, Glides",PMB1:NMP:4GB,0,0,1,1
"29Hx30Dx72W,Dean In-Surface Pattern Module,No Modesty Panel,Glides",PAFCV3072,PAFCV3072-74P:PMD1:NMP:4GB,29,30,72,74P,PMD1,Dean In-Surface Pattern Module,No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Dean In-Surface Pattern Module, No Modesty Panel, Glides",PMD1:NMP:4GB,0,0,1,2
"29Hx30Dx72W,Node In Surface Pattern Module,No Modesty Panel,Glides",PAFCV3072,PAFCV3072-74P:PMO1:NMP:4GB,29,30,72,74P,PMO1,Node In Surface Pattern Module,No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Node In Surface Pattern Module, No Modesty Panel, Glides",PMO1:NMP:4GB,0,0,1,3
"29Hx30Dx72W,Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1),No Modesty Panel,Glides",PAFCV3072,PAFCV3072-74P:PS2GA1:NMP:4GB,29,30,72,74P,PS2GA1,"Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1)",No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1), No Modesty Panel, Glides",PS2GA1:NMP:4GB,0,0,1,10
"29Hx30Dx72W,Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1),No Modesty Panel,Glides",PAFCV3072,PAFCV3072-74P:PS2MB1GA1:NMP:4GB,29,30,72,74P,PS2MB1GA1,"Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1)",No Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1), No Modesty Panel, Glides",PS2MB1GA1:NMP:4GB,0,0,1,11
"29Hx30Dx72W,Nacre In-Surface Pattern Module,Polyester Modesty Panel,Casters",PAFCV3072,PAFCV3072-74P:PMA1:PMP:4EC,29,30,72,74P,PMA1,Nacre In-Surface Pattern Module,Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Nacre In-Surface Pattern Module, Polyester Modesty Panel, Casters",PMA1:PMP:4EC,0,1,0,0
"29Hx30Dx72W,Dubble Under-Surface Pattern Module,Polyester Modesty Panel,Casters",PAFCV3072,PAFCV3072-74P:PMB1:PMP:4EC,29,30,72,74P,PMB1,Dubble Under-Surface Pattern Module,Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Dubble Under-Surface Pattern Module, Polyester Modesty Panel, Casters",PMB1:PMP:4EC,0,1,0,1
"29Hx30Dx72W,Dean In-Surface Pattern Module,Polyester Modesty Panel,Casters",PAFCV3072,PAFCV3072-74P:PMD1:PMP:4EC,29,30,72,74P,PMD1,Dean In-Surface Pattern Module,Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Dean In-Surface Pattern Module, Polyester Modesty Panel, Casters",PMD1:PMP:4EC,0,1,0,2
"29Hx30Dx72W,Node In Surface Pattern Module,Polyester Modesty Panel,Casters",PAFCV3072,PAFCV3072-74P:PMO1:PMP:4EC,29,30,72,74P,PMO1,Node In Surface Pattern Module,Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Node In Surface Pattern Module, Polyester Modesty Panel, Casters",PMO1:PMP:4EC,0,1,0,3
"29Hx30Dx72W,Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1),Polyester Modesty Panel,Casters",PAFCV3072,PAFCV3072-74P:PS2GA1:PMP:4EC,29,30,72,74P,PS2GA1,"Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1)",Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1), Polyester Modesty Panel, Casters",PS2GA1:PMP:4EC,0,1,0,10
"29Hx30Dx72W,Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1),Polyester Modesty Panel,Casters",PAFCV3072,PAFCV3072-74P:PS2MB1GA1:PMP:4EC,29,30,72,74P,PS2MB1GA1,"Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1)",Polyester Modesty Panel,Casters,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1), Polyester Modesty Panel, Casters",PS2MB1GA1:PMP:4EC,0,1,0,11
"29Hx30Dx72W,Nacre In-Surface Pattern Module,Polyester Modesty Panel,Glides",PAFCV3072,PAFCV3072-74P:PMA1:PMP:4GB,29,30,72,74P,PMA1,Nacre In-Surface Pattern Module,Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Nacre In-Surface Pattern Module, Polyester Modesty Panel, Glides",PMA1:PMP:4GB,0,1,1,0
"29Hx30Dx72W,Dubble Under-Surface Pattern Module,Polyester Modesty Panel,Glides",PAFCV3072,PAFCV3072-74P:PMB1:PMP:4GB,29,30,72,74P,PMB1,Dubble Under-Surface Pattern Module,Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Dubble Under-Surface Pattern Module, Polyester Modesty Panel, Glides",PMB1:PMP:4GB,0,1,1,1
"29Hx30Dx72W,Dean In-Surface Pattern Module,Polyester Modesty Panel,Glides",PAFCV3072,PAFCV3072-74P:PMD1:PMP:4GB,29,30,72,74P,PMD1,Dean In-Surface Pattern Module,Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Dean In-Surface Pattern Module, Polyester Modesty Panel, Glides",PMD1:PMP:4GB,0,1,1,2
"29Hx30Dx72W,Node In Surface Pattern Module,Polyester Modesty Panel,Glides",PAFCV3072,PAFCV3072-74P:PMO1:PMP:4GB,29,30,72,74P,PMO1,Node In Surface Pattern Module,Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Node In Surface Pattern Module, Polyester Modesty Panel, Glides",PMO1:PMP:4GB,0,1,1,3
"29Hx30Dx72W,Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1),Polyester Modesty Panel,Glides",PAFCV3072,PAFCV3072-74P:PS2GA1:PMP:4GB,29,30,72,74P,PS2GA1,"Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1)",Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Grommet, Nacre, Qty (1), Polyester Modesty Panel, Glides",PS2GA1:PMP:4GB,0,1,1,10
"29Hx30Dx72W,Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1),Polyester Modesty Panel,Glides",PAFCV3072,PAFCV3072-74P:PS2MB1GA1:PMP:4GB,29,30,72,74P,PS2MB1GA1,"Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1)",Polyester Modesty Panel,Glides,"Pirouette Fixed Chevron Standard Height Table - 30""D x 72""W x 29""H, 74P Edge, Pattern Snap RPT's (2) & Pattern Module, Dubbel Under-Surface (1), & Grommet, Nacre (1), Polyester Modesty Panel, Glides",PS2MB1GA1:PMP:4GB,0,1,1,11
