{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[[24,0,24,1]],"flags":["formulas_cached_only"]}
["LEED- CI - Potential Credits Analysis: Vecta Au Lait Table"]
[]
["Credit","Desctiption","Potential Points",null,"Contribution",null,"Notes"]
[]
["MR4.1","Recylcled Content 10%",1,null,"Yes",null," "]
["MR4.2","Recylcled Content 20%",1,null,"Yes",null," "]
["MR5.1","Local Manufacturing",1,null,"No",null,"Vecta manufactures in Grand Prairie, TX"]
["MR6","Rapid Renewable Materials",1,null,"Yes, see note",null,"If wheatboard top special is selected"]
["MR7","FSC Certified Wood - Particle/MDF",1,null,"No, see note",null,"Our particle board meets Composite Panel Associations EPP Grademark and Sustainable Foriest Initiative SFI program"]
["MR7","FSC Certified Wood - Veneer",1,null,"Yes, see note",null,"FSC veneer can be provided on request"]
["EQ4.4","Low Emitting Materials - urea-formaldehyde",1,null,"Yes, see note",null,"On tables ordered with special laminate and wheatboard topspecial"]
["EQ4.5","Low Emitting Materials - systems/seating",1,null,"No",null,"Vecta is beginning the certification process"]
[]
["Recycled Content Summary -"]
["Steelcase Inc."]
[]
[null,"Product Line:","Vecta - Au Lait Table",null,null,null,"Date Compiled:","2005-06-05"]
[]
[null,"Description:","30 x 30 table with flip top",null,null,null,"Contact:","Tom Di Lillo"]
[]
[null,"Style Number:","AL3030FSC",null,null,null,"Plant of Record:"]
[]
[null,"Surface Materials:","laminate top"]
[null,"(in example)"]
["Materials",null,"Total Weight (lbs)","% Recycled Content*","Recycled Content  (lbs)","% Post Consumer Recycled Content*","Post Consumer Content (lbs)","% Recyclable*","Recyclable (lbs)"]
["Metal"]
[null,"Steel",13,0.3,3.9,0," ",1,13]
[null,"Aluminum"," "," "," ",null," "]
[null,"Other"]
["Plastic"]
[null,"Polypropylene"]
[null,"Polyurethane foam"]
[null,"Nylon",7.2,0,0,0,null,0,0]
[null,"Acetal (delrin)"]
[null,"PVC",3,0,0,0,null,0,0]
[null,"ABS"]
[null,"HDPE"]
[null,"Other"]
["Laminate",null,1.8,0,0,0,null,0,0]
["Wood"]
[null,"Particle Board/MDF",27,1,27,0,0,1,27]
[null,"Plywood"]
[null,"Veneer"]
[null,"OSB"]
[null,"Solid"]
[null,"Other"]
["Glass"]
[null,"Tempered glass"]
[null,"Fiberglass"]
["Fabric"]
["Miscellaneous"]
["TOTAL",null,52,0.5942307692307692,30.9,0,0,0.7692307692307693,40]
[" "]
[]
["Comments: "]
[" "]
[" "]
[]
["Disclaimer:"]
["Calculations of recycled content are based on data provided by suppliers and other available information.  This data may include"]
["industry averages, ranges or other broadly based information.  Steelcase makes conservative assumptions when compiling this "]
["information to provide the most accurate recycled content calculations possible but variability in market conditions or manufacturing"]
["processes may result in higher or lower content.  This document will be reviewed and updated periodically and is subject to change"]
["without notice."]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}