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TRITON BATH ACCESSORIES

Part 1 GENERAL
1.01 SUMMARY

A. Bathroom accessories for safety and decoration.

1.02 SECTION INCLUDES

A. Section 10800 – Color towel bars and holders

B. Section 10800 – Color toilet paper holders

C. Section 10800 – Color toilet brush units

D. Section 10800 – Miscellaneous accessories (soap holder, sponge holder, robe hooks, shower curtain rail and hooks)

E. Section 08830 – Adjustable mirror with color profiles

1.03 REFERENCES

A. American with Disabilities Act Accessibility Guidelines (ADAAG)

B. American National Standards Institute (ANSI)

C. American Society for Testing and Materials (ASTM)

1.04 SUBMITTALS

A. Product Data: Manufacturer’s standard product data for each product specified, including detail dimen​sions, function, and finish.

B. Samples: Manufacturer’s color selection and verifica​tion samples – full size or 12" in length.

C. Manufacturer’s printed installation instruction: Include anchoring and fastening details.

1.05 DELIVERY, STORAGE AND HANDLING

A. Deliver materials in unopened factory packaging to the jobsite

B. Inspect materials at delivery to assure that specified products have been received.

C. Store in original packaging in a climate controlled location away from direct sunlight.

1.06 PROJECT CONDITIONS

A. Environmental Requirements: Products must be in​stalled in an interior climate controlled environment.

1.07 WARRANTY

A. Standard IPC Limited Lifetime Warranty against material and manufacturing defects.

Part 2 - PRODUCTS
2.01 MANUFACTURER

A. Acceptable Distributor/Manufacturer: IPC Door and Wall Protection Systems, InPro Corporation, PO Box 406, Muskego, WI 53150, USA; Telephone: 800-222-5556, Fax: 888-715-8407, Internet address: http://www.inprocorp.com

B. Substitutions: Not permitted.

C. Provide all grab bars and bathroom accessories from a single manufacturer.

2.02 MANUFACTURED UNITS

A. Towel bars, holders and shelf.

1. Corrosion resistant steel core with PVC finish coating, round 7/8"(22mm) diameter.

2. Colors as selected from manufacturers standard range.

a. Size 11" long

b. Size 17" long

c. Size 23" long

d. Shelf 7" deep by 17" wide.

B. Miscellaneous toilet and bath accessories.

1. Toilet tissue holder. Nylon, 53/4" wide by 141/2"deep, with concealed fasteners. Colors as selected from manufacturers standard range.

2. Reserve roll holder. Nylon, 5" deep with concealed fastener. Colors as selected from manufacturers standard range.

3. Toilet brush unit. Nylon, concealed fasteners for holder with container and brush. Colors as selected from manufacturers standard range.

4. Soap holder. Nylon, 4" wide by 41/2" deep, with concealed fasteners. Colors as selected from manufacturers standard range.

5. Sponge holder. Nylon, 6" by 6", with concealed fasteners. Colors as selected from manufacturers standard range.

6. Robe hook. Nylon, 11/4" deep, with concealed fasteners. Colors as selected from manufacturers standard range.

7. Double robe hook. Nylon, 11/4" deep by 11/2" wide. With concealed fasteners. Colors as selected from manufacturers standard range.

8. Shower curtain rail. Corrosion resistant steel core with PVC finish coating, round 11/4" (32mm) diameter. Colors as selected from manufacturers standard range.

9. Shower curtain hook. Nylon, Colors as selected from manufacturers standard range.

C. Adjustable mirror with colored profiles.

1. Safety glass-2B with tilt feature, framed top and bottom with color accent as selected from manufacturers standard range.

Part 3 EXECUTION
3.01 EXAMINATION

A. Do not begin installation until substrates finishing operations are completed, including painting.

B. Verify that prepared openings are sized and located in accordance with architects recommendations. Verify that blocking, reinforcement and anchoring devices are the correct type.
END OF SECTION
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