,Watts##ELECTRICAL_WATTAGE##WATTS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Luminous Flux##Electrical_Luminous_Flux##Lumens,Photometric File Name##OTHER##,Model##OTHER##,Direct Mount##OTHER##,Pendant Mount##OTHER##,Air Craft Cable Mount##OTHER##
DW-LED-SS-WW,44,3500,5295,DW-LED-SS-WW.ies,DW-LED-SS-WW,1,0,0
DW-LED-SS-NW,44,4000,5218,DW-LED-SS-NW.ies,DW-LED-SS-NW,1,0,0
DW-LED-SS-CW,44,5000,5866,DW-LED-SS-CW.ies,DW-LED-SS-CW,1,0,0
DW-LED-HO-WW,57,3500,6363,DW-LED-HO-WW.ies,DW-LED-HO-WW,1,0,0
DW-LED-HO-NW,59,4000,6262,DW-LED-HO-NW.ies,DW-LED-HO-NW,1,0,0
DW-LED-HO-CW,57,5000,7105,DW-LED-HO-CW.ies,DW-LED-HO-CW,1,0,0
DW-LED-SS-WW-PMK,44,3500,5295,DW-LED-SS-WW.ies,DW-LED-SS-WW-PMK,0,1,0
DW-LED-SS-NW-PMK,44,4000,5218,DW-LED-SS-NW.ies,DW-LED-SS-NW-PMK,0,1,0
DW-LED-SS-CW-PMK,44,5000,5866,DW-LED-SS-CW.ies,DW-LED-SS-CW-PMK,0,1,0
DW-LED-HO-WW-PMK,57,3500,6363,DW-LED-HO-WW.ies,DW-LED-HO-WW-PMK,0,1,0
DW-LED-HO-NW-PMK,59,4000,6262,DW-LED-HO-NW.ies,DW-LED-HO-NW-PMK,0,1,0
DW-LED-HO-CW-PMK,57,5000,7105,DW-LED-HO-CW.ies,DW-LED-HO-CW-PMK,0,1,0
DW-LED-SS-WW-CHSIMX,44,3500,5295,DW-LED-SS-WW.ies,DW-LED-SS-WW-CHSIMX,0,0,1
DW-LED-SS-NW-CHSIMX,44,4000,5218,DW-LED-SS-NW.ies,DW-LED-SS-NW-CHSIMX,0,0,1
DW-LED-SS-CW-CHSIMX,44,5000,5866,DW-LED-SS-CW.ies,DW-LED-SS-CW-CHSIMX,0,0,1
DW-LED-HO-WW-CHSIMX,57,3500,6363,DW-LED-HO-WW.ies,DW-LED-HO-WW-CHSIMX,0,0,1
DW-LED-HO-NW-CHSIMX,59,4000,6262,DW-LED-HO-NW.ies,DW-LED-HO-NW-CHSIMX,0,0,1
DW-LED-HO-CW-CHSIMX,57,5000,7105,DW-LED-HO-CW.ies,DW-LED-HO-CW-CHSIMX,0,0,1
