,Watts##ELECTRICAL_WATTAGE##WATTS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Luminous Flux##Electrical_Luminous_Flux##Lumens,Width##LENGTH##INCHES,Photometric File Name##OTHER##,Model##OTHER##
WNA10-LED-HO-CW,57.2,5000,6910.6,9.875,WNA10-LED-HO-CW.ies,WNA10-LED-HO-CW
WNA10-LED-HO-NW,57.2,4000,6340.6,9.875,WNA10-LED-HO-NW.ies,WNA10-LED-HO-NW
WNA10-LED-HO-WW,58,3500,6742.9,9.875,WNA10-LED-HO-WW.ies,WNA10-LED-HO-WW
WNA10-LED-SS-CW,33,5000,4445.9,9.875,WNA10-LED-SS-CW.ies,WNA10-LED-SS-CW
WNA10-LED-SS-NW,33,4000,4078.8,9.875,WNA10-LED-SS-NW.ies,WNA10-LED-SS-NW
WNA10-LED-SS-WW,33,3500,4476.4,9.875,WNA10-LED-SS-WW.ies,WNA10-LED-SS-WW
WNA14-LED-HO-CW,55,5000,7559.2,14.375,WNA14-LED-HO-CW.ies,WNA14-LED-HO-CW
WNA14-LED-HO-NW,56,4000,6679.8,14.375,WNA14-LED-HO-NW.ies,WNA14-LED-HO-NW
WNA14-LED-HO-WW,56,3500,6783.9,14.375,WNA14-LED-HO-WW.ies,WNA14-LED-HO-WW
WNA14-LED-VHO-CW,89,5000,12592.6,14.375,WNA14-LED-VHO-CW.ies,WNA14-LED-VHO-CW
WNA14-LED-VHO-NW,89,4000,10020,14.375,WNA14-LED-VHO-NW.ies,WNA14-LED-VHO-NW
WNA14-LED-VHO-WW,89,3500,10577.4,14.375,WNA14-LED-VHO-WW.ies,WNA14-LED-VHO-WW
