,Watts##ELECTRICAL_WATTAGE##WATTS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Luminous Flux##Electrical_Luminous_Flux##Lumens,Housing Type##OTHER##,Width##LENGTH##INCHES,Length##LENGTH##INCHES,Height##LENGTH##INCHES,Photometric File Name##OTHER##,Model##OTHER##
LPASC22-LED-HO-CW,36,5000,4052,Housing : LPASC22,23.75,24,3,LPASC22-LED-HO-CW.ies,LPASC22-LED-HO-CW
LPASC22-LED-HO-NW,35,4000,3620,Housing : LPASC22,23.75,24,3,LPASC22-LED-HO-NW.ies,LPASC22-LED-HO-NW
LPASC22-LED-HO-WW,35,3500,3323,Housing : LPASC22,23.75,24,3,LPASC22-LED-HO-WW.ies,LPASC22-LED-HO-WW
LPASC22-LED-SS-CW,29,5000,3430,Housing : LPASC22,23.75,24,3,LPASC22-LED-SS-CW.ies,LPASC22-LED-SS-CW
LPASC22-LED-SS-NW,29,4000,3061,Housing : LPASC22,23.75,24,3,LPASC22-LED-SS-NW.ies,LPASC22-LED-SS-NW
LPASC22-LED-SS-WW,29,3500,2809,Housing : LPASC22,23.75,24,3,LPASC22-LED-SS-WW.ies,LPASC22-LED-SS-WW
LPASC24-LED-HO-CW,46,5000,5185,Housing : LPASC24,23.75,48,3,LPASC24-LED-HO-CW.ies,LPASC24-LED-HO-CW
LPASC24-LED-HO-NW,46,4000,4657,Housing : LPASC24,23.75,48,3,LPASC24-LED-HO-NW.ies,LPASC24-LED-HO-NW
LPASC24-LED-HO-WW,46,3500,4319,Housing : LPASC24,23.75,48,3,LPASC24-LED-HO-WW.ies,LPASC24-LED-HO-WW
LPASC24-LED-SS-CW,36,5000,4273,Housing : LPASC24,23.75,48,3,LPASC24-LED-SS-CW.ies,LPASC24-LED-SS-CW
LPASC24-LED-SS-NW,36,4000,3787,Housing : LPASC24,23.75,48,3,LPASC24-LED-SS-NW.ies,LPASC24-LED-SS-NW
LPASC24-LED-SS-WW,35,3500,3528,Housing : LPASC24,23.75,48,3,LPASC24-LED-SS-WW.ies,LPASC24-LED-SS-WW
LPASC14-LED-HO-CW,35,5000,4332,Housing : LPASC14,11.75,48,3.25,LPASC14-LED-HO-CW.ies,LPASC14-LED-HO-CW
LPASC14-LED-HO-NW,35,4000,3857,Housing : LPASC14,11.75,48,3.25,LPASC14-LED-HO-NW.ies,LPASC14-LED-HO-NW
LPASC14-LED-HO-WW,35,3500,3580,Housing : LPASC14,11.75,48,3.25,LPASC14-LED-HO-WW.ies,LPASC14-LED-HO-WW
LPASC14-LED-SS-CW,29,5000,3694,Housing : LPASC14,11.75,48,3.25,LPASC14-LED-SS-CW.ies,LPASC14-LED-SS-CW
LPASC14-LED-SS-NW,29,4000,3295,Housing : LPASC14,11.75,48,3.25,LPASC14-LED-SS-NW.ies,LPASC14-LED-SS-NW
LPASC14-LED-SS-WW,29,3500,3074,Housing : LPASC14,11.75,48,3.25,LPASC14-LED-SS-WW.ies,LPASC14-LED-SS-WW
