900.51.10460
Hook-on seat, System 900
- construction consisting of seat, backrest and hook-on device
- reinforcement of the seat and hook-on device made of aluminium, powder coated in HEWI colours AS (matt white), CV (matt black) and AF (anthracite grey matt)
- slip-resistant, textured seat and backrest made of matt synthetic material in colour of the hook-on device
- seat with hygiene cutout can be folded up to save space
- for hooking onto HEWI shower grab rails and support rails with diameter 30, 32 and 33 mm
- weight capacity up to 150 kg
- 450 mm wide, 637 mm deep and 533 mm high
- seat 450 mm wide and 450 mm deep
- product weight: 8.8 kg
- fulfils the DIN 18040 and ÖNORM B1600/1601 requirements

Article no.: HEWI 900.51.10460

