V 230720HEWI Produktkatalog                                                                                                04EUR
A;N;900.51.10060;10;HEWI Removable hanging seat;;1;0;PCE;0; ; ;2;
T;N;2;;1;;Hook-on seat, System 900;2;;- construction consisting of seat,;;
T;N;2;;3;;backrest and hook-on device;4;;- reinforcement of the seat and hook-on;;
T;N;2;;5;;device made of aluminium, powder coated;6;;in HEWI colours AS (matt white), CV;;
T;N;2;;7;;(matt black) and AF (anthracite grey;8;;matt);;
T;N;2;;9;;- slip-resistant, textured seat and;10;;backrest made of matt synthetic;;
T;N;2;;11;;material in colour of the hook-on device;12;;- seat can be folded up to save space;;
T;N;2;;13;;- for hooking onto HEWI shower grab;14;;rails and support rails with diameter;;
T;N;2;;15;;30, 32 and 33 mm;16;;- weight capacity up to 150 kg;;
T;N;2;;17;;- 350 mm wide, 526 mm deep and 533 mm;18;;high;;
T;N;2;;19;;- seat 350 mm wide and 340 mm deep;20;;- product weight: 8.0 kg;;
T;N;2;;21;;Article no.: HEWI 900.51.10060;;;;;
