900.50.10060
Mono hinged support rail, design (A), System 900
- with one horizontal, round gripping level
- can be folded upwards and folded downwards with braked movement
- projection 23 5/8 inch (600 mm), 8 1/4 inch (210 mm) high and 4 inch (101 mm) wide, bar diameter 1 5/16 inch (33.7 mm)
- load capacity up to 220 lbs (100 kg)
- made of stainless steel, powder-coated in the HEWI colours DX (matt white), DC (matt black), AY (matt light gray pearl mica) and SC (matt dark gray pearl mica)
- for mounting with non-corrosive and tested HEWI fixing materials for different wall systems (to be ordered separately)
- sealing tape for sealing the fixing points is included in the scope of supply
- CE marking according to Directive 93/42/EEC
- fulfils the DIN 18040 requirements

Article no.: HEWI 900.50.10060

