950.50.06690
Toilet roll holder with WC flushing mechanism and function button upgrade kit (radio controlled)
- right angle-shaped toilet roll holder with WC flushing mechanism and function button (radio controlled)
- blue button for releasing the flushing mechanism, red button for triggering a freely definable function (The function button does not meet the requirements for an emergency call according to DIN VDE 0834-1)
- right-hand version
- for retrofitting on hinged support rails 950.50.1... and stationary support rails 950.50.3...
- easy installation
- integrated toilet roll brake
- 35 mm wide, 122.5 mm high, 149 mm deep
- made of high-quality polyamide according to HEWI colour chart
- transmission frequency 868.4 MHz
- suitable for radio-controlled WC flushing systems made by Geberit, Friatec, Mepa, Sanit, Viega, TECE and Grohe

Article no.: HEWI 950.50.06690

