,Worksurface Material##OTHER##,Width##LENGTH##INCHES,URL##OTHER##,Model##OTHER##,Manufacturer##OTHER##,Height from Floor##LENGTH##INCHES,Height##LENGTH##INCHES,Support Material##OTHER##,Description##OTHER##,Depth##LENGTH##INCHES,Copyright ©##OTHER##,Catalog##OTHER##,Authoring Version##OTHER##,Assembly Code##OTHER##
WORKSURFACE SIDE MODESTY SOFT 23W FROSTED ACRYLIC,OFS RANGE Frosted Acrylic,23.000000000000,http://www.ofs.com/,HB-WEMAR-23/22.5,CAROLINA,24.500000000000,22.500000000000,OFS RANGE Metal Support,"OFS RANGE WORKSURFACE SIDE MODESTY SOFT FROSTED ACRYLIC, 23"" Width, Use with 24""W Worksurface",0.250000000000,©OFS 2019,https://ofs.com/products/open-plan/benching/range,Autodesk Revit Architecture 2015,E2020200
WORKSURFACE SIDE MODESTY SOFT 29W FROSTED ACRYLIC,OFS RANGE Frosted Acrylic,29.000000000000,http://www.ofs.com/,HB-WEMAR-29/22.5,CAROLINA,24.500000000000,22.500000000000,OFS RANGE Metal Support,"OFS RANGE WORKSURFACE SIDE MODESTY SOFT FROSTED ACRYLIC, 29"" Width, Use with 30""W Worksurface",0.250000000000,©OFS 2019,https://ofs.com/products/open-plan/benching/range,Autodesk Revit Architecture 2015,E2020200
